                                                      劇劅劅劅劅劅劅劅劅劅劅劉
                                                      劆俬俷俋侾俁侾侽亅侽侾劆
                                                      劋劅劅劅劅劅劅劅劅劅劅劊
























                       FR/FRex僼傽儈儕 MB91310僔儕乕僘梡
                          僒儞僾儖I/O儗僕僗僞僼傽僀儖
                               巊  梡  庤  堷  彂

                                 晉巑捠姅幃夛幮

                                   戞侾丏侽斉

偼偠傔偵

  MB91310僔儕乕僘梡僒儞僾儖I/O儗僕僗僞僼傽僀儖偼丄MB91310僔儕乕僘偺
I/O儗僕僗僞傪傾僙儞僽儔尵岅偺僔儞儃儖偲偟偰愰尵丄偍傛傃掕媊偟偰偄傞僒儞僾儖
僾儘僌儔儉偱偡丅
  杮彂偼丄MB91310僔儕乕僘梡I/O儗僕僗僞僼傽僀儖偺僼傽僀儖峔惉丄曄悢偺愰尵丄
偍傛傃掕媊撪梕傪愢柧偟偰偄傑偡丅




I/O儗僕僗僞僼傽僀儖傪偛棙梡偄偨偩偔応崌偺拲堄

  丒  I/O儗僕僗僞僼傽僀儖偼丄懳徾昳庬傪尷掕偟偰採嫙偟偰偄傑偡丅偟偨偑偭偰丄懠偺
    昳庬偵墳梡偝傟傞応崌偵偼丄採嫙偟偰偄傞昳庬偺僾儘僌儔儉傪嶲峫偵偟偰丄奩摉偡
    傞昳庬偺I/O儗僕僗僞僼傽僀儖傪嶌惉偟偰壓偝偄丅

  丒  I/O儗僕僗僞僼傽僀儖傪巊梡偟偰丄I/O儗僕僗僞偺憖嶌傪峴偆僾儘僌儔儉傪婰弎偡
    傞応崌丄I/O儗僕僗僞偺傾僋僙僗弴彉丄僞僀儈儞僌摍傪僔僗僥儉揑偵峫椂偡傞昁梫偑
    偁傝傑偡偺偱丄僴乕僪僂僃傾儅僯儏傾儖傪嶲徠偟偰壓偝偄丅

  丒  I/O儗僕僗僞僼傽僀儖偼丄MB91310僔儕乕僘偺墳梡僾儘僌儔儉傪奐敪偡傞帪偵丄
    栶棫偰偰偄偨偩偔偨傔偵嶌惉偟偨嶲峫僾儘僌儔儉偱偡丅尩枾偵偼丄屄乆偺僔僗僥儉
    偵墳偠偰僾儘僌儔儉偵庤傪壛偊傞昁梫偑弌偰偔傞応崌傕偁傝傑偡偺偱丄偛巊梡偺嵺
    偵偼廫暘昡壙偺忋偛巊梡壓偝偄丅

  丒  I/O儗僕僗僞僼傽僀儖偺岆傝偵偮偄偰偼丄愑擟傪晧偄偐偹傞応崌偑偁傝丄傑偨岆傝
    偑敪尒偝傟偰傕捈偪偵廋惓偱偒側偄応崌偑偁傝傑偡偺偱偛椆彸壓偝偄丅




仭嶲徠儅僯儏傾儖堦棗

  MB91310僔儕乕僘梡僒儞僾儖I/O儗僕僗僞僼傽僀儖偼丄
  埲壓偺僴乕僪僂僃傾儅僯儏傾儖傪婎偵嶌惉偝傟偰偄傑偡丅

    丒乽MB91310 俴俽俬巇條彂 巄掕戞1.2斉 2002擭10寧07擔
        (mb91310lsi巇條彂1.2斉.pdf)乿

栚師

戞侾復  MB91310僔儕乕僘梡I/O儗僕僗僞僼傽僀儖峔惉

戞俀復  MB91310僔儕乕僘梡I/O儗僕僗僞僼傽僀儖巊梡曽朄

戞俁復  MB91310僔儕乕僘梡I/O儗僕僗僞愰尵僼傽僀儖偺愰尵撪梕

戞係復  MB91310僔儕乕僘梡I/O儗僕僗僞愰尵僼傽僀儖偱巊梡壜擻側曄悢柤媦傃儊儞僶柤

戞侾復  MB91310僔儕乕僘梡I/O儗僕僗僞僼傽僀儖峔惉

 ${FETOOL}        仼娐嫬曄悢FETOOL偵愝掕偝傟偰偄傞僨傿儗僋僩儕
  劘lib
    劘911
      劘include
        劘sample
          劘mb91310
            劙_fr.h乮I/O儗僕僗僞愰尵僼傽僀儖乯
            劔
            劙_mb91310.h乮MB91310僔儕乕僘梡I/O儗僕僗僞愰尵僼傽僀儖乯
            劙_ra91310.h乮MB91310僔儕乕僘梡I/O儗僕僗僞峔憿懱愰尵僼傽僀儖乯
            劔
            劘_fr_a.asm 乮奺I/O儗僕僗僞掕媊僼傽僀儖乯

  仭I/O儗僕僗僞愰尵僼傽僀儖

      I/O儗僕僗僞曄悢乮I/O儗僕僗僞偵懳墳偡傞曄悢乯愰尵僼傽僀儖偱偡丅
    I/O儗僕僗僞曄悢傪憖嶌偡傞墳梡僾儘僌儔儉傪婰弎偡傞帪偵丄偙偺僼傽僀儖傪
    僀儞僋儖乕僪偟偰壓偝偄丅

  仭MB91310僔儕乕僘梡I/O儗僕僗僞愰尵僼傽僀儖

      MB91310僔儕乕僘梡偺I/O儗僕僗僞僔儞儃儖愰尵僼傽僀儖偱偡丅

  仭MB91310僔儕乕僘梡I/O儗僕僗僞峔憿懱愰尵僼傽僀儖

      MB91310僔儕乕僘偺奺I/O儗僕僗僞偵懳墳偡傞峔憿傪愰尵偟偰偄傞僼傽僀儖偱偡丅

  仭奺I/O儗僕僗僞掕媊僼傽僀儖

      MB91310僔儕乕僘偺丄奺I/O儗僕僗僞僔儞儃儖傪掕媊偟偰偄傞僼傽僀儖偱偡丅

戞俀復  MB91310僔儕乕僘梡I/O儗僕僗僞僼傽僀儖巊梡曽朄

  (1) 巊梡偡傞昳庬傪-cpu僆僾僔儑儞偵巜掕偟偰丄I/O儗僕僗僞掕媊僼傽僀儖傪傾僙儞僽
      儖偟偰壓偝偄丅

        椺丗 > fasm911s -cpu mb91*** _fr_a.asm

  (2) I/O儗僕僗僞僔儞儃儖傪嶲徠偡傞墳梡僾儘僌儔儉傪婰弎偡傞応崌丄嫟捠I/O儗僕僗
      僞愰尵僼傽僀儖傪僀儞僋儖乕僪偟偰壓偝偄丅

        椺丗#include "_fr.h"
                    .....
               LDI:32  #_IO_PDR2,  R4
                    .....


  (3) 巊梡偡傞昳庬傪-cpu僆僾僔儑儞偵巜掕偟偰丄墳梡僾儘僌儔儉傪傾僙儞僽儖偟偰
      壓偝偄丅

        椺丗 > fasm911s  -cpu mb91*** sample.asm

        拲) CPU僆僾僔儑儞偱巜掕偟偨昳庬偑丄I/O儗僕僗僞僼傽僀儖偑巊梡壜擻側昳庬
            偱側偄応崌丄傾僙儞僽儖帪偵壓婰偺僄儔乕儊僢僙乕僕傪弌椡偟傑偡丅

              #error "The I/O register file of the specified CPU option
                      does not exist"

  (4) 巊梡偡傞昳庬傪-cpu僆僾僔儑儞偵巜掕偟偰丄(1)偱嶌惉偟偨僆僽僕僃僋僩僼傽
      僀儖偲丄(3)偱嶌惉偟偨墳梡僾儘僌儔儉偺僆僽僕僃僋僩僼傽僀儖傪儕儞僋偟偰
      壓偝偄丅

        椺丗 > flnk911s -cpu mb91*** -o sample.abs _fr_a.obj sample.obj

戞俁復  MB91310僔儕乕僘梡I/O儗僕僗僞愰尵僼傽僀儖偺愰尵撪梕

  僴乕僪僂僃傾儅僯儏傾儖偵婰嵹偝傟偰偄傞I/O儗僕僗僞柤偵懳墳偡傞丄
I/O儗僕僗僞僔儞儃儖傪丄埲壓偺傛偆偵愰尵偟偰偄傑偡丅

乵拲堄乶
  FR/FRex僼傽儈儕偺偺傾僙儞僾儔偱偼價僢僩扨埵偺傾僋僙僗偑偱偒傑偣傫偺偱丄
  慡偰僶僀僩扨埵偺傾僋僙僗偲側傝傑偡丅
  價僢僩柤偺傾僋僙僗偼俙俶俢丆俷俼摍偺婡夿岅柦椷傪梡偄偰壓偝偄丅

  仭I/O儗僕僗僞僔儞儃儖偼丄僶僀僩扨埵偱愰尵

  仭I/O儗僕僗僞僔儞儃儖柤偼丄婎杮揑偵懳墳偡傞I/O儗僕僗僞柤偺愭摢偵 '_IO_'傪晅
    壛偟偨宍偱愰尵乮堦晹丄傾僋僙僗偺搒崌忋丄暋悢偺I/O儗僕僗僞傪侾偮偺僔儞儃儖
    柤偱愰尵偟偨傝丄僔儞儃儖柤傪庒姳曄峏偟偰愰尵乯


  亂椺亃I/O儗僕僗僞PDR0偵懳偡傞愰尵撪梕

    丒I/O儗僕僗僞峔惉

          7       6       5       4       3       2       1       0    bit No.
      劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
      劔  P07 劆  P06 劆  P05 劆  P04 劆  P03 劆  P02 劆  P01 劆  P00 劔PDR0
      劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

    丒愰尵撪梕(儅僋儘傪巊梡)

        #macro io_pdr0 symbol
                BYTE_MEM
                STRUCT_TYPE_B
                        UCHARBIT(	P00, 1)
                        UCHARBIT(	P01, 1)
                        UCHARBIT(	P02, 1)
                        UCHARBIT(	P03, 1)
                        UCHARBIT(	P04, 1)
                        UCHARBIT(	P05, 1)
                        UCHARBIT(	P06, 1)
                        UCHARBIT(	P07, 1)
                STRUCT_TYPE_E(bit)
        #endm

        __IO_EXTERN  UNION_D(io_pdr0,   IO_PDR0)

    丒傾僙儞僽儖帪偵儅僋儘揥奐偝傟傞撪梕

        [奜晹掕媊帪]                              [奜晹嶲徠帪]
                      .GLOBAL _IO_PDR0             .GLOBAL _IO_PDR0
        _IO_PDR0      .res.b  1

戞係復  MB91310僔儕乕僘梡I/O儗僕僗僞愰尵僼傽僀儖偱巊梡壜擻側僔儞儃儖柤

仭柦椷僉儍僢僔儏惂屼儗僕僗僞

仭俬乛俷億乕僩

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 Pn7  劆 Pn6  劆 Pn5  劆 Pn4  劆 Pn3  劆 Pn2  劆 Pn1  劆 Pn0  劔PDRn,
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗DDRn
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔I2CTST劆  劒  劆  劒  劆I2CE4 劆I2CE3 劆I2CE2 劆I2CE1 劆I2CE0 劔PFR0
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔UART3 劆SCKE3 劆UART2 劆SCKE2 劆UART1 劆SCKE1 劆UART0 劆SCKE0 劔PFR1
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 TOE2 劆 TOE1 劆 TOE0 劆  劒  劆  劒  劆  劒  劆UART4 劆SCKE4 劔PFR2
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 TME3 劆 TME2 劆 TME1 劆 TME0 劆PPGE3 劆PPGE2 劆PPGE1 劆PPGE0 劔PFR3
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 MSE  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劔PFR4
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      PDRn(n:0-7)      _IO_PDRn               側偟

      DDRn(n:0-7)      _IO_PORT_IO_DDRn       側偟

      PFR0             _IO_PORT_IO_PFR0       側偟

      PFR1             _IO_PORT_IO_PFR1       側偟

      PFR2             _IO_PORT_IO_PFR2       側偟

      PFR3             _IO_PORT_IO_PFR3       側偟

      PFR4             _IO_PORT_IO_PFR4       側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲乯  埲壓偵帵偡價僢僩偼懚嵼偟傑偣傫丅

              PDR2,DDR2 : P26-P27
              PDR3,DDR3 : P37
              PDR6,DDR6 : P66-P67
              PDR7,DDR7 : P75-P77

仭侾侽價僢僩俙乛俢僐儞僶乕僞

  丒I/O儗僕僗僞峔惉

      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆0 劆  劆  劔ADCTH,
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗ADCTL
                              劆 STR  劆 ASS2 劆 ASS0 劆      劆 INTE
                             TRG     ASS3    ASS1    BUSY    INT 
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔0 劆0 劆0 劆0 劆0 劆0 劆i9劆i8劆i7劆i6劆i5劆i4劆i3劆i2劆i1劆i0劔ADCH
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔0 劆0 劆0 劆0 劆0 劆0 劆d9劆d8劆d7劆d6劆d5劆d4劆d3劆d2劆d1劆d0劔ADATn
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      ADCTH/ADCHL      _IO_ADCT               側偟

      ADCH             _IO_ADCH               側偟

      ADATn(n:0 - 9)   _IO_ADATn              側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

仭奜晹妱崬傒

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 EN7  劆 EN6  劆 EN5  劆 EN4  劆 EN3  劆 EN2  劆 EN1  劆 EN0  劔ENIR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 ER7  劆 ER6  劆 ER5  劆 ER4  劆 ER3  劆 ER2  劆 ER1  劆 ER0  劔EIRR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔ELVR
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
      劆 LA7  劆 LA6  劆 LA5  劆 LA4  劆 LA3  劆 LA2  劆 LA1  劆 LA0
     LB7     LB6     LB5     LB4     LB3     LB2     LB1     LB0

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      ENIR             _IO_ENIR               側偟

      EIRR             _IO_EIRR               側偟

      ELVR             _IO_ELVR               側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

仭抶墑妱崬傒儌僕儏乕儖

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆 DLYI 劔DICR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      DICR             _IO_DICR               側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

仭妱崬傒僐儞僩儘乕儔

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  劒  劆  劒  劆  劒  劆 ICR4 劆 ICR3 劆 ICR2 劆 ICR1 劆 ICR0 劔ICRn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔MHALTI劆  劒  劆  劒  劆 LVL4 劆 LVL3 劆 LVL2 劆 LVL1 劆 LVL0 劔HRCL
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      ICRn(n:0 - 47)   _IO_ICR_n              側偟

      HRCL             _IO_HRCL               側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲乯  ICRn偺ICR4價僢僩偲HRCL偺LVL4價僢僩偺抣偼侾屌掕偱丄
          侽傪彂崬傓帠偼偱偒傑偣傫丅

仭侾俇價僢僩儕儘乕僪僞僀儅

  丒I/O儗僕僗僞峔惉

      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔劒劆劒劆劒劆劒劆  劆  劆  劆  劆  劆劒劆劒劆  劆  劆  劆  劆  劔TMCSRn
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                      劆 CSL0 劆 MOD1 劆         RELD 劆  UF  劆 TRG
                     CSL1    MOD2    MOD0            INTE    CNTE

      15                                                           0  bit No.
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔TMRn
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔TMRLRn
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      TMCSRn(n:0 - 2)  _IO_TMCSRn             側偟

      TMRn  (n:0 - 2)  _IO_TMRn               側偟

      TMRLRn(n:0 - 2)  _IO_TMRLRn             側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲乯  TMCSRn傊偺彂崬傒傪峴偆帪丄5,12,13bit偵偼
          忢偵抣侽傪彂崬傫偱壓偝偄丅

仭倀俙俼俿

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 MD1  劆 MD0  劆  劒  劆  劒  劆 CS0  劆  劒  劆  劒  劆  劒  劔SMRn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 PEN  劆   P  劆 SBL  劆  CL  劆 A/D  劆 REC  劆 RXE  劆 TXE  劔SCRn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  D7  劆  D6  劆  D5  劆  D4  劆  D3  劆  D2  劆  D1  劆  D0  劔SIDRn/
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗SODRn
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  PE  劆 ORE  劆 FRE  劆 RDRF 劆 TDRE 劆 BDS  劆 RIE  劆 TIE  劔SSRn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劔DRCLn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      SMRn(n:0 - 4)    _IO_SMRn               側偟

      SCRn(n:0 - 4)    _IO_SCRn               側偟

      SIDRn/           _IO_SIDRn              側偟
      SODRn(n:0 - 4)

      SSRn(n:0 - 4)    _IO_SSRn               側偟

      DRCLn(n:0 - 4)   _IO_DRCLn              側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲乯  SMRn傊偺彂崬傒帪偼丄bit1,bit2偵偼抣侽傪丄bit4,bit5偵偼忢偵抣侾傪
          彂崬傫偱壓偝偄丅

仭倀亅俿俬俵俤俼

  丒I/O儗僕僗僞峔惉

      15                                                           0  bit No.
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔UTIMn/
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗UTIMRn

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 UCC1 劆  劒  劆  劒  劆 UTIE 劆 UNDR 劆 CLKS 劆 UTST 劆 UTCR 劔UTIMCn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      UTIMn/           _IO_UTIMn              側偟
      UTIMRn(n:0 - 4)

      UTIMCn(n:0 - 4)  _IO_UTIMCn             側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲乯  UTIMCn傊偺彂崬傒傪峴偆帪丄CLKS價僢僩偵偼忢偵抣侽傪彂崬傫偱壓偝偄丅

仭侾俇價僢僩丒僷儖僗暆僇僂儞僞

  丒I/O儗僕僗僞峔惉

      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆劒劆劒劆  劆  劆  劆  劆劒劆  劆  劆  劆  劆  劔PWCC
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
      劆 INTE 劆OVFLE         劆  ST  劆TEST0   CSFL1 劆 CSK2 劆 CSK0
     INT     OVFL            MSKE   TEST1           CSFL0    CSK1
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔PWCD
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤     1/2/4byte傾僋僙僗梡   價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      PWCC              IO_PWCC               側偟

      PWCD              IO_PWCD               側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

仭俬俬俠僀儞僞乕僼僃乕僗

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 BER  劆 BEIE 劆 SCC  劆 MSS  劆 ACK  劆 GCAA 劆 INTE 劆 INT  劔IBCRn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  BB  劆 RSC  劆  AL  劆 LRB  劆 TRX  劆 AAS  劆 GCA  劆 ADT  劔IBSRn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔劒劆劒劆劒劆劒劆劒劆劒劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔ITBAn
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                              劆 TA8  劆 TA6  劆 TA4  乥 TA2  劆 TA0
                             TA9     TA7     TA5     TA3     TA1
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆劒劆劒劆劒劆劒劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔ITMKn
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
      劆 RAL                  劆 TM8  劆 TM6  劆 TM4  乥 TM2  劆 TM0
     ENTB                    TM9     TM7     TM5     TM3     TM1

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  劒  劆 SA6  劆 SA5  劆 SA4  劆 SA3  劆 SA2  劆 SA1  劆 SA0  劔ISBAn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 ENSB 劆 SM6  劆 SM5  劆 SM4  劆 SM3  劆 SM2  劆 SM1  劆 SM0  劔ISMKn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  D7  劆  D6  劆  D5  劆  D4  劆  D3  劆  D2  劆  D1  劆  D0  劔IDARn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 TEST 劆  劒  劆  EN  劆 CS4  劆 CS3  劆 CS2  劆 CS1  劆 CS0  劔ICCRn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆 DBL  劔IDBLn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      IBCRn(n:0 - 3)   _IO_IBCRn              側偟

      IBSRn(n:0 - 3)   _IO_IBSRn              側偟

      ITBAn(n:0 - 3)   _IO_ITBAn              側偟

      ITMKn(n:0 - 3)   _IO_ITMKn              側偟

      ISBAn(n:0 - 3)   _IO_ISBAn              側偟

      ISMKn(n:0 - 3)   _IO_ISMKn              側偟

      IDARn(n:0 - 3)   _IO_IDARn              側偟

      ICCRn(n:0 - 3)   _IO_ICCRn              側偟

      IDBLn(n:0 - 3)   _IO_IDBLn              側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲乯  ICCRn傊偺彂崬傒傪峴偆帪丄TEST價僢僩偲俇價僢僩偵偼
          忢偵抣侽傪彂崬傫偱壓偝偄丅

仭懡婡擻僞僀儅

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆 FCn1 劆 FCn0 劆 FnEN 劔TnLPCR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 CPF  劆  劒  劆 CPST 劆 CPED 劆 CPIE 劆 CPOV 劆 CPMD 劆 CPIS 劔TnCCR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 TCF  劆 TSES 劆 TCC  劆 TIE  劆 CINV 劆 TCS2 劆 TCS1 劆 TCS0 劔TnTCR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  劒  劆  劒  劆  劒  劆 TST2 劆 TST2 劆 MD1  劆 MD0  劆  ST  劔TnR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

      15                                                          0   bit No.
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔TnDRR
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔TnCRR
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      TnLPCR(n:0 - 3)  _IO_TnLPCR             側偟

      TnCCR(n:0 - 3)   _IO_TnCCR              側偟

      TnTCR(n:0 - 3)   _IO_TnTCR              側偟

      TnR  (n:0 - 3)   _IO_TnR                側偟

      TnDRR(n:0 - 3)   _IO_TnDRR              側偟

      TnCRR(n:0 - 3)   _IO_TnCRR              側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲乯  TnR傊彂崬傒傪峴偆帪丄TST1,TST2價僢僩偵偼
          忢偵抣侽傪彂崬傫偱壓偝偄丅

仭俹俹俧僞僀儅

  丒I/O儗僕僗僞峔惉

      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆劒劆  劆  劆  劆  劆  劆  劆劒劆  劔PCNn
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
      乥 STGR 乥 RTRG 劆 CKS0 劆      劆 EGS0 劆 IRQF 乥 IRS0    OSEL
     CNTE    MDSE    CKS1    PGMS    EGS1    IREN    IRS1
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔PCSRn,
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗PDUTn
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔PTMRn
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      PCNn (n:0 - 3)   _IO_PCNn               側偟

      PCSRn(n:0 - 3)   _IO_PCSRn              側偟

      PDUTn(n:0 - 3)   _IO_PDUTn              側偟

      PTMRn(n:0 - 3)   _IO_PTMRn              側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

仭俢俵俙俠乮俢俵俙僐儞僩儘乕儔乯

  丒I/O儗僕僗僞峔惉

      31  30  29  28  27  26  25  24  23  22  21  20  19  18  17  16  bit No.
    劕劒劧劒劧劒劧劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劧
    劔  劆  劆  劆      IS[4:0]     劆  DDNO[3:0]   劆   BLK[3:0]   劆
    劘劒劯劒劯劒劯劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劯
      劆 PAUS 劆
     DENB    STRG
        15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
      劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
      劆                          DTC[15:0]                           劔DMACAn
      劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

      31  30  29  28  27  26  25  24  23  22  21  20  19  18  17  16  bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劒劒劒劒劧
    劔 TYPE 劆 MOD  劆  WS  劆  劆  劆  劆  劆  劆  劆  劆 DSS[2:0] 劆
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劒劒劒劒劯
                              劆 DADM 劆 SADR 劆 ERIE 劆
                             SADM    DTCR    DADR    EDIE
        15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
      劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
      劆          SASZ[7:0]           劆          DASZ[7:0]           劔DMACBn
      劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

      31  30  29  28  27  26  25  24  23  22  21  20  19  18  17  16  bit No.
    劕劒劧劒劧劒劧劒劧劒劒劒劒劒劒劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧
    劔  劆劒劆劒劆  劆  DMAH[3:0]   劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆
    劘劒劯劒劯劒劯劒劯劒劒劒劒劒劒劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯
     DMAE        PM01
        15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
      劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
      劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劔DMACR
      劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗

      31                                                           0  bit No.
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔DMASAn,
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗DMADAn

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      DMACAn(n:0 - 4)  _IO_DMACAn             側偟

      DMACBn(n:0 - 4)  _IO_DMACBn             側偟

      DMACR            _IO_DMACR              側偟

      DMASAn(n:0 - 4)  _IO_DMAD_IO_DMASAn     側偟

      DMADAn(n:0 - 4)  _IO_DMAD_IO_DMADAn     側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

仭價僢僩僒乕僠儌僕儏乕儖

  丒I/O儗僕僗僞峔惉

      31                                                           0  bit No.
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔BSD0
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔BSD1
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔BSDC
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔BSRR
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      BSD0             _IO_BSD0               側偟

      BSD1             _IO_BSD1               側偟

      BSDC             _IO_BSDC               側偟

      BSRR             _IO_BSRR               側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

仭僋儘僢僋惗惉惂屼晹

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 INIT 劆  劒  劆 WDOG 劆  劒  劆 SRST 劆  劒  劆 WT1  劆 WT0  劔RSRR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 STOP 劆SLEEP 劆 HIZ  劆 SRST 劆 OS1  劆 OS0  劆OSCD2 劆OSCD1 劔STCR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 TBIF 劆 TBIE 劆 TBC2 劆 TBC1 劆 TBC0 劆  劒  劆SYNCR 劆SYNCS 劔TBCR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  D7  劆  D6  劆  D5  劆  D4  劆  D3  劆  D2  劆  D1  劆  D0  劔CTBR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔PLL2S0劆PLL1S2劆PLL1S1劆PLL1S0劆PLL2EN劆PLL1EN劆CLKS1 劆CLKS0 劔CLKR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  D7  劆  D6  劆  D5  劆  D4  劆  D3  劆  D2  劆  D1  劆  D0  劔WPR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  B3  劆  B2  劆  B1  劆  B0  劆  P3  劆  P2  劆  P1  劆  P0  劔DIVR0
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  T3  劆  T2  劆  T1  劆  T0  劆  劒  劆  劒  劆  劒  劆  劒  劔DIVR1
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劆OSCDS1劔OSCCR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      RSRR             _IO_CLK_IO_RSRR        側偟

      STCR             _IO_CLK_IO_STCR        側偟

      TBCR             _IO_CLK_IO_TBCR        側偟

      CTBR             _IO_CLK_IO_CTBR        側偟

      CLKR             _IO_CLK_IO_CLKR        側偟

      WPR              _IO_CLK_IO_WPR         側偟

      DIVR0            _IO_CLK_IO_DIVR0       側偟

      DIVR1            _IO_CLK_IO_DIVR1       側偟

      OSCCR            _IO_CLK_IO_OSCCR       側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

仭帪寁僞僀儅

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 WIF  劆 WIE  劆  劒  劆  劒  劆  劒  劆 WS1  劆 WS0  劆 WCL  劔WPCR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      WPCR             _IO_WPCR               側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲乯  WPCR傊偺彂崬傒傪峴偆帪丄bit3-bit5偵偼忢偵抣侽傪彂崬傫偱壓偝偄丅

仭儊僀儞敪怳埨掕懸偪僞僀儅

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 WIF  劆 WIE  劆  劒  劆  劒  劆  劒  劆 WS1  劆 WS0  劆 WCL  劔OSCR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      OSCR             _IO_OSCR               側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲乯  OSCR傊偺彂崬傒傪峴偆帪丄bit3-bit5偵偼忢偵抣侽傪彂崬傫偱壓偝偄丅

仭奜晹僶僗僀儞僞乕僼僃乕僗

  丒I/O儗僕僗僞峔惉

      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔ASRn
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
      劆 A30  劆 A28  劆 A26  劆 A24  劆 A22  劆 A20  劆 A18  劆 A16
     A31     A29     A27     A25     A23     A21     A19     A17
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔ACRn
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
      劆 ASZ2 劆 ASZ0 劆 DBW0 劆 BST0 劆 PFEN 劆 LEND 劆 TYP2 劆 TYP0
     ASZ3    ASZ1    DBW1    BST1    SREN    WREN    TYP3    TYP1
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔AWRn
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
      劆 W14  劆 W12  劆 W10  劆 W08  劆 W06  劆 W04  劆 W02  劆 W00
     W15     W13     W11     W09     W07     W05     W03     W01

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 RYEn 劆 HLDn 劆 WRn1 劆 WRn0 劆 IWn3 劆 IWn2 劆 IWn1 劆 IWn0 劔IOWRn
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 CSE7 劆 CSE6 劆 CSE5 劆 CSE4 劆 CSE3 劆 CSE2 劆 CSE1 劆 CSE0 劔CSER
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 CHE7 劆 CHE6 劆 CHE5 劆 CHE4 劆 CHE3 劆 CHE2 劆 CHE1 劆 CHE0 劔CHER
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 BREN 劆 PSUS 劆 PCLR 劆 梊栺 劆 OHT1 劆 OHT0 劆 RWD1 劆 RWD0 劔TCR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
     I/O儗僕僗僞柤   1/2/4byte傾僋僙僗梡   價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
     ASRn(n:0 - 7)   _IO_EBUS_IO_ASRn      側偟

     ACRn(n:0 - 7)   _IO_EBUS_IO_ACRn      側偟

     AWRn(n:0 - 7)   _IO_EBUS_IO_AWRn      側偟

     IOWRn(n:0 - 2)  _IO_EBUS_IO_IOWRn     側偟

     CSER            _IO_EBUS_IO_CSER      側偟

     CHER            _IO_EBUS_IO_CHER      側偟

     TCR             _IO_EBUS_IO_TCR       側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲乯  TCR傊偺彂崬傒傪峴偆帪丄梊栺價僢僩偵偼忢偵抣侽傪彂崬傫偱壓偝偄丅

仭儌乕僪僨乕僞

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  *   劆  *   劆  *   劆  *   劆  *   劆 ROMA 劆 WTH1 劆 WTH0 劔MODR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      MODR             _IO_MODR               側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲乯  *價僢僩偵偼丄忢偵抣侽傪彂崬傫偱壓偝偄丅

仭僼儔僢僔儏儊儌儕惂屼

  丒I/O儗僕僗僞峔惉

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  劒  劆  劒  劆  劒  劆  劒  劆 RDY  劆  劒  劆  WE  劆  劒  劔FLCR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔  劒  劆  劒  劆 FAC1 劆 FAC0 劆  劒  劆 WTC1 劆 WTC1 劆 WTC0 劔FLWC
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      FLCR             _IO_FLCR               側偟

      FLWC             _IO_FLWC               側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      拲侾乯  FLCR傊偺彂崬傒傪峴偆帪丄bit2,4,7偵偼抣侽傪bit5,6偵偼抣侾傪
            彂崬傫偱壓偝偄丅
      拲俀乯  FLWC傊偺彂崬傒傪峴偆帪丄bit3,6,7偵偼抣侽傪彂崬傫偱壓偝偄丅

仭倀俽俛儂僗僩

  丒I/O儗僕僗僞峔惉

    31                              8   7   6   5   4   3   2   1   0   bit No.
  劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
  劔                劒                劆             REV              劔HR
  劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

    31                  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劒劒劒劒劒劒劒劒劒劒劧劒劧劒劧劒劧劒劒劒劧劒劧劒劧劒劧劒劧劒劒劒劖
  劔          劒          劆  劆  劆IR劆 HCFS 劆  劆  劆IE劆  劆 CBSR 劔HC
  劘劒劒劒劒劒劒劒劒劒劒劒劯劒劯劒劯劒劯劒劒劒劯劒劯劒劯劒劯劒劯劒劒劒劗
                           RWE RWC             BLE CLE     PLE

    31    18  17  16  15                            4   3   2   1   0   bit No.
  劕劒劒劒劒劧劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劧劒劧劒劧劒劖
  劔        劆 SOC  劆                     劒         劆  劆  劆  劆  劔HCS
  劘劒劒劒劒劯劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劯劒劯劒劯劒劗
                                                       OCR BLF CLF HCR

    31  30  29                          7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔劒劆OC劆              劒              劆  劆  劆UE劆RD劆SF劆  劆SO劔HIS
  劘劒劯劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                                          RHSC FNO             WDH
  劕劒劧劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔  劆OC劆              劒              劆  劆  劆UE劆RD劆SF劆  劆SO劔HIE
  劘劒劯劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
   MIE                                    RHSC FNO             WDH
  劕劒劧劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔ME劆OC劆              劒              劆  劆  劆UE劆RD劆SF劆  劆SO劔HID
  劘劒劯劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                                          RHSC FNO             WDH

    31                              8   7                           0   bit No.
  劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
  劔               HCCA               劆              劒              劔HHCCA
  劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

    31                                          4   3               0   bit No.
  劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劖
  劔                       PCED                   劆        劒        劔HPCED
  劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劗
  劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劖
  劔                       CHED                   劆        劒        劔HCHED
  劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劗
  劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劖
  劔                       CCED                   劆        劒        劔HCCED
  劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劗
  劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劖
  劔                       BHED                   劆        劒        劔HBHED
  劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劗
  劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劖
  劔                       BCED                   劆        劒        劔HBCED
  劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劗
  劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劖
  劔                        DH                    劆        劒        劔HDH
  劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劗

    31  30                  16  15  14  13                          0   bit No.
  劕劒劧劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
  劔  劆          FSMPS       劆  劒  劆                FI            劔HFI
  劘劒劯劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗
   FIT
    31  30                          14  13                          0   bit No.
  劕劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
  劔  劆                 劒           劆                FR            劔HFR
  劘劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗
   FRT
    31                    16  15                                    0   bit No.
  劕劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
  劔              劒        劆                      FN                劔HFN
  劘劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗
    31                            14  13                            0   bit No.
  劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
  劔              劒                劆              PS                劔HPS
  劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗
    31                                    12  11                    0   bit No.
  劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劖
  劔              劒                        劆            LST         劔HLST
  劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劗

    31    24  23                      13  12  11  10  9   8   7     0   bit No.
  劕劒劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劧劒劧劒劧劒劧劒劧劒劒劒劒劖
  劔 POTPGT 劆             劒           劆  劆  劆DT劆  劆  劆  NDP   劔HRDA
  劘劒劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劯劒劯劒劯劒劯劒劯劒劒劒劒劗
                                        NOCP OCPM    NPS PSM
    31                    16  15                                    0   bit No.
  劕劒劒劒劒劒劒劒劒劒劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
  劔         PPCM           劆                      DR                劔HRDB
  劘劒劒劒劒劒劒劒劒劒劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

    31  30        18  17  16  15  14                        2   1   0   bit No.
  劕劒劧劒劒劒劒劒劒劧劒劧劒劧劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劧劒劖
  劔  劆     劒     劆  劆  劆  劆               劒           劆  劆  劔HRS
  劘劒劯劒劒劒劒劒劒劯劒劯劒劯劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劯劒劗
   CWRE             OCIC LPSC DRWE                             OCI LPS

    31  30  29  28  27  26  25  24  23  22  21  20  19  18  17  16      bit No.
  劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劧劒劧劒劧劒劧劒劧劒劧
  劔                      劒                  劆  劆  劆  劆  劆  劆
  劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劯劒劯劒劯劒劯劒劯劒劯
                                               PRSC 劆 PSSC 劆 CSC
                                                   OCIC    PESC
        15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
      劧劒劒劒劒劒劒劒劒劒劒劒劧劒劧劒劧劒劒劒劒劒劧劒劧劒劧劒劧劒劧劒劖
      劆          劒          劆  劆  劆    劒    劆  劆  劆  劆  劆  劔HRPSn
      劯劒劒劒劒劒劒劒劒劒劒劒劯劒劯劒劯劒劒劒劒劒劯劒劯劒劯劒劯劒劯劒劗
                              LSDA PPS            PRS POCI PSS PES CCS

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤    1/2/4byte傾僋僙僗梡    價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      HR               _IO_USBH_IO_HR         側偟

      HC               _IO_USBH_IO_HC         側偟

      HCS              _IO_USBH_IO_HCS        側偟

      HIS              _IO_USBH_IO_HIS        側偟

      HIE              _IO_USBH_IO_HIE        側偟

      HID              _IO_USBH_IO_HID        側偟

      HHCCA            _IO_USBH_IO_HHCCA      側偟

      HPCED            _IO_USBH_IO_HPCED      側偟

      HCHED            _IO_USBH_IO_HCHED      側偟

      HCCED            _IO_USBH_IO_HCCED      側偟

      HBHED            _IO_USBH_IO_HBHED      側偟

      HBCED            _IO_USBH_IO_HBCED      側偟

      HDH              _IO_USBH_IO_HDH        側偟

      HFI              _IO_USBH_IO_HFI        側偟

      HFR              _IO_USBH_IO_HFR        側偟

      HFN              _IO_USBH_IO_HFN        側偟

      HPS              _IO_USBH_IO_HPS        側偟

      HLST             _IO_USBH_IO_HLST       側偟

      HRDA             _IO_USBH_IO_HRDA       側偟

      HRDB             _IO_USBH_IO_HRDB       側偟

      HRS              _IO_USBH_IO_HRS        側偟

      HRPSn(n:1 - 2)   _IO_USBH_IO_HRPSn      側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

仭倀俽俛僼傽儞僋僔儑儞

  丒I/O儗僕僗僞峔惉

      15                                                          0   bit No.
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔FIFO0o,
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗FIFO0i
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔FIFOn
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆N 劆A 劆N 劆A 劆N 劆A 劆N 劆A 劆N 劆A 劔
    劔  劆  劆  劆  劆  劆  劆A 劆C 劆A 劆C 劆A 劆C 劆A 劆C 劆A 劆C 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆C 劆K 劆C 劆K 劆C 劆K 劆C 劆K 劆C 劆K 劔ST1
    劔  劆  劆  劆  劆  劆  劆K 劆3 劆K 劆2 劆K 劆1 劆K 劆0 劆K 劆0 劔
    劔  劆  劆  劆  劆  劆  劆3 劆  劆2 劆  劆1 劆  劆0 劆i 劆0 劆o 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆i 劆  劆o 劆  劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆D 劆D 劆D 劆D 劆D 劆D 劆D 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆C 劆C 劆C 劆C 劆C 劆C 劆C 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆T 劆T 劆T 劆T 劆T 劆T 劆T 劔ST2
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆6 劆5 劆4 劆3 劆2 劆1 劆0 劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆S 劆C 劆S 劆S 劆N 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆E 劆F 劆O 劆U 劆A 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆T 劆E 劆F 劆S 劆C 劔ST3
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆U 劆N 劆  劆F 劆K 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆P 劆D 劆  劆  劆O 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆S 劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆F 劆F 劆F 劆F 劆F 劆F 劆F 劆F 劆F 劆F 劆F 劔
    劔  劆  劆  劆  劆  劆M 劆M 劆M 劆M 劆M 劆M 劆M 劆M 劆M 劆M 劆M 劔
    劔劒劆劒劆劒劆劒劆劒劆R 劆R 劆R 劆R 劆R 劆R 劆R 劆R 劆R 劆R 劆R 劔ST4
    劔  劆  劆  劆  劆  劆1 劆9 劆8 劆7 劆6 劆5 劆4 劆3 劆2 劆1 劆0 劔
    劔  劆  劆  劆  劆  劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆U 劆  劆  劆  劆  劆  劆S 劆S 劆S 劆S 劆T 劆T 劔
    劔  劆  劆  劆  劆S 劆  劆  劆  劆  劆  劆T 劆T 劆T 劆T 劆R 劆T 劔
    劔  劆  劆  劆  劆B 劆  劆  劆  劆  劆  劆S 劆S 劆S 劆S 劆C 劆R 劔
    劔劒劆劒劆劒劆劒劆R 劆劒劆劒劆劒劆劒劆劒劆T 劆T 劆T 劆T 劆V 劆S 劔ST5
    劔  劆  劆  劆  劆E 劆  劆  劆  劆  劆  劆A 劆A 劆A 劆A 劆E 劆E 劔
    劔  劆  劆  劆  劆S 劆  劆  劆  劆  劆  劆L 劆L 劆L 劆L 劆N 劆N 劔
    劔  劆  劆  劆  劆E 劆  劆  劆  劆  劆  劆L 劆L 劆L 劆L 劆D 劆D 劔
    劔  劆  劆  劆  劆T 劆  劆  劆  劆  劆  劆3 劆2 劆1 劆0 劆  劆  劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆R 劆R 劆R 劆R 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆S 劆S 劆S 劆S 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆I 劆I 劆I 劆I 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆Z 劆Z 劆Z 劆Z 劔RSIZE0
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆E 劆E 劆E 劆E 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆0 劆0 劆0 劆0 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆3 劆2 劆1 劆0 劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆R 劆R 劆R 劆R 劆R 劆R 劆R 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆S 劆S 劆S 劆S 劆S 劆S 劆S 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆I 劆I 劆I 劆I 劆I 劆I 劆I 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆Z 劆Z 劆Z 劆Z 劆Z 劆Z 劆Z 劔RSIZE1
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆E 劆E 劆E 劆E 劆E 劆E 劆E 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆1 劆1 劆1 劆1 劆1 劆1 劆1 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆6 劆5 劆4 劆3 劆2 劆1 劆0 劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆R 劆  劆  劆  劆  劆  劆S 劆S 劆S 劆S 劆C 劔
    劔  劆  劆  劆  劆  劆E 劆  劆  劆  劆  劆  劆T 劆T 劆T 劆T 劆F 劔
    劔  劆  劆  劆  劆  劆S 劆  劆  劆  劆  劆  劆A 劆A 劆A 劆A 劆G 劔
    劔劒劆劒劆劒劆劒劆劒劆U 劆劒劆劒劆劒劆劒劆劒劆L 劆L 劆L 劆L 劆E 劔CONT1
    劔  劆  劆  劆  劆  劆M 劆  劆  劆  劆  劆  劆L 劆L 劆L 劆L 劆N 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆3 劆2 劆1 劆0 劆  劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆I 劆I 劆I 劆I 劆I 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆N 劆N 劆N 劆N 劆N 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆I 劆I 劆I 劆I 劆I 劔CONT2
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆3 劆2 劆1 劆0 劆0 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆i 劆o 劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆B 劆B 劆B 劆B 劆B 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆F 劆F 劆F 劆F 劆F 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆O 劆O 劆O 劆O 劆O 劔CONT3
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆K 劆K 劆K 劆K 劆K 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆3 劆2 劆1 劆0 劆0 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆i 劆o 劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆B 劆B 劆B 劆B 劆B 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆I 劆I 劆I 劆I 劆I 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆F 劆F 劆F 劆F 劆F 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆O 劆O 劆O 劆O 劆O 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆B 劆B 劆B 劆B 劆B 劔CONT3
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆U 劆U 劆U 劆U 劆U 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆S 劆S 劆S 劆S 劆S 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆Y 劆Y 劆Y 劆Y 劆Y 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆3 劆2 劆1 劆0 劆0 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆i 劆o 劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆F 劆F 劆F 劆F 劆F 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆I 劆I 劆I 劆I 劆I 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆F 劆F 劆F 劆F 劆F 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆O 劆O 劆O 劆O 劆O 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆B 劆B 劆B 劆B 劆B 劔CONT4
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆U 劆U 劆U 劆U 劆U 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆S 劆S 劆S 劆S 劆S 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆Y 劆Y 劆Y 劆Y 劆Y 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆3 劆2 劆1 劆0 劆0 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆i 劆o 劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆D 劆D 劆  劆  劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆I 劆I 劆  劆  劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆F 劆F 劆  劆  劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆O 劆O 劆  劆  劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆B 劆B 劆劒劆劒劔CONT5
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆U 劆U 劆  劆  劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆S 劆S 劆  劆  劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆Y 劆Y 劆  劆  劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆2 劆1 劆  劆  劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆M 劆M 劆  劆  劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆D 劆D 劆  劆  劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆R 劆R 劆劒劆劒劔CONT6
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆E 劆E 劆  劆  劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆Q 劆Q 劆  劆  劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆2 劆1 劆  劆  劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆M 劆M 劆M 劆M 劆M 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆A 劆A 劆A 劆A 劆A 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆C 劆C 劆C 劆C 劆C 劔CONT7
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆K 劆K 劆K 劆K 劆K 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆3 劆2 劆1 劆0 劆0 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆i 劆o 劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆M 劆M 劆M 劆M 劆M 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆N 劆N 劆N 劆N 劆N 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆A 劆A 劆A 劆A 劆A 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆C 劆C 劆C 劆C 劆C 劔CONT8
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆K 劆K 劆K 劆K 劆K 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆3 劆2 劆1 劆0 劆0 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆i 劆o 劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆M 劆  劆  劆  劆  劆M 劆M 劆M 劆M 劔
    劔  劆  劆  劆  劆  劆  劆  劆U 劆  劆  劆  劆  劆S 劆S 劆S 劆S 劔
    劔  劆  劆  劆  劆  劆  劆  劆S 劆  劆  劆  劆  劆T 劆T 劆T 劆T 劔
    劔  劆  劆  劆  劆  劆  劆  劆B 劆  劆  劆  劆  劆A 劆A 劆A 劆A 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆R 劆劒劆劒劆劒劆劒劆L 劆L 劆L 劆L 劔CONT9
    劔  劆  劆  劆  劆  劆  劆  劆E 劆  劆  劆  劆  劆L 劆L 劆L 劆L 劔
    劔  劆  劆  劆  劆  劆  劆  劆S 劆  劆  劆  劆  劆3 劆2 劆1 劆0 劔
    劔  劆  劆  劆  劆  劆  劆  劆E 劆  劆  劆  劆  劆  劆  劆  劆  劔
    劔  劆  劆  劆  劆  劆  劆  劆T 劆  劆  劆  劆  劆  劆  劆  劆  劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆N 劆N 劆N 劆D 劆  劆L 劆L 劆L 劆T 劆T 劆O 劆  劔
    劔  劆  劆  劆  劆U 劆U 劆U 劆M 劆  劆S 劆S 劆S 劆R 劆T 劆D 劆  劔
    劔  劆  劆  劆  劆L 劆L 劆L 劆A 劆  劆T 劆T 劆T 劆C 劆C 劆D 劆  劔
    劔劒劆劒劆劒劆劒劆L 劆L 劆L 劆M 劆劒劆D 劆D 劆D 劆N 劆N 劆  劆劒劔CONT10
    劔  劆  劆  劆  劆S 劆S 劆S 劆O 劆  劆3 劆2 劆0 劆T 劆T 劆  劆  劔
    劔  劆  劆  劆  劆E 劆E 劆E 劆D 劆  劆  劆  劆  劆E 劆E 劆  劆  劔
    劔  劆  劆  劆  劆T 劆T 劆T 劆E 劆  劆  劆  劆  劆N 劆N 劆  劆  劔
    劔  劆  劆  劆  劆3 劆2 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗

      15                                                          0   bit No.
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔TTSIZE
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                                                              劔TRSIZE
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆S 劆R 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆U 劆E 劔
    劔劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆劒劆S 劆S 劔RESET
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆P 劆E 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆E 劆T 劔
    劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆N 劆X 劔
    劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤  1/2/4byte傾僋僙僗梡      價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      FIFO0o         _IO_USBF_IO_FIFO0o       側偟
      FIFO0i         _IO_USBF_IO_FIFO0i       側偟
      FIFOn(n:1 - 3) _IO_USBF_IO_FIFOn        側偟

      ST1            _IO_USBF_IO_ST1          側偟
      ST2            _IO_USBF_IO_ST2          側偟
      ST3            _IO_USBF_IO_ST3          側偟
      ST4            _IO_USBF_IO_ST4          側偟
      ST5            _IO_USBF_IO_ST5          側偟

      RSIZE0         _IO_USBF_IO_RSIZE0       側偟
      RSIZE1         _IO_USBF_IO_RSIZE1       側偟

      CONT1          _IO_USBF_IO_CONT1        側偟
      CONT2          _IO_USBF_IO_CONT2        側偟
      CONT3          _IO_USBF_IO_CONT3        側偟
      CONT4          _IO_USBF_IO_CONT4        側偟
      CONT5          _IO_USBF_IO_CONT5        側偟
      CONT6          _IO_USBF_IO_CONT6        側偟
      CONT7          _IO_USBF_IO_CONT7        側偟
      CONT8          _IO_USBF_IO_CONT8        側偟
      CONT9          _IO_USBF_IO_CONT9        側偟
      CONT10         _IO_USBF_IO_CONT10       側偟

      TTSIZE         _IO_USBF_IO_TTSIZE       側偟
      TRSIZE         _IO_USBF_IO_TRSIZE       側偟

      RESET          _IO_USBF_IO_RESET        側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

仭儊儌儕乕僗僥傿僢僋

  丒I/O儗僕僗僞峔惉

      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劒劒劒劒劒劒劧劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔     PID      劆      劆              DATASIZE                劔MSCR
    劘劒劒劒劒劒劒劒劯劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 INT  劆 DRQ  劆  劒  劆  劒  劆 RBE  劆 RBF  劆 TBE  劆 TBF  劔MSSR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劒劒劒劒劒劒劒劒劖
    劔 RST  劆 PWS  劆 SIEN 劆DAKEN 劆NONCRC劆        BSYCNT        劔MSCNTR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劒劒劒劒劒劒劒劒劗

      15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
    劕劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劖
    劔                          RTDB[0:15]                          劔MSRTDR
    劘劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劗

        7       6       5       4       3       2       1       0     bit No.
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 RDY  劆 SIF  劆 DREQ 劆 PIN  劆  劒  劆  劒  劆 CRC  劆 TOE  劔MSIDR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔 INT  劆 DREQ 劆 PIN  劆  劒  劆  劒  劆  劒  劆  劒  劆  劒  劔MSIR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔XPIN3 劆XPIN2 劆XPIN1 劆XPIN0 劆POUT3 劆POUT2 劆POUT1 劆POUT0 劔MSPPDR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗
    劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
    劔PIEN3 劆PIEN2 劆PIEN1 劆PIEN0 劆POEN3 劆POEN2 劆POEN1 劆POEN0 劔MSPPCR
    劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗


  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      I/O儗僕僗僞柤  1/2/4byte傾僋僙僗梡      價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
      MSCR           _IO_MEMS_IO_MSCR         側偟

      MSSR           _IO_MEMS_IO_MSSR         側偟

      MSCNTR         _IO_MEMS_IO_MSCNTR       側偟

      MSRTDR         _IO_MEMS_IO_MSRTDR       側偟

      MSIDR          _IO_MEMS_IO_MSIDR        側偟

      MSIR           _IO_MEMS_IO_MSIR         側偟

      MSPPDR         _IO_MEMS_IO_MSPPDR       側偟

      MSPPCR         _IO_MEMS_IO_MSPPCR       側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

仭俷俽俢俠

  丒I/O儗僕僗僞峔惉

    15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔FL劆0 劆0 劆0 劆  劆  劆  劆  劆0 劆0 劆  劆  劆  劆  劆  劆  劔OSD_VADR
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                    劆 AY2  劆 AY0          劆 AX4  劆 AX2  劆 AX0
                   AY3     AY1             AX5     AX3     AX1
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_CD1
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劆 MUL  劆 MBB  劆 MS0  劆 MM0  劆 MB2  劆 MB0  劆 MC2  劆 MC0
   MIT     MBL     MS1     MM1     MB3     MB1     MC3     MC1
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔MR劆MG劆0 劆0 劆0 劆  劆M9劆M8劆M7劆M6劆M5劆M4劆M3劆M2劆M1劆M0劔OSD_CD2
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                       M10

    15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆  劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_RCD1
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
               LHS     LW2  劆 LW0  劆 LFC  劆 LFA  劆 LF2  劆 LF0
                           LW1     LFD     LFB     LF3     LF1
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆  劆  劆  劆  劆  劆LD劆LE劆  劆  劆L3劆L2劆L1劆L0劔OSD_RCD2
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
               LDS  劆 LGY0 劆 LGX0         劆 LM0
                   LGY1    LGX1            LM1

    15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆0 劆0 劆0 劆0 劔OSD_SOC1
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                                    劆 UDS  劆 DSP
                                   SDS     PDS
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆0 劆0 劆0 劆0 劔OSD_SOC2
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                            劆 FM0  劆 BT0  劆 BD0
                           FM1     BT1     BD1

    15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆Y8劆Y7劆Y6劆Y5劆Y4劆Y3劆Y2劆Y1劆Y0劔OSD_VDPC
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆X8劆X7劆X6劆X5劆X4劆X3劆X2劆X1劆X0劔OSD_HDPC
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆0 劆  劆  劆  劔OSD_CVSC
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                                       HB2  劆 HB0     HA2  劆 HA0
                                           HB1             HA1

    15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_SBFCC
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                                    劆 BH2  劆 BH0  劆 BS2  劆 BS0
                                   BH3     BH1     BS3     BS1
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_THCC
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                            劆 HCC  劆 TCC2 劆 TCC0 劆 HCC2 劆 HCC0
                           TCC     TCC3    TCC1    HCC3    HCC1
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_GFCC
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                            劆 GCC  劆 GFC2 劆 GFC0 劆 GC2  劆 GC0
                           GFC     GFC3    GFC1    GC3     GC1 

    15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔  劆0 劆  劆  劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_SBCC1
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劆      劆 PD0     PM10 劆 PM8  劆 PM6  劆 PM4  劆 PM2  劆 PM0
   PCUT    PD1             PM9     PM7     PM5     PM3     PM1 
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆U3劆U2劆U1劆U0劔OSD_SBCC2
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                                       PH2  劆 PH0
                                           PH1

    15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔  劆0 劆  劆  劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_SPCC1
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
    劆      劆 SD0     SM10 劆 SM8  劆 SM6  劆 SM4  劆 SM2  劆 SM0
   SCUT    SD1             SM9     SM7     SM5     SM3     SM1 
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆  劆0 劆  劆  劆  劆0 劆0 劆0 劆0 劔OSD_SPCC2
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                               SBL     SH2  劆 SH0
                                           SH1
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_SPCC3
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                            劆 SY8  劆 SY6  劆 SY4  劆 SY2  劆 SY0
                           SY9     SY7     SY5     SY3     SY1 
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_SPCC4
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                            劆 SX8  劆 SX6  劆 SX4  劆 SX2  劆 SX0
                           SX9     SX7     SX5     SX3     SX1 

    15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆IN劆0 劆FC劆0 劆0 劆0 劆0 劔OSD_SYNCC
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆0 劆0 劆  劆  劔OSD_DCLKC1
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                                    劆 DR0  劆 DP0          劆 DC0
                                   DR1     DP1             DHRS
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_DCLKC2
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                    劆 DK10 劆 DK8  劆 DK6  劆 DK4  劆 DK2  劆 DK0
                   DK11    DK9     DK7     DK5     DK3     DK1 
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_DCLKC3
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                                    劆 VSL2 劆 VSL0 劆 CPB0 劆 PDE
                                    VC     VSL1    CPB1    CPE 

    15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劔OSD_IOC1
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                                                       OHX  劆 OCX
                                                           OBX
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆  劆  劆0 劆0 劆0 劆0 劆  劆  劆0 劔OSD_IOC2
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                               VHE  劆                 IHX  劆
                                    HE                     IVX

    15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_DPC1
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                      DYS10 劆 DYS8 劆 DYS6 劆 DYS4 劆 DYS2 劆 DYS0
                           DYS9    DYS7    DYS5    DYS3    DYS1
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_DPC2
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                      DYE10 劆 DYE8 劆 DYE6 劆 DYE4 劆 DYE2 劆 DYE0
                           DYE9    DYE7    DYE5    DYE3    DYE1
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_DPC3
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                      DXS10 劆 DXS8 劆 DXS6 劆 DXS4 劆 DXS2 劆 DXS0
                           DXS9    DXS7    DXS5    DXS3    DXS1
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劆  劔OSD_DPC4
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                      DXE10 劆 DXE8 劆 DXE6 劆 DXE4 劆 DXE2 劆 DXE0
                           DXE9    DXE7    DXE5    DXE3    DXE1

    15  14  13  12  11  10  9   8   7   6   5   4   3   2   1   0   bit No.
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆  劆  劆  劆0 劆0 劆0 劆0 劆0 劆  劆  劆  劔OSD_JRC
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                       FIF  劆 VIF                     FIE  劆 VIE
                           LIF                             LIE
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆  劆  劆  劆0 劆  劆  劆  劆0 劆  劆  劆  劔OSD_PLTn
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                       PLR2 劆 PLR0    PLG2 劆 PLG0    PLB2 劆 PLB0
                           PLR1            PLG1            PLB1
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆  劆0 劆0 劆0 劆  劔OSD_ACT1
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                                               DCK             DPD
  劕劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劧劒劖
  劔0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆0 劆  劆0 劆  劆  劆  劔OSD_ACT2
  劘劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劯劒劗
                                              OSDEN    FHO  劆 ANO
                                                           DGO

  丒巊梡壜擻側曄悢柤偍傛傃儊儞僶柤

    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
    儗僕僗僞   1/2/4byte傾僋僙僗梡         價僢僩傾僋僙僗梡
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
    OSD_VADR   _IO_OSDC_IO_OSD_VADR        側偟

    OSD_CD1    _IO_OSDC_IO_OSD_CD1         側偟
    OSD_CD2    _IO_OSDC_IO_OSD_CD2         側偟

    OSD_RCD1   _IO_OSDC_IO_OSD_RCD1        側偟
    OSD_RCD2   _IO_OSDC_IO_OSD_RCD2        側偟

    OSD_SOC1   _IO_OSDC_IO_OSD_SOC1        側偟
    OSD_SOC2   _IO_OSDC_IO_OSD_SOC2        側偟

    OSD_VDPC   _IO_OSDC_IO_OSD_VDPC        側偟
    OSD_HDPC   _IO_OSDC_IO_OSD_HDPC        側偟

    OSD_CVSC   _IO_OSDC_IO_OSD_CVSC        側偟

    OSD_SBFCC  _IO_OSDC_IO_OSD_SBFCC       側偟

    OSD_THCC   _IO_OSDC_IO_OSD_THCC        側偟

    OSD_GFCC   _IO_OSDC_IO_OSD_GFCC        側偟

    OSD_SBCC1  _IO_OSDC_IO_OSD_SBCC1       側偟
    OSD_SBCC2  _IO_OSDC_IO_OSD_SBCC2       側偟

    OSD_SPCC1  _IO_OSDC_IO_OSD_SPCC1       側偟
    OSD_SPCC2  _IO_OSDC_IO_OSD_SPCC2       側偟
    OSD_SPCC3  _IO_OSDC_IO_OSD_SPCC3       側偟
    OSD_SPCC4  _IO_OSDC_IO_OSD_SPCC4       側偟

    OSD_SYNCC  _IO_OSDC_IO_OSD_SYNCC       側偟

    OSD_DCLKC1 _IO_OSDC_IO_OSD_DCLKC1      側偟
    OSD_DCLKC2 _IO_OSDC_IO_OSD_DCLKC2      側偟
    OSD_DCLKC3 _IO_OSDC_IO_OSD_DCLKC3      側偟

    OSD_IOC1   _IO_OSDC_IO_OSD_IOC1        側偟
    OSD_IOC2   _IO_OSDC_IO_OSD_IOC2        側偟

    OSD_DPC1   _IO_OSDC_IO_OSD_DPC1        側偟
    OSD_DPC2   _IO_OSDC_IO_OSD_DPC2        側偟
    OSD_DPC3   _IO_OSDC_IO_OSD_DPC3        側偟
    OSD_DPC4   _IO_OSDC_IO_OSD_DPC4        側偟

    OSD_JRC    _IO_OSDC_IO_OSD_JRC         側偟

    OSD_PLRn   _IO_OSDC_IO_OSD_PLRn        側偟
    (n:0 - 15)

    OSD_ACT1   _IO_OSDC_IO_OSD_ACT1        側偟
    OSD_ACT2   _IO_OSDC_IO_OSD_ACT2        側偟
    劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒






















劇劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劉
劆1. 杮帒椏偺婰嵹撪梕偼丆梊崘側偟偵曄峏偡傞偙偲偑偁傝傑偡偺偱丆偛梡柦偺嵺偼 劆
劆 摉幮塩嬈扴摉晹栧偵偛妋擣偔偩偝偄丅                                       劆
劆2. 杮彂偵婰嵹偝傟偨忣曬丒夞楬恾偼丆敿摫懱僨僶僀僗偺墳梡椺偲偟偰巊梡偝傟偰 劆
劆 偍傝丆幚嵺偵巊梡偡傞婡婍傊偺搵嵹傪栚揑偲偟偨傕偺偱偼偁傝傑偣傫丅傑偨丆偙 劆
劆 傟傜偺忣曬丒夞楬恾偺巊梡偵婲場偡傞丆戞嶰幰偺摿嫋尃丆偦偺懠偺尃棙怤奞偵偮 劆
劆 偄偰丆摉幮偼偦偺愑擟傪晧偄傑偣傫丅                                       劆
劆3. 杮帒椏偵婰嵹偝傟偨撪梕傪丆摉幮偵柍抐偱揮嵹傑偨偼暋惢偡傞偙偲偼偛墦椂偔 劆
劆 偩偝偄丅                                                                 劆
劆4. 摉幮敿摫懱僨僶僀僗偼丆昗弨梡搑乮僐儞僺儏乕僞乛俷俙側偳偺帠柋梡婡婍丆嶻 劆
劆 嬈乛捠怣乛寁應梡偺娭楢婡婍丆僷乕僜僫儖乛壠揹梡偺婡婍側偳乯偵巊梡偝傟傞偙 劆
劆 偲傪堄恾偟偰偄傑偡丅偦偺屘忈傗岆摦嶌偑捈愙恖柦傪嫼偐偟偨傝丆恖懱偵婋奞偑 劆
劆 媦傇嫲傟偺偁傞丆傑偨偼嬌傔偰崅偄怣棅惈偑梫媮偝傟傞摿暿梡搑乮峲嬻丒塅拡梡,劆
劆 尨巕椡惂屼梡丆奀掙拞宲婍丆憱峴惂屼梡丆惗柦堐帩偺偨傔偺堛椕梡側偳乯偵偛巊 劆
劆 梡傪偍峫偊偺偍媞條偼昁偢帠慜偵摉幮塩嬈扴摉晹栧傑偱偛憡択偔偩偝偄丅偛憡択 劆
劆 側偔巊梡偝傟偨偙偲偵傛傝敪惗偟偨懝奞側偳偵偮偄偰偼丆愑擟傪晧偄偐偹傑偡偺 劆
劆 偱偛椆彸偔偩偝偄丅                                                       劆
劆5. 敿摫懱僨僶僀僗偼偁傞妋棪偱屘忈偑敪惗偟傑偡丅摉幮敿摫懱僨僶僀僗偑屘忈偟 劆
劆 偰傕丆寢壥揑偵恖恎帠屘丆壩嵭帠屘丆幮夛揑側懝奞傪惗偠偝偣側偄傛偆丆偍媞條 劆
劆 偼丆憰抲偺忕挿愝寁丆墑從懳嶔愝寁丆夁揹棳杊巭懳嶔愝寁丆岆摦嶌杊巭愝寁側偳 劆
劆 偺埨慡愝寁傪偍婅偄偟傑偡丅                                               劆
劆6. 杮帒椏偵婰嵹偝傟偨惢昳偑丆乽奜崙堊懼偍傛傃奜崙杅堈娗棟朄乿偵婎偯偒婯惂 劆
劆 偝傟偰偄傞壿暔傑偨偼媄弍偵奩摉偡傞応崌偵偼丆杮惢昳傪桝弌偡傞偵嵺偟偰丆摨 劆
劆 朄偵婎偯偔嫋壜偑昁梫偲側傝傑偡丅                                         劆
劋劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劊
  (C)2002  FUJITSU LIMITED Printed in Japan
