Par Statistics
Total Non-vccgnd Signals=3876
Total Non-vccgnd Design Pins=13048
Total Non-vccgnd Conns=13048
Total Non-vccgnd Timing Constrained Conns=12173
Phase 1 CPU=12.9 sec
Phase 2 CPU=17.0 sec
Phase 3 CPU=27.3 sec
Phase 4 CPU=30.2 sec
Phase 5 CPU=37.4 sec
Phase 6 CPU=37.4 sec
Phase 7 CPU=37.4 sec
Phase 8 CPU=37.4 sec
Phase 9 CPU=37.4 sec
Phase 10 CPU=38.8 sec
AvgWirelenPerPin Fanout 1=2.0
AvgWirelenPerPin Fanout 2=2.0
AvgWirelenPerPin Fanout 3=2.3
AvgWirelenPerPin Fanout 4=7.5
AvgWirelenPerPin Fanout 10=2.1
AvgWirelenPerPin Fanout 50=2.4
AvgWirelenPerPin Fanout 100=12.9
AvgWirelenPerPin Fanout 500=7.9
AvgWirelenPerPin Fanout 5000=4.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
IRR Gamma=1.5185