Release 12.2 - xst M.63c (nt)
Copyright (c) 1995-2010 Xilinx, Inc.  All rights reserved.
--> Parameter TMPDIR set to xst/projnav.tmp


Total REAL time to Xst completion: 0.00 secs
Total CPU time to Xst completion: 0.11 secs
 
--> Parameter xsthdpdir set to xst


Total REAL time to Xst completion: 0.00 secs
Total CPU time to Xst completion: 0.11 secs
 
--> Reading design: exp6t_disp.prj

TABLE OF CONTENTS
  1) Synthesis Options Summary
  2) HDL Parsing
  3) HDL Elaboration
  4) HDL Synthesis
       4.1) HDL Synthesis Report
  5) Advanced HDL Synthesis
       5.1) Advanced HDL Synthesis Report
  6) Low Level Synthesis
  7) Partition Report
  8) Design Summary
       8.1) Primitive and Black Box Usage
       8.2) Device utilization summary
       8.3) Partition Resource Summary
       8.4) Timing Report
            8.4.1) Clock Information
            8.4.2) Asynchronous Control Signals Information
            8.4.3) Timing Summary
            8.4.4) Timing Details


=========================================================================
*                      Synthesis Options Summary                        *
=========================================================================
---- Source Parameters
Input File Name                    : "exp6t_disp.prj"
Input Format                       : mixed
Ignore Synthesis Constraint File   : NO

---- Target Parameters
Output File Name                   : "exp6t_disp"
Output Format                      : NGC
Target Device                      : xc6slx45t-3-fgg484

---- Source Options
Top Module Name                    : exp6t_disp
Automatic FSM Extraction           : YES
FSM Encoding Algorithm             : Auto
Safe Implementation                : No
FSM Style                          : LUT
RAM Extraction                     : Yes
RAM Style                          : Auto
ROM Extraction                     : Yes
Shift Register Extraction          : YES
ROM Style                          : Auto
Resource Sharing                   : YES
Asynchronous To Synchronous        : NO
Shift Register Minimum Size        : 2
Use DSP Block                      : Auto
Automatic Register Balancing       : Yes

---- Target Options
LUT Combining                      : Auto
Reduce Control Sets                : Auto
Add IO Buffers                     : YES
Global Maximum Fanout              : 500
Add Generic Clock Buffer(BUFG)     : 16
Register Duplication               : YES
Move First FlipFlop Stage          : YES
Move Last FlipFlop Stage           : YES
Optimize Instantiated Primitives   : NO
Use Clock Enable                   : Yes
Use Synchronous Set                : Yes
Use Synchronous Reset              : Yes
Pack IO Registers into IOBs        : Auto
Equivalent register Removal        : YES

---- General Options
Optimization Goal                  : Speed
Optimization Effort                : 2
Power Reduction                    : NO
Library Search Order               : "C:/PROJECT/EXP6T_PCIE3F/xise/exp6t_disp.lso"
Keep Hierarchy                     : Soft
Netlist Hierarchy                  : As_Optimized
RTL Output                         : Yes
Global Optimization                : AllClockNets
Read Cores                         : YES
Write Timing Constraints           : NO
Cross Clock Analysis               : NO
Hierarchy Separator                : /
Bus Delimiter                      : <>
Case Specifier                     : Maintain
Slice Utilization Ratio            : 100
BRAM Utilization Ratio             : 100
DSP48 Utilization Ratio            : 100
Auto BRAM Packing                  : NO
Slice Utilization Ratio Delta      : 5

---- Other Options
Cores Search Directories           : {".."  }

=========================================================================


=========================================================================
*                          HDL Parsing                                  *
=========================================================================
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/iodrp_mcb_controller.v\" into library work
Parsing module <iodrp_mcb_controller>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/iodrp_controller.v\" into library work
Parsing module <iodrp_controller>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/pcie_bram_s6.v\" into library work
Parsing module <pcie_bram_s6>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_PIO_32_TX_ENGINE.v\" into library work
Parsing module <xt_PIO_32_TX_ENGINE>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_PIO_32_RX_ENGINE.v\" into library work
Parsing module <xt_PIO_32_RX_ENGINE>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v\" into library work
Parsing module <mcb_soft_calibration>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/pcie_brams_s6.v\" into library work
Parsing module <pcie_brams_s6>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper_tile.v\" into library work
Parsing module <GTPA1_DUAL_WRAPPER_TILE>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_PIO_TO_CTRL.v\" into library work
Parsing module <xt_PIO_TO_CTRL>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_PIO_EP.v\" into library work
Parsing module <xt_PIO_EP>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../xil_blk_mem_gen_v4_2_dp108x256.v\" into library work
Parsing module <xil_blk_mem_gen_v4_2_dp108x256>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../xil_blk_mem_gen_v4_2_1024x32.v\" into library work
Parsing module <xil_blk_mem_gen_v4_2_1024x32>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration_top.v\" into library work
Parsing module <mcb_soft_calibration_top>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/pcie_bram_top_s6.v\" into library work
Parsing module <pcie_bram_top_s6>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper.v\" into library work
Parsing module <GTPA1_DUAL_WRAPPER>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_PIO.v\" into library work
Parsing module <xt_PIO>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_mem.v\" into library work
Parsing module <xt_mem>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp_tile.v\" into library work
Parsing module <XIL_S6_GTPWIZARD_V1_6_DP_TILE>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dvi_data_enc.v\" into library work
Parsing module <dvi_data_enc>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v\" into library work
Parsing module <dp_main_tbc1>.
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 55: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 56: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 57: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 59: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 60: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 61: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 62: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 63: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 64: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 65: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 66: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 67: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 68: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 69: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 70: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 71: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
WARNING:HDLCompiler:693 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 72: Parameter declaration becomes local in dp_main_tbc1 with formal parameter declaration list
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v\" into library work
Parsing module <dp_main_scramble>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v\" into library work
Parsing module <dp_main_linkup1>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_crtc1.v\" into library work
Parsing module <dp_main_crtc1>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_aux_tx.v\" into library work
Parsing module <dp_aux_tx>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_aux_rx.v\" into library work
Parsing module <dp_aux_rx>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_raw_wrapper.v\" into library work
Parsing module <mcb_raw_wrapper>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v\" into library work
Parsing module <eptest>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_pcie_app_s6.v\" into library work
Parsing module <xt_pcie_app_s6>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../xt_crtc2.v\" into library work
Parsing module <xt_crtc2>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../xt_crtc.v\" into library work
Parsing module <xt_crtc>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp.v\" into library work
Parsing module <XIL_S6_GTPWIZARD_V1_6_DP>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../xil_clk_wiz_v1_6_50x62x312.v\" into library work
Parsing module <xil_clk_wiz_v1_6_50x62x312>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../xil_clk_wiz_v1_6_50x200.v\" into library work
Parsing module <xil_clk_wiz_v1_6_50x200>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../xil_clk_wiz_v1_6_27x162.v\" into library work
Parsing module <xil_clk_wiz_v1_6_27x162>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../pciesample/sp6wrap.v\" into library work
Parsing module <sp6wrap>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../LYNX/xil_dvi.v\" into library work
Parsing module <xil_dvi>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v\" into library work
Parsing module <dp_main_640x480>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v\" into library work
Parsing module <memc3_wrapper>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_infrastructure.v\" into library work
Parsing module <memc3_infrastructure>.
Analyzing Verilog file \"\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v\" into library work
Parsing module <exp6t_disp>.

=========================================================================
*                            HDL Elaboration                            *
=========================================================================

Elaborating module <exp6t_disp>.

Elaborating module <IBUFG>.

Elaborating module <xil_clk_wiz_v1_6_50x200>.

Elaborating module <BUFG>.

Elaborating module <DCM_SP(CLKDV_DIVIDE=5.0,CLKFX_DIVIDE=1,CLKFX_MULTIPLY=4,CLKIN_DIVIDE_BY_2="FALSE",CLKIN_PERIOD=20.0,CLKOUT_PHASE_SHIFT="NONE",CLK_FEEDBACK="1X",DESKEW_ADJUST="SYSTEM_SYNCHRONOUS",PHASE_SHIFT=0,STARTUP_WAIT="FALSE")>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_clk_wiz_v1_6_50x200.v" Line 129: Assignment to status_int ignored, since the identifier is never used

Elaborating module <xil_clk_wiz_v1_6_50x62x312>.

Elaborating module <PLL_BASE(BANDWIDTH="OPTIMIZED",CLK_FEEDBACK="CLKFBOUT",COMPENSATION="SYSTEM_SYNCHRONOUS",DIVCLK_DIVIDE=2,CLKFBOUT_MULT=25,CLKFBOUT_PHASE=0.0,CLKOUT0_DIVIDE=10,CLKOUT0_PHASE=0.0,CLKOUT0_DUTY_CYCLE=0.5,CLKOUT1_DIVIDE=2,CLKOUT1_PHASE=0.0,CLKOUT1_DUTY_CYCLE=0.5,CLKIN_PERIOD=20.0,REF_JITTER=0.01)>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_clk_wiz_v1_6_50x62x312.v" Line 121: Assignment to clkout2_unused ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_clk_wiz_v1_6_50x62x312.v" Line 122: Assignment to clkout3_unused ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_clk_wiz_v1_6_50x62x312.v" Line 123: Assignment to clkout4_unused ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_clk_wiz_v1_6_50x62x312.v" Line 124: Assignment to clkout5_unused ignored, since the identifier is never used

Elaborating module <xil_clk_wiz_v1_6_27x162>.

Elaborating module <DCM_SP(CLKDV_DIVIDE=2.0,CLKFX_DIVIDE=1,CLKFX_MULTIPLY=6,CLKIN_DIVIDE_BY_2="FALSE",CLKIN_PERIOD=37.037,CLKOUT_PHASE_SHIFT="NONE",CLK_FEEDBACK="1X",DESKEW_ADJUST="SYSTEM_SYNCHRONOUS",PHASE_SHIFT=0,STARTUP_WAIT="FALSE")>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_clk_wiz_v1_6_27x162.v" Line 129: Assignment to status_int ignored, since the identifier is never used
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 421: Result of 9-bit expression is truncated to fit in 8-bit target.

Elaborating module <sp6wrap(FAST_TRAIN="FALSE")>.

Elaborating module <IBUFDS>.

Elaborating module <xt_pcie_app_s6>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_pcie_app_s6.v" Line 243: Assignment to bar0_buff_rd_data ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_pcie_app_s6.v" Line 248: Assignment to bar1_buff_rd_data ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_pcie_app_s6.v" Line 262: Assignment to bar2_buff_rd_data ignored, since the identifier is never used

Elaborating module <xil_blk_mem_gen_v4_2_1024x32>.
WARNING:HDLCompiler:1499 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_blk_mem_gen_v4_2_1024x32.v" Line 40: Empty module <xil_blk_mem_gen_v4_2_1024x32> remains a black box.

Elaborating module <xt_PIO>.

Elaborating module <xt_PIO_EP>.

Elaborating module <xt_PIO_32_RX_ENGINE>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_PIO_32_RX_ENGINE.v" Line 167: Assignment to mem64_bar_hit_n ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_PIO_32_RX_ENGINE.v" Line 168: Assignment to io_bar_hit_n ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_PIO_32_RX_ENGINE.v" Line 169: Assignment to mem32_bar_hit_n ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_PIO_32_RX_ENGINE.v" Line 170: Assignment to erom_bar_hit_n ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_PIO_32_RX_ENGINE.v" Line 342: Assignment to wr_w ignored, since the identifier is never used

Elaborating module <xt_PIO_32_TX_ENGINE>.

Elaborating module <xt_PIO_TO_CTRL>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_pcie_app_s6.v" Line 295: Assignment to user_rreq ignored, since the identifier is never used

Elaborating module <xt_mem>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/example_design/xt_mem.v" Line 176: Assignment to mem_wait_r ignored, since the identifier is never used

Elaborating module <eptest(FAST_TRAIN="FALSE")>.

Elaborating module <BUFIO2>.

Elaborating module <PLL_BASE(CLKFBOUT_MULT=5,CLKFBOUT_PHASE=0,CLKIN_PERIOD=10,CLKOUT0_DIVIDE=2,CLKOUT0_PHASE=0,CLKOUT1_DIVIDE=4,CLKOUT1_PHASE=0,CLKOUT2_DIVIDE=8,CLKOUT2_PHASE=0,COMPENSATION="INTERNAL")>.

Elaborating module <pcie_bram_top_s6(DEV_CAP_MAX_PAYLOAD_SUPPORTED=3'b0,VC0_TX_LASTPACKET=5'b01100,TLM_TX_OVERHEAD=20,TL_TX_RAM_RADDR_LATENCY=1'b0,TL_TX_RAM_RDATA_LATENCY=2'b10,TL_TX_RAM_WRITE_LATENCY=1'b0,VC0_RX_LIMIT=12'b0111111111,TL_RX_RAM_RADDR_LATENCY=1'b0,TL_RX_RAM_RDATA_LATENCY=2'b10,TL_RX_RAM_WRITE_LATENCY=1'b0)>.

Elaborating module <pcie_brams_s6(NUM_BRAMS=1,RAM_RADDR_LATENCY=1'b0,RAM_RDATA_LATENCY=2'b10,RAM_WRITE_LATENCY=1'b0)>.

Elaborating module <pcie_bram_s6(DOB_REG=1,WIDTH=7'b0100100)>.

Elaborating module <RAMB16BWER(DATA_WIDTH_A=7'b0100100,DATA_WIDTH_B=7'b0100100,DOA_REG=0,DOB_REG=1,WRITE_MODE_A="NO_CHANGE",WRITE_MODE_B="NO_CHANGE")>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 458: Assignment to mim_rx_rdata_unused ignored, since the identifier is never used

Elaborating module <GTPA1_DUAL_WRAPPER(WRAPPER_SIM_GTPRESET_SPEEDUP=1,WRAPPER_CLK25_DIVIDER_0=4,WRAPPER_CLK25_DIVIDER_1=4,WRAPPER_PLL_DIVSEL_FB_0=5,WRAPPER_PLL_DIVSEL_FB_1=5,WRAPPER_PLL_DIVSEL_REF_0=2,WRAPPER_PLL_DIVSEL_REF_1=2,WRAPPER_SIMULATION=0)>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper.v" Line 194: Assignment to tied_to_ground_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper.v" Line 195: Assignment to tied_to_ground_vec_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper.v" Line 196: Assignment to tied_to_vcc_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper.v" Line 197: Assignment to tied_to_vcc_vec_i ignored, since the identifier is never used

Elaborating module <GTPA1_DUAL_WRAPPER_TILE(TILE_SIM_GTPRESET_SPEEDUP=1,TILE_CLK25_DIVIDER_0=4,TILE_CLK25_DIVIDER_1=4,TILE_PLL_DIVSEL_FB_0=5,TILE_PLL_DIVSEL_FB_1=5,TILE_PLL_DIVSEL_REF_0=2,TILE_PLL_DIVSEL_REF_1=2,TILE_PLL_SOURCE_0="PLL0",TILE_PLL_SOURCE_1="PLL1")>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper_tile.v" Line 226: Assignment to tied_to_vcc_vec_i ignored, since the identifier is never used

Elaborating module
<GTPA1_DUAL(SIM_TX_ELEC_IDLE_LEVEL="Z",SIM_RECEIVER_DETECT_PASS="TRUE",SIM_VERSION="2.0",SIM_REFCLK0_SOURCE=3'b0,SIM_REFCLK1_SOURCE=3'b0,SIM_GTPRESET_SPEEDUP=1,CLK25_DIVIDER_0=4,CLK25_DIVIDER_1=4,PLL_DIVSEL_FB_0=5,PLL_DIVSEL_FB_1=5,PLL_DIVSEL_REF_0=2,PLL_DIVSEL_REF_1=2,CLKINDC_B_0="TRUE",CLKRCV_TRST_0="TRUE",OOB_CLK_DIVIDER_0=4,PLL_COM_CFG_0=24'b01000010110100000001010,PLL_CP_CFG_0=8'b0,PLL_RXDIVSEL_OUT_0=1,PLL_SATA_0="FALSE",PLL_SOURCE_0="PLL0",PLL_TXDIVSEL_OUT_0=1,PLLLKDET_CFG_0=3'b111,CLKINDC_B_1="TRUE",CLKRCV_TRST_1="TRUE",OOB_CLK_DIVIDER_1=4,PLL_COM_CFG_1=24'b01000010110100000001010,PLL_CP_CFG_1=8'b0,PLL_RXDIVSEL_OUT_1=1,PLL_SATA_1="FALSE",PLL_SOURCE_1="PLL1",PLL_TXDIVSEL_OUT_1=1,PLLLKDET_CFG_1=3'b111,PMA_COM_CFG_EAST=36'b01000000000000000,PMA_COM_CFG_WEST=36'b01000000000000000,TST_ATTR_0=32'b0,TST_ATTR_1=32'b0,CLK_OUT_GTP_SEL_0="REFCLKPLL0",TX_TDCC_CFG_0=2'b11,CLK_OUT_GTP_SEL_1="REFCLKPLL1",TX_TDCC_CFG_1=2'b11,PMA_TX_CFG_0=20'b010000010,TX_BUFFER_USE_0="TRUE",TX_XCLK_SEL_0="TXOUT",TXRX_INVERT_0=3'b011,P
MA_TX_CFG_1=20'b010000010,TX_BUFFER_USE_1="TRUE",TX_XCLK_SEL_1="TXOUT",TXRX_INVERT_1=3'b011,CM_TRIM_0=2'b0,TX_IDLE_DELAY_0=3'b010,CM_TRIM_1=2'b0,TX_IDLE_DELAY_1=3'b010,COM_BURST_VAL_0=4'b1111,COM_BURST_VAL_1=4'b1111,AC_CAP_DIS_0="FALSE",OOBDETECT_THRESHOLD_0=3'b111,PMA_CDR_SCAN_0=27'b110010000000100000001000000,PMA_RX_CFG_0=25'b010111001110000001001000,PMA_RXSYNC_CFG_0=7'b0,RCV_TERM_GND_0="TRUE",RCV_TERM_VTTRX_0="FALSE",RXEQ_CFG_0=8'b01111011,TERMINATION_CTRL_0=5'b10100,TERMINATION_OVRD_0="FALSE",TX_DETECT_RX_CFG_0=14'b01100000110010,AC_CAP_DIS_1="FALSE",OOBDETECT_THRESHOLD_1=3'b111,PMA_CDR_SCAN_1=27'b110010000000100000001000000,PMA_RX_CFG_1=25'b010111001110000001001000,PMA_RXSYNC_CFG_1=7'b0,RCV_TERM_GND_1="TRUE",RCV_TERM_VTTRX_1="FALSE",RXEQ_CFG_1=8'b01111011,TERMINATION_CTRL_1=5'b10100,TERMINATION_OVRD_1="FALSE",TX_DETECT_RX_CFG_1=14'b01100000110010,RXPRBSERR_LOOPBACK_0=1'b0,RXPRBSERR_LOOPBACK_1=1'b0,ALIGN_COMMA_WORD_0=1,COMMA_10B_ENABLE_0=10'b1111111111,DEC_MCOMMA_DETECT_0="TRUE",DEC_PCOMMA_DETECT_0="TRUE"
,DEC_VALID_COMMA_ONLY_0="TRUE",MCOMMA_10B_VALUE_0=10'b1010000011,MCOMMA_DETECT_0="TRUE",PCOMMA_10B_VALUE_0=10'b0101111100,PCOMMA_DETECT_0="TRUE",RX_SLIDE_MODE_0="PCS",ALIGN_COMMA_WORD_1=1,COMMA_10B_ENABLE_1=10'b1111111111,DEC_MCOMMA_DETECT_1="TRUE",DEC_PCOMMA_DETECT_1="TRUE",DEC_VALID_COMMA_ONLY_1="TRUE",MCOMMA_10B_VALUE_1=10'b1010000011,MCOMMA_DETECT_1="TRUE",PCOMMA_10B_VALUE_1=10'b0101111100,PCOMMA_DETECT_1="TRUE",RX_SLIDE_MODE_1="PCS",RX_LOS_INVALID_INCR_0=8,RX_LOS_THRESHOLD_0=128,RX_LOSS_OF_SYNC_FSM_0="FALSE",RX_LOS_INVALID_INCR_1=8,RX_LOS_THRESHOLD_1=128,RX_LOSS_OF_SYNC_FSM_1="FALSE",RX_BUFFER_USE_0="TRUE",RX_EN_IDLE_RESET_BUF_0="TRUE",RX_IDLE_HI_CNT_0=4'b1000,RX_IDLE_LO_CNT_0=4'b0,RX_XCLK_SEL_0="RXREC",RX_BUFFER_USE_1="TRUE",RX_EN_IDLE_RESET_BUF_1="TRUE",RX_IDLE_HI_CNT_1=4'b1000,RX_IDLE_LO_CNT_1=4'b0,RX_XCLK_SEL_1="RXREC",CLK_COR_ADJ_LEN_0=1,CLK_COR_DET_LEN_0=1,CLK_COR_INSERT_IDLE_FLAG_0="FALSE",CLK_COR_KEEP_IDLE_0="FALSE",CLK_COR_MAX_LAT_0=20,CLK_COR_MIN_LAT_0=18,CLK_COR_PRECEDENCE_0="TRUE",CLK_COR_REP
EAT_WAIT_0=0,CLK_COR_SEQ_1_1_0=10'b0100011100,CLK_COR_SEQ_1_2_0=10'b0,CLK_COR_SEQ_1_3_0=10'b0,CLK_COR_SEQ_1_4_0=10'b0,CLK_COR_SEQ_1_ENABLE_0=4'b01,CLK_COR_SEQ_2_1_0=10'b0,CLK_COR_SEQ_2_2_0=10'b0,CLK_COR_SEQ_2_3_0=10'b0,CLK_COR_SEQ_2_4_0=10'b0,CLK_COR_SEQ_2_ENABLE_0=4'b0,CLK_COR_SEQ_2_USE_0="FALSE",CLK_CORRECT_USE_0="TRUE",RX_DECODE_SEQ_MATCH_0="TRUE",CLK_COR_ADJ_LEN_1=1,CLK_COR_DET_LEN_1=1,CLK_COR_INSERT_IDLE_FLAG_1="FALSE",CLK_COR_KEEP_IDLE_1="FALSE",CLK_COR_MAX_LAT_1=20,CLK_COR_MIN_LAT_1=18,CLK_COR_PRECEDENCE_1="TRUE",CLK_COR_REPEAT_WAIT_1=0,CLK_COR_SEQ_1_1_1=10'b0100011100,CLK_COR_SEQ_1_2_1=10'b0,CLK_COR_SEQ_1_3_1=10'b0,CLK_COR_SEQ_1_4_1=10'b0,CLK_COR_SEQ_1_ENABLE_1=4'b01,CLK_COR_SEQ_2_1_1=10'b0,CLK_COR_SEQ_2_2_1=10'b0,CLK_COR_SEQ_2_3_1=10'b0,CLK_COR_SEQ_2_4_1=10'b0,CLK_COR_SEQ_2_ENABLE_1=4'b0,CLK_COR_SEQ_2_USE_1="FALSE",CLK_CORRECT_USE_1="TRUE",RX_DECODE_SEQ_MATCH_1="TRUE",CHAN_BOND_1_MAX_SKEW_0=1,CHAN_BOND_2_MAX_SKEW_0=1,CHAN_BOND_KEEP_ALIGN_0="FALSE",CHAN_BOND_SEQ_1_1_0=10'b01001010,CHAN_BOND_SEQ_1_2_0=
10'b01001010,CHAN_BOND_SEQ_1_3_0=10'b01001010,CHAN_BOND_SEQ_1_4_0=10'b0110111100,CHAN_BOND_SEQ_1_ENABLE_0=4'b0,CHAN_BOND_SEQ_2_1_0=10'b0100111100,CHAN_BOND_SEQ_2_2_0=10'b0100111100,CHAN_BOND_SEQ_2_3_0=10'b0110111100,CHAN_BOND_SEQ_2_4_0=10'b0100011100,CHAN_BOND_SEQ_2_ENABLE_0=4'b0,CHAN_BOND_SEQ_2_USE_0="FALSE",CHAN_BOND_SEQ_LEN_0=1,RX_EN_MODE_RESET_BUF_0="TRUE",CHAN_BOND_1_MAX_SKEW_1=1,CHAN_BOND_2_MAX_SKEW_1=1,CHAN_BOND_KEEP_ALIGN_1="FALSE",CHAN_BOND_SEQ_1_1_1=10'b01001010,CHAN_BOND_SEQ_1_2_1=10'b01001010,CHAN_BOND_SEQ_1_3_1=10'b01001010,CHAN_BOND_SEQ_1_4_1=10'b0110111100,CHAN_BOND_SEQ_1_ENABLE_1=4'b0,CHAN_BOND_SEQ_2_1_1=10'b0100111100,CHAN_BOND_SEQ_2_2_1=10'b0100111100,CHAN_BOND_SEQ_2_3_1=10'b0110111100,CHAN_BOND_SEQ_2_4_1=10'b0100011100,CHAN_BOND_SEQ_2_ENABLE_1=4'b0,CHAN_BOND_SEQ_2_USE_1="FALSE",CHAN_BOND_SEQ_LEN_1=1,RX_EN_MODE_RESET_BUF_1="TRUE",CB2_INH_CC_PERIOD_0=8,CDR_PH_ADJ_TIME_0=5'b01010,PCI_EXPRESS_MODE_0="TRUE",RX_EN_IDLE_HOLD_CDR_0="TRUE",RX_EN_IDLE_RESET_FR_0="TRUE",RX_EN_IDLE_RESET_PH_0="TRUE",RX
_STATUS_FMT_0="PCIE",TRANS_TIME_FROM_P2_0=12'b0111100,TRANS_TIME_NON_P2_0=8'b011001,TRANS_TIME_TO_P2_0=10'b01100100,CB2_INH_CC_PERIOD_1=8,CDR_PH_ADJ_TIME_1=5'b01010,PCI_EXPRESS_MODE_1="TRUE",RX_EN_IDLE_HOLD_CDR_1="TRUE",RX_EN_IDLE_RESET_FR_1="TRUE",RX_EN_IDLE_RESET_PH_1="TRUE",RX_STATUS_FMT_1="PCIE",TRANS_TIME_FROM_P2_1=12'b0111100,TRANS_TIME_NON_P2_1=8'b011001,TRANS_TIME_TO_P2_1=10'b01100100,SATA_BURST_VAL_0=3'b100,SATA_IDLE_VAL_0=3'b100,SATA_MAX_BURST_0=7,SATA_MAX_INIT_0=22,SATA_MAX_WAKE_0=7,SATA_MIN_BURST_0=4,SATA_MIN_INIT_0=12,SATA_MIN_WAKE_0=4,SATA_BURST_VAL_1=3'b100,SATA_IDLE_VAL_1=3'b100,SATA_MAX_BURST_1=7,SATA_MAX_INIT_1=22,SATA_MAX_WAKE_1=7,SATA_MIN_BURST_1=4,SATA_MIN_INIT_1=12,SATA_MIN_WAKE_1=4>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper_tile.v" Line 573: Assignment to rxcharisk0_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper_tile.v" Line 574: Assignment to rxcharisk1_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper_tile.v" Line 577: Assignment to rxdisperr0_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper_tile.v" Line 578: Assignment to rxdisperr1_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper_tile.v" Line 579: Assignment to rxnotintable0_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/gtpa1_dual_wrapper_tile.v" Line 580: Assignment to rxnotintable1_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 540: Assignment to gt_rx_valid ignored, since the identifier is never used

Elaborating module
<PCIE_A1(BAR0=32'b11111111111111110000000000000000,BAR1=32'b11111110000000000000000000000000,BAR2=32'b0,BAR3=32'b0,BAR4=32'b0,BAR5=32'b0,CARDBUS_CIS_POINTER=32'b0,CLASS_CODE=24'b01000000000000000000,DEV_CAP_ENDPOINT_L0S_LATENCY=3'b111,DEV_CAP_ENDPOINT_L1_LATENCY=3'b111,DEV_CAP_EXT_TAG_SUPPORTED="FALSE",DEV_CAP_MAX_PAYLOAD_SUPPORTED=3'b0,DEV_CAP_PHANTOM_FUNCTIONS_SUPPORT=2'b0,DEV_CAP_ROLE_BASED_ERROR="TRUE",DISABLE_BAR_FILTERING="FALSE",DISABLE_ID_CHECK="FALSE",DISABLE_SCRAMBLING="FALSE",ENABLE_RX_TD_ECRC_TRIM="FALSE",EXPANSION_ROM=22'b0,FAST_TRAIN="FALSE",GTP_SEL=1'b1,LINK_CAP_ASPM_SUPPORT=2'b01,LINK_CAP_L0S_EXIT_LATENCY=3'b111,LINK_CAP_L1_EXIT_LATENCY=3'b111,LINK_STATUS_SLOT_CLOCK_CONFIG="FALSE",LL_ACK_TIMEOUT=15'b0,LL_ACK_TIMEOUT_EN="FALSE",LL_REPLAY_TIMEOUT=15'b0,LL_REPLAY_TIMEOUT_EN="FALSE",MSI_CAP_MULTIMSG_EXTENSION=1'b0,MSI_CAP_MULTIMSGCAP=3'b0,PCIE_CAP_CAPABILITY_VERSION=4'b01,PCIE_CAP_DEVICE_PORT_TYPE=4'b01,PCIE_CAP_INT_MSG_NUM=5'b0,PCIE_CAP_SLOT_IMPLEMENTED="FALSE",PCIE_GENERIC=12'b011101111,PLM_AUTO
_CONFIG="FALSE",PM_CAP_AUXCURRENT=3'b0,PM_CAP_DSI="FALSE",PM_CAP_D1SUPPORT="TRUE",PM_CAP_D2SUPPORT="TRUE",PM_CAP_PME_CLOCK="FALSE",PM_CAP_PMESUPPORT=5'b01111,PM_CAP_VERSION=3'b011,PM_DATA_SCALE0=2'b0,PM_DATA_SCALE1=2'b0,PM_DATA_SCALE2=2'b0,PM_DATA_SCALE3=2'b0,PM_DATA_SCALE4=2'b0,PM_DATA_SCALE5=2'b0,PM_DATA_SCALE6=2'b0,PM_DATA_SCALE7=2'b0,PM_DATA0=8'b0,PM_DATA1=8'b0,PM_DATA2=8'b0,PM_DATA3=8'b0,PM_DATA4=8'b0,PM_DATA5=8'b0,PM_DATA6=8'b0,PM_DATA7=8'b0,SLOT_CAP_ATT_BUTTON_PRESENT="FALSE",SLOT_CAP_ATT_INDICATOR_PRESENT="FALSE",SLOT_CAP_POWER_INDICATOR_PRESENT="FALSE",TL_RX_RAM_RADDR_LATENCY=1'b0,TL_RX_RAM_RDATA_LATENCY=2'b10,TL_RX_RAM_WRITE_LATENCY=1'b0,TL_TFC_DISABLE="FALSE",TL_TX_CHECKS_DISABLE="FALSE",TL_TX_RAM_RADDR_LATENCY=1'b0,TL_TX_RAM_RDATA_LATENCY=2'b10,USR_CFG="FALSE",USR_EXT_CFG="FALSE",VC0_CPL_INFINITE="TRUE",VC0_RX_RAM_LIMIT=12'b0111111111,VC0_TOTAL_CREDITS_CD=11'b0101001,VC0_TOTAL_CREDITS_CH=7'b010000,VC0_TOTAL_CREDITS_NPH=7'b01000,VC0_TOTAL_CREDITS_PD=11'b0101001,VC0_TOTAL_CREDITS_PH=7'b010000,VC0_TX
_LASTPACKET=5'b01100)>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 773: Assignment to cfg_ltssm_state ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 786: Assignment to dbg_bad_dllp_status ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 787: Assignment to dbg_bad_tlp_lcrc ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 788: Assignment to dbg_bad_tlp_seq_num ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 789: Assignment to dbg_bad_tlp_status ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 790: Assignment to dbg_dl_protocol_status ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 791: Assignment to dbg_fc_protocol_err_status ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 792: Assignment to dbg_mlfrmd_length ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 793: Assignment to dbg_mlfrmd_mps ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 794: Assignment to dbg_mlfrmd_tcvc ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 795: Assignment to dbg_mlfrmd_tlp_status ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 796: Assignment to dbg_mlfrmd_unrec_type ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 797: Assignment to dbg_poistlpstatus ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 798: Assignment to dbg_rcvr_overflow_status ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 799: Assignment to dbg_reg_detected_correctable ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 800: Assignment to dbg_reg_detected_fatal ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 801: Assignment to dbg_reg_detected_non_fatal ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 802: Assignment to dbg_reg_detected_unsupported ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 803: Assignment to dbg_rply_rollover_status ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 804: Assignment to dbg_rply_timeout_status ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 805: Assignment to dbg_ur_no_bar_hit ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 806: Assignment to dbg_ur_pois_cfg_wr ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 807: Assignment to dbg_ur_status ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 808: Assignment to dbg_ur_unsup_msg ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 844: Assignment to pipe_tx_char_disp_val_a ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/eptest/source/eptest.v" Line 845: Assignment to pipe_tx_char_disp_val_b ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../pciesample/sp6wrap.v" Line 445: Assignment to received_hot_reset ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 480: Assignment to user_addr ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 481: Assignment to user_length ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 485: Assignment to user_dreq ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 488: Assignment to bar0_rdreq ignored, since the identifier is never used

Elaborating module <xil_dvi(DVI_TX0=0,DVI_TX1=0,DVI_TX2=0,DVI_TXC=0)>.

Elaborating module <dvi_data_enc>.

Elaborating module <FDDRRSE>.

Elaborating module <OBUFDS>.

Elaborating module <xt_crtc(init_mode=32'b0,init_addr=32'b0,init_hdisp=32'b01111111111,init_hsync=32'b010000100111,init_hbp=32'b010010010111,init_htotal=32'b010100101111,init_vdisp=32'b01011111111,init_vsync=32'b01100000010,init_vbp=32'b01100000110,init_vtotal=32'b01100011101)>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xt_crtc.v" Line 190: Assignment to io_rdata_r ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xt_crtc.v" Line 252: Assignment to vram_ofst ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xt_crtc.v" Line 385: Assignment to crtc_rd_req_r ignored, since the identifier is never used
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../xt_crtc.v" Line 768: Result of 32-bit expression is truncated to fit in 20-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../xt_crtc.v" Line 779: Result of 32-bit expression is truncated to fit in 12-bit target.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 668: Assignment to crtc1_io_rdata ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 672: Assignment to crtc1_io_ack ignored, since the identifier is never used

Elaborating module <xt_crtc2(init_mode=32'b0,init_addr=32'b010000000000000000000000,init_hdisp=32'b01001111111,init_hsync=32'b01010001111,init_hbp=32'b01011101111,init_htotal=32'b01100011111,init_vdisp=32'b0111011111,init_vsync=32'b0111101001,init_vbp=32'b0111101011,init_vtotal=32'b01000001100)>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xt_crtc2.v" Line 192: Assignment to io_rdata_r ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xt_crtc2.v" Line 254: Assignment to vram_ofst ignored, since the identifier is never used
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../xt_crtc2.v" Line 770: Result of 32-bit expression is truncated to fit in 20-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../xt_crtc2.v" Line 781: Result of 32-bit expression is truncated to fit in 12-bit target.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 738: Assignment to crtc2_io_rdata ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 742: Assignment to crtc2_io_ack ignored, since the identifier is never used

Elaborating module <OBUFTDS>.
WARNING:HDLCompiler:1016 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 173: Port link_timeout is not connected to this instance

Elaborating module <dp_main_640x480(dp_mvid=24'b01010101010100,dp_nvid=24'b01000000000000000,dp_maud=8'b0,dp_htotal=16'b01100100000,dp_vtotal=16'b01000001101,dp_hstart=16'b010010000,dp_vstart=16'b0100011,dp_hwidth=16'b01010000000,dp_vheight=16'b0111100000,dp_hsync=16'b01100000,dp_vsync=16'b010,dp_misc0=8'b0100000,dp_misc1=8'b0,dp_link=1)>.

Elaborating module <dp_main_linkup1>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 135: Assignment to link_aux_cmd_init_wr_req ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 136: Assignment to link_aux_cmd_idle_wr_req ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 137: Assignment to link_aux_cmd_tr1_wr_req ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 138: Assignment to link_aux_stat_tr1_rd_req ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 139: Assignment to link_aux_cmd_tr2_wr_req ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 140: Assignment to link_aux_stat_tr2_rd_req ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 433: Assignment to aux_rx_cmd ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 434: Assignment to aux_rx_data ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 435: Assignment to aux_rx_cmd_ack ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 436: Assignment to aux_rx_data_ack ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 586: Assignment to aux_ack_r ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 819: Assignment to aux_stat_rd ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_linkup1.v" Line 827: Assignment to aux_rd_count_w ignored, since the identifier is never used

Elaborating module <dp_aux_tx>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_aux_tx.v" Line 122: Assignment to aux_data_r ignored, since the identifier is never used
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_aux_tx.v" Line 203: Result of 21-bit expression is truncated to fit in 20-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_aux_tx.v" Line 496: Result of 4-bit expression is truncated to fit in 1-bit target.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 302: Assignment to link_aux_tx_data_req ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 303: Assignment to link_aux_tx_select ignored, since the identifier is never used

Elaborating module <dp_aux_rx>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_aux_rx.v" Line 100: Assignment to aux_rx_one ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_aux_rx.v" Line 186: Assignment to aux_clk_sync_req ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 315: Assignment to link_aux_rx_sync ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 316: Assignment to link_aux_rx_stop ignored, since the identifier is never used

Elaborating module <dp_main_crtc1>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_crtc1.v" Line 190: Assignment to disp_hcount_sbp ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_crtc1.v" Line 194: Assignment to disp_vcount_sbp ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_crtc1.v" Line 195: Assignment to disp_vcount_sav ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_crtc1.v" Line 203: Assignment to disp_reg_hsize_r ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_crtc1.v" Line 608: Assignment to tbc_dcount_sync_r ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_crtc1.v" Line 657: Assignment to tbc_de1 ignored, since the identifier is never used

Elaborating module <dp_main_tbc1>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 125: Assignment to disp_dclk_sync ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 229: Assignment to tx_req_in_r ignored, since the identifier is never used

Elaborating module <xil_blk_mem_gen_v4_2_dp108x256>.
WARNING:HDLCompiler:1499 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_blk_mem_gen_v4_2_dp108x256.v" Line 40: Empty module <xil_blk_mem_gen_v4_2_dp108x256> remains a black box.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_tbc1.v" Line 536: Result of 10-bit expression is truncated to fit in 9-bit target.

Elaborating module <dp_main_scramble>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 223: Assignment to pack_data1_in_bs_r ignored, since the identifier is never used
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 330: Result of 22-bit expression is truncated to fit in 11-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 339: Result of 22-bit expression is truncated to fit in 11-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 346: Result of 22-bit expression is truncated to fit in 11-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 353: Result of 22-bit expression is truncated to fit in 11-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 386: Result of 22-bit expression is truncated to fit in 11-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 423: Result of 18-bit expression is truncated to fit in 11-bit target.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 453: Assignment to sc_op_sr ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 454: Assignment to sc_op_ss ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 455: Assignment to sc_op_fs ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 456: Assignment to sc_op_fe ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 725: Assignment to tr0_disp_out ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 726: Assignment to tr0_kerr ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 728: Assignment to tr1_disp_out ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 729: Assignment to tr1_kerr ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 731: Assignment to tr2_disp_out ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 732: Assignment to tr2_kerr ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 734: Assignment to tr3_disp_out ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_scramble.v" Line 735: Assignment to tr3_kerr ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 578: Assignment to sc_enc0_8b10b ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 579: Assignment to sc_enc1_8b10b ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 580: Assignment to sc_enc2_8b10b ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 581: Assignment to sc_enc3_8b10b ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 592: Assignment to sc_raw0 ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 593: Assignment to sc_raw1 ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 594: Assignment to sc_raw2 ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../LYNX/dp_main_640x480.v" Line 595: Assignment to sc_raw3 ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 899: Assignment to REF_HS ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 900: Assignment to REF_VS ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 901: Assignment to REF_DE ignored, since the identifier is never used

Elaborating module <BUFIO2(DIVIDE=1,DIVIDE_BYPASS="TRUE")>.

Elaborating module <XIL_S6_GTPWIZARD_V1_6_DP(WRAPPER_SIM_GTPRESET_SPEEDUP=0,WRAPPER_SIMULATION=0)>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp.v" Line 210: Assignment to tied_to_ground_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp.v" Line 211: Assignment to tied_to_ground_vec_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp.v" Line 212: Assignment to tied_to_vcc_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp.v" Line 213: Assignment to tied_to_vcc_vec_i ignored, since the identifier is never used

Elaborating module <XIL_S6_GTPWIZARD_V1_6_DP_TILE(TILE_SIM_GTPRESET_SPEEDUP=0,TILE_CLK25_DIVIDER_0=6,TILE_CLK25_DIVIDER_1=6,TILE_PLL_DIVSEL_FB_0=2,TILE_PLL_DIVSEL_FB_1=2,TILE_PLL_DIVSEL_REF_0=1,TILE_PLL_DIVSEL_REF_1=1,TILE_PLL_SOURCE_0="PLL0",TILE_PLL_SOURCE_1="PLL1")>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp_tile.v" Line 240: Assignment to tied_to_vcc_vec_i ignored, since the identifier is never used

Elaborating module
<GTPA1_DUAL(SIM_TX_ELEC_IDLE_LEVEL="Z",SIM_RECEIVER_DETECT_PASS="TRUE",SIM_VERSION="2.0",SIM_REFCLK0_SOURCE=3'b0,SIM_REFCLK1_SOURCE=3'b0,SIM_GTPRESET_SPEEDUP=0,CLK25_DIVIDER_0=6,CLK25_DIVIDER_1=6,PLL_DIVSEL_FB_0=2,PLL_DIVSEL_FB_1=2,PLL_DIVSEL_REF_0=1,PLL_DIVSEL_REF_1=1,CLKINDC_B_0="TRUE",CLKRCV_TRST_0="TRUE",OOB_CLK_DIVIDER_0=6,PLL_COM_CFG_0=24'b01000010110100000001010,PLL_CP_CFG_0=8'b0,PLL_RXDIVSEL_OUT_0=1,PLL_SATA_0="FALSE",PLL_SOURCE_0="PLL0",PLL_TXDIVSEL_OUT_0=1,PLLLKDET_CFG_0=3'b111,CLKINDC_B_1="TRUE",CLKRCV_TRST_1="TRUE",OOB_CLK_DIVIDER_1=4,PLL_COM_CFG_1=24'b01000010110100000001010,PLL_CP_CFG_1=8'b0,PLL_RXDIVSEL_OUT_1=1,PLL_SATA_1="FALSE",PLL_SOURCE_1="PLL1",PLL_TXDIVSEL_OUT_1=2,PLLLKDET_CFG_1=3'b111,PMA_COM_CFG_EAST=36'b01000000000000000,PMA_COM_CFG_WEST=36'b01010000000000000,TST_ATTR_0=32'b0,TST_ATTR_1=32'b0,CLK_OUT_GTP_SEL_0="TXOUTCLK0",TX_TDCC_CFG_0=2'b11,CLK_OUT_GTP_SEL_1="TXOUTCLK1",TX_TDCC_CFG_1=2'b11,PMA_TX_CFG_0=20'b010000010,TX_BUFFER_USE_0="TRUE",TX_XCLK_SEL_0="TXOUT",TXRX_INVERT_0=3'b011,PMA
_TX_CFG_1=20'b010000010,TX_BUFFER_USE_1="TRUE",TX_XCLK_SEL_1="TXOUT",TXRX_INVERT_1=3'b111,CM_TRIM_0=2'b0,TX_IDLE_DELAY_0=3'b011,CM_TRIM_1=2'b0,TX_IDLE_DELAY_1=3'b011,COM_BURST_VAL_0=4'b1111,COM_BURST_VAL_1=4'b1111,AC_CAP_DIS_0="FALSE",OOBDETECT_THRESHOLD_0=3'b110,PMA_CDR_SCAN_0=27'b110010000000100000001000000,PMA_RX_CFG_0=25'b010111001110000010001001,PMA_RXSYNC_CFG_0=7'b0,RCV_TERM_GND_0="FALSE",RCV_TERM_VTTRX_0="TRUE",RXEQ_CFG_0=8'b01111011,TERMINATION_CTRL_0=5'b10100,TERMINATION_OVRD_0="FALSE",TX_DETECT_RX_CFG_0=14'b01100000110010,AC_CAP_DIS_1="TRUE",OOBDETECT_THRESHOLD_1=3'b110,PMA_CDR_SCAN_1=27'b110010000000100000001000000,PMA_RX_CFG_1=25'b010111001110000000000100,PMA_RXSYNC_CFG_1=7'b0,RCV_TERM_GND_1="FALSE",RCV_TERM_VTTRX_1="TRUE",RXEQ_CFG_1=8'b01111011,TERMINATION_CTRL_1=5'b10100,TERMINATION_OVRD_1="FALSE",TX_DETECT_RX_CFG_1=14'b01100000110010,RXPRBSERR_LOOPBACK_0=1'b0,RXPRBSERR_LOOPBACK_1=1'b0,ALIGN_COMMA_WORD_0=2,COMMA_10B_ENABLE_0=10'b1111111111,DEC_MCOMMA_DETECT_0="TRUE",DEC_PCOMMA_DETECT_0="TRUE",DE
C_VALID_COMMA_ONLY_0="FALSE",MCOMMA_10B_VALUE_0=10'b1010000011,MCOMMA_DETECT_0="TRUE",PCOMMA_10B_VALUE_0=10'b0101111100,PCOMMA_DETECT_0="TRUE",RX_SLIDE_MODE_0="PCS",ALIGN_COMMA_WORD_1=1,COMMA_10B_ENABLE_1=10'b1111111111,DEC_MCOMMA_DETECT_1="FALSE",DEC_PCOMMA_DETECT_1="FALSE",DEC_VALID_COMMA_ONLY_1="TRUE",MCOMMA_10B_VALUE_1=10'b1010000011,MCOMMA_DETECT_1="TRUE",PCOMMA_10B_VALUE_1=10'b0101111100,PCOMMA_DETECT_1="TRUE",RX_SLIDE_MODE_1="PCS",RX_LOS_INVALID_INCR_0=8,RX_LOS_THRESHOLD_0=128,RX_LOSS_OF_SYNC_FSM_0="FALSE",RX_LOS_INVALID_INCR_1=8,RX_LOS_THRESHOLD_1=128,RX_LOSS_OF_SYNC_FSM_1="TRUE",RX_BUFFER_USE_0="TRUE",RX_EN_IDLE_RESET_BUF_0="TRUE",RX_IDLE_HI_CNT_0=4'b1000,RX_IDLE_LO_CNT_0=4'b0,RX_XCLK_SEL_0="RXREC",RX_BUFFER_USE_1="TRUE",RX_EN_IDLE_RESET_BUF_1="TRUE",RX_IDLE_HI_CNT_1=4'b1000,RX_IDLE_LO_CNT_1=4'b0,RX_XCLK_SEL_1="RXREC",CLK_COR_ADJ_LEN_0=4,CLK_COR_DET_LEN_0=4,CLK_COR_INSERT_IDLE_FLAG_0="FALSE",CLK_COR_KEEP_IDLE_0="FALSE",CLK_COR_MAX_LAT_0=18,CLK_COR_MIN_LAT_0=16,CLK_COR_PRECEDENCE_0="TRUE",CLK_COR_REPE
AT_WAIT_0=0,CLK_COR_SEQ_1_1_0=10'b0110111100,CLK_COR_SEQ_1_2_0=10'b01001010,CLK_COR_SEQ_1_3_0=10'b01001010,CLK_COR_SEQ_1_4_0=10'b01111011,CLK_COR_SEQ_1_ENABLE_0=4'b1111,CLK_COR_SEQ_2_1_0=10'b0100000000,CLK_COR_SEQ_2_2_0=10'b0,CLK_COR_SEQ_2_3_0=10'b0,CLK_COR_SEQ_2_4_0=10'b0,CLK_COR_SEQ_2_ENABLE_0=4'b0,CLK_COR_SEQ_2_USE_0="FALSE",CLK_CORRECT_USE_0="TRUE",RX_DECODE_SEQ_MATCH_0="TRUE",CLK_COR_ADJ_LEN_1=1,CLK_COR_DET_LEN_1=1,CLK_COR_INSERT_IDLE_FLAG_1="FALSE",CLK_COR_KEEP_IDLE_1="FALSE",CLK_COR_MAX_LAT_1=18,CLK_COR_MIN_LAT_1=16,CLK_COR_PRECEDENCE_1="TRUE",CLK_COR_REPEAT_WAIT_1=5,CLK_COR_SEQ_1_1_1=10'b0100000000,CLK_COR_SEQ_1_2_1=10'b0100000000,CLK_COR_SEQ_1_3_1=10'b0100000000,CLK_COR_SEQ_1_4_1=10'b0100000000,CLK_COR_SEQ_1_ENABLE_1=4'b0,CLK_COR_SEQ_2_1_1=10'b0100000000,CLK_COR_SEQ_2_2_1=10'b0100000000,CLK_COR_SEQ_2_3_1=10'b0100000000,CLK_COR_SEQ_2_4_1=10'b0100000000,CLK_COR_SEQ_2_ENABLE_1=4'b0,CLK_COR_SEQ_2_USE_1="FALSE",CLK_CORRECT_USE_1="FALSE",RX_DECODE_SEQ_MATCH_1="TRUE",CHAN_BOND_1_MAX_SKEW_0=1,CHAN_BOND_2_MAX
_SKEW_0=1,CHAN_BOND_KEEP_ALIGN_0="FALSE",CHAN_BOND_SEQ_1_1_0=10'b0,CHAN_BOND_SEQ_1_2_0=10'b0,CHAN_BOND_SEQ_1_3_0=10'b0,CHAN_BOND_SEQ_1_4_0=10'b0,CHAN_BOND_SEQ_1_ENABLE_0=4'b0,CHAN_BOND_SEQ_2_1_0=10'b0,CHAN_BOND_SEQ_2_2_0=10'b0,CHAN_BOND_SEQ_2_3_0=10'b0,CHAN_BOND_SEQ_2_4_0=10'b0,CHAN_BOND_SEQ_2_ENABLE_0=4'b0,CHAN_BOND_SEQ_2_USE_0="FALSE",CHAN_BOND_SEQ_LEN_0=1,RX_EN_MODE_RESET_BUF_0="TRUE",CHAN_BOND_1_MAX_SKEW_1=1,CHAN_BOND_2_MAX_SKEW_1=1,CHAN_BOND_KEEP_ALIGN_1="FALSE",CHAN_BOND_SEQ_1_1_1=10'b0,CHAN_BOND_SEQ_1_2_1=10'b0,CHAN_BOND_SEQ_1_3_1=10'b0,CHAN_BOND_SEQ_1_4_1=10'b0,CHAN_BOND_SEQ_1_ENABLE_1=4'b0,CHAN_BOND_SEQ_2_1_1=10'b0,CHAN_BOND_SEQ_2_2_1=10'b0,CHAN_BOND_SEQ_2_3_1=10'b0,CHAN_BOND_SEQ_2_4_1=10'b0,CHAN_BOND_SEQ_2_ENABLE_1=4'b0,CHAN_BOND_SEQ_2_USE_1="FALSE",CHAN_BOND_SEQ_LEN_1=1,RX_EN_MODE_RESET_BUF_1="FALSE",CB2_INH_CC_PERIOD_0=8,CDR_PH_ADJ_TIME_0=5'b01010,PCI_EXPRESS_MODE_0="FALSE",RX_EN_IDLE_HOLD_CDR_0="FALSE",RX_EN_IDLE_RESET_FR_0="TRUE",RX_EN_IDLE_RESET_PH_0="TRUE",RX_STATUS_FMT_0="SATA",TRANS_TIME_FRO
M_P2_0=12'b0111100,TRANS_TIME_NON_P2_0=8'b011001,TRANS_TIME_TO_P2_0=10'b01100100,CB2_INH_CC_PERIOD_1=8,CDR_PH_ADJ_TIME_1=5'b01010,PCI_EXPRESS_MODE_1="FALSE",RX_EN_IDLE_HOLD_CDR_1="FALSE",RX_EN_IDLE_RESET_FR_1="TRUE",RX_EN_IDLE_RESET_PH_1="TRUE",RX_STATUS_FMT_1="PCIE",TRANS_TIME_FROM_P2_1=12'b0111100,TRANS_TIME_NON_P2_1=8'b011001,TRANS_TIME_TO_P2_1=10'b01100100,SATA_BURST_VAL_0=3'b100,SATA_IDLE_VAL_0=3'b100,SATA_MAX_BURST_0=7,SATA_MAX_INIT_0=22,SATA_MAX_WAKE_0=7,SATA_MIN_BURST_0=4,SATA_MIN_INIT_0=12,SATA_MIN_WAKE_0=4,SATA_BURST_VAL_1=3'b100,SATA_IDLE_VAL_1=3'b100,SATA_MAX_BURST_1=10,SATA_MAX_INIT_1=29,SATA_MAX_WAKE_1=10,SATA_MIN_BURST_1=5,SATA_MIN_INIT_1=16,SATA_MIN_WAKE_1=5>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp_tile.v" Line 587: Assignment to rxchariscomma0_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp_tile.v" Line 589: Assignment to rxcharisk0_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp_tile.v" Line 590: Assignment to rxcharisk1_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp_tile.v" Line 593: Assignment to rxdisperr0_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp_tile.v" Line 594: Assignment to rxdisperr1_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp_tile.v" Line 595: Assignment to rxnotintable0_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp_tile.v" Line 596: Assignment to rxnotintable1_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../xil_s6_gtpwizard_v1_6_dp_tile.v" Line 724: Assignment to txkerr1_float_i ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1011: Assignment to GTPlocked0 ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1013: Assignment to GTPREFCLK1 ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1014: Assignment to GTPdone0 ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1066: Assignment to GTPCLKOUT0 ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1080: Assignment to GTPTXCLKOUT1 ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1377: Assignment to mig2_cmd_empty ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1378: Assignment to mig2_cmd_full ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1379: Assignment to mig2_wr_full ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1380: Assignment to mig2_wr_empty ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1381: Assignment to mig2_wr_count ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1382: Assignment to mig2_wr_underrun ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1383: Assignment to mig2_wr_error ignored, since the identifier is never used

Elaborating module <memc3_infrastructure(C_MEMCLK_PERIOD=5000,C_RST_ACT_LOW=1,C_INPUT_CLK_TYPE="SINGLE_ENDED",C_CLKOUT0_DIVIDE=1,C_CLKOUT1_DIVIDE=1,C_CLKOUT2_DIVIDE=2,C_CLKOUT3_DIVIDE=8,C_CLKFBOUT_MULT=2,C_DIVCLK_DIVIDE=1)>.

Elaborating module <PLL_ADV(BANDWIDTH="OPTIMIZED",CLKIN1_PERIOD=5.0,CLKIN2_PERIOD=5.0,CLKOUT0_DIVIDE=1,CLKOUT1_DIVIDE=1,CLKOUT2_DIVIDE=2,CLKOUT3_DIVIDE=8,CLKOUT4_DIVIDE=1,CLKOUT5_DIVIDE=1,CLKOUT0_PHASE=0.0,CLKOUT1_PHASE=180.0,CLKOUT2_PHASE=0.0,CLKOUT3_PHASE=0.0,CLKOUT4_PHASE=0.0,CLKOUT5_PHASE=0.0,CLKOUT0_DUTY_CYCLE=0.5,CLKOUT1_DUTY_CYCLE=0.5,CLKOUT2_DUTY_CYCLE=0.5,CLKOUT3_DUTY_CYCLE=0.5,CLKOUT4_DUTY_CYCLE=0.5,CLKOUT5_DUTY_CYCLE=0.5,COMPENSATION="INTERNAL",DIVCLK_DIVIDE=1,CLKFBOUT_MULT=2,CLKFBOUT_PHASE=0.0,REF_JITTER=0.005)>.

Elaborating module <BUFPLL_MCB>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1612: Assignment to c3_rst0 ignored, since the identifier is never used

Elaborating module
<memc3_wrapper(C_MEMCLK_PERIOD=5000,C_CALIB_SOFT_IP="TRUE",C_SIMULATION="FALSE",C_ARB_NUM_TIME_SLOTS=12,C_ARB_TIME_SLOT_0=18'b01010011100101,C_ARB_TIME_SLOT_1=18'b01010011100101000,C_ARB_TIME_SLOT_2=18'b010011100101000001,C_ARB_TIME_SLOT_3=18'b011100101000001010,C_ARB_TIME_SLOT_4=18'b100101000001010011,C_ARB_TIME_SLOT_5=18'b101000001010011100,C_ARB_TIME_SLOT_6=18'b01010011100101,C_ARB_TIME_SLOT_7=18'b01010011100101000,C_ARB_TIME_SLOT_8=18'b010011100101000001,C_ARB_TIME_SLOT_9=18'b011100101000001010,C_ARB_TIME_SLOT_10=18'b100101000001010011,C_ARB_TIME_SLOT_11=18'b101000001010011100,C_MEM_TRAS=40000,C_MEM_TRCD=15000,C_MEM_TREFI=7800000,C_MEM_TRFC=105000,C_MEM_TRP=15000,C_MEM_TWR=15000,C_MEM_TRTP=7500,C_MEM_TWTR=7500,C_MEM_ADDR_ORDER="ROW_BANK_COLUMN",C_NUM_DQ_PINS=16,C_MEM_TYPE="DDR2",C_MEM_DENSITY="512Mb",C_MEM_BURST_LEN=4,C_MEM_CAS_LATENCY=3,C_MEM_ADDR_WIDTH=13,C_MEM_BANKADDR_WIDTH=2,C_MEM_NUM_COL_BITS=10,C_MEM_DDR1_2_ODS="FULL",C_MEM_DDR2_RTT="50OHMS",C_MEM_DDR2_DIFF_DQS_EN="YES",C_MEM_DDR2_3_PA_SR="FULL",C_
MEM_DDR2_3_HIGH_TEMP_SR="NORMAL",C_MEM_DDR3_CAS_LATENCY=6,C_MEM_DDR3_ODS="DIV6",C_MEM_DDR3_RTT="DIV2",C_MEM_DDR3_CAS_WR_LATENCY=5,C_MEM_DDR3_AUTO_SR="ENABLED",C_MEM_DDR3_DYN_WRT_ODT="OFF",C_MEM_MOBILE_PA_SR="FULL",C_MEM_MDDR_ODS="FULL",C_MC_CALIB_BYPASS="NO",C_MC_CALIBRATION_MODE="CALIBRATION",C_MC_CALIBRATION_DELAY="HALF",C_SKIP_IN_TERM_CAL=0,C_SKIP_DYNAMIC_CAL=0,C_LDQSP_TAP_DELAY_VAL=0,C_LDQSN_TAP_DELAY_VAL=0,C_UDQSP_TAP_DELAY_VAL=0,C_UDQSN_TAP_DELAY_VAL=0,C_DQ0_TAP_DELAY_VAL=0,C_DQ1_TAP_DELAY_VAL=0,C_DQ2_TAP_DELAY_VAL=0,C_DQ3_TAP_DELAY_VAL=0,C_DQ4_TAP_DELAY_VAL=0,C_DQ5_TAP_DELAY_VAL=0,C_DQ6_TAP_DELAY_VAL=0,C_DQ7_TAP_DELAY_VAL=0,C_DQ8_TAP_DELAY_VAL=0,C_DQ9_TAP_DELAY_VAL=0,C_DQ10_TAP_DELAY_VAL=0,C_DQ11_TAP_DELAY_VAL=0,C_DQ12_TAP_DELAY_VAL=0,C_DQ13_TAP_DELAY_VAL=0,C_DQ14_TAP_DELAY_VAL=0,C_DQ15_TAP_DELAY_VAL=0)>.

Elaborating module
<mcb_raw_wrapper(C_MEMCLK_PERIOD=5000,C_P0_MASK_SIZE=4,C_P0_DATA_PORT_SIZE=32,C_P1_MASK_SIZE=4,C_P1_DATA_PORT_SIZE=32,C_ARB_NUM_TIME_SLOTS=12,C_ARB_TIME_SLOT_0=18'b101100011010001000,C_ARB_TIME_SLOT_1=18'b0101100011010001,C_ARB_TIME_SLOT_2=18'b01000101100011010,C_ARB_TIME_SLOT_3=18'b010001000101100011,C_ARB_TIME_SLOT_4=18'b011010001000101100,C_ARB_TIME_SLOT_5=18'b100011010001000101,C_ARB_TIME_SLOT_6=18'b101100011010001000,C_ARB_TIME_SLOT_7=18'b0101100011010001,C_ARB_TIME_SLOT_8=18'b01000101100011010,C_ARB_TIME_SLOT_9=18'b010001000101100011,C_ARB_TIME_SLOT_10=18'b011010001000101100,C_ARB_TIME_SLOT_11=18'b100011010001000101,C_PORT_CONFIG="B32_B32_W32_W32_R32_R32",C_PORT_ENABLE=6'b111111,C_MEM_TRAS=40000,C_MEM_TRCD=15000,C_MEM_TREFI=7800000,C_MEM_TRFC=105000,C_MEM_TRP=15000,C_MEM_TWR=15000,C_MEM_TRTP=7500,C_MEM_TWTR=7500,C_MEM_ADDR_ORDER="ROW_BANK_COLUMN",C_NUM_DQ_PINS=16,C_MEM_TYPE="DDR2",C_MEM_DENSITY="512Mb",C_MEM_BURST_LEN=4,C_MEM_CAS_LATENCY=3,C_MEM_ADDR_WIDTH=13,C_MEM_BANKADDR_WIDTH=2,C_MEM_NUM_COL_BITS=10
,C_MEM_DDR1_2_ODS="FULL",C_MEM_DDR2_RTT="50OHMS",C_MEM_DDR2_DIFF_DQS_EN="YES",C_MEM_DDR2_3_PA_SR="FULL",C_MEM_DDR2_3_HIGH_TEMP_SR="NORMAL",C_MEM_DDR3_CAS_LATENCY=6,C_MEM_DDR3_ODS="DIV6",C_MEM_DDR3_RTT="DIV2",C_MEM_DDR3_CAS_WR_LATENCY=5,C_MEM_DDR3_AUTO_SR="ENABLED",C_MEM_DDR3_DYN_WRT_ODT="OFF",C_MEM_MOBILE_PA_SR="FULL",C_MEM_MDDR_ODS="FULL",C_MC_CALIBRATION_CLK_DIV=1,C_MC_CALIBRATION_MODE="CALIBRATION",C_MC_CALIBRATION_DELAY="HALF",C_MC_CALIB_BYPASS="NO",C_MC_CALIBRATION_RA=16'b0,C_MC_CALIBRATION_BA=4'b0,C_MC_CALIBRATION_CA=12'b0,C_CALIB_SOFT_IP="TRUE",C_SKIP_IN_TERM_CAL=0,C_SKIP_DYNAMIC_CAL=0,C_MEM_TZQINIT_MAXCNT=10'b1000000000,C_SKIP_DYN_IN_TERM=1'b1,C_SIMULATION="FALSE",LDQSP_TAP_DELAY_VAL=0,UDQSP_TAP_DELAY_VAL=0,LDQSN_TAP_DELAY_VAL=0,UDQSN_TAP_DELAY_VAL=0,DQ0_TAP_DELAY_VAL=0,DQ1_TAP_DELAY_VAL=0,DQ2_TAP_DELAY_VAL=0,DQ3_TAP_DELAY_VAL=0,DQ4_TAP_DELAY_VAL=0,DQ5_TAP_DELAY_VAL=0,DQ6_TAP_DELAY_VAL=0,DQ7_TAP_DELAY_VAL=0,DQ8_TAP_DELAY_VAL=0,DQ9_TAP_DELAY_VAL=0,DQ10_TAP_DELAY_VAL=0,DQ11_TAP_DELAY_VAL=0,DQ12_TAP_DELA
Y_VAL=0,DQ13_TAP_DELAY_VAL=0,DQ14_TAP_DELAY_VAL=0,DQ15_TAP_DELAY_VAL=0)>.
WARNING:HDLCompiler:872 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_raw_wrapper.v" Line 681: Using initial value of allzero since it is never assigned

Elaborating module
<MCB(PORT_CONFIG="B32_B32_W32_W32_R32_R32",MEM_WIDTH=16,MEM_TYPE="DDR2",MEM_BURST_LEN=4,MEM_ADDR_ORDER="ROW_BANK_COLUMN",MEM_CAS_LATENCY=3,MEM_DDR3_CAS_LATENCY=6,MEM_DDR2_WRT_RECOVERY=3,MEM_DDR3_WRT_RECOVERY=5,MEM_MOBILE_PA_SR="FULL",MEM_DDR1_2_ODS="FULL",MEM_DDR3_ODS="DIV6",MEM_DDR2_RTT="50OHMS",MEM_DDR3_RTT="DIV2",MEM_DDR3_ADD_LATENCY="OFF",MEM_DDR2_ADD_LATENCY=0,MEM_MOBILE_TC_SR=0,MEM_MDDR_ODS="FULL",MEM_DDR2_DIFF_DQS_EN="YES",MEM_DDR2_3_PA_SR="FULL",MEM_DDR3_CAS_WR_LATENCY=5,MEM_DDR3_AUTO_SR="ENABLED",MEM_DDR2_3_HIGH_TEMP_SR="NORMAL",MEM_DDR3_DYN_WRT_ODT="OFF",MEM_RA_SIZE=13,MEM_BA_SIZE=2,MEM_CA_SIZE=10,MEM_RAS_VAL=8,MEM_RCD_VAL=3,MEM_REFI_VAL=1560,MEM_RFC_VAL=21,MEM_RP_VAL=3,MEM_WR_VAL=3,MEM_RTP_VAL=32'sb010,MEM_WTR_VAL=2,CAL_BYPASS="NO",CAL_RA=16'b0,CAL_BA=4'b0,CAL_CA=12'b0,CAL_CLK_DIV=1,CAL_DELAY="HALF",ARB_NUM_TIME_SLOTS=12,ARB_TIME_SLOT_0=18'b101100011010001000,ARB_TIME_SLOT_1=18'b0101100011010001,ARB_TIME_SLOT_2=18'b01000101100011010,ARB_TIME_SLOT_3=18'b010001000101100011,ARB_TIME_SLOT_4=18'b0110100
01000101100,ARB_TIME_SLOT_5=18'b100011010001000101,ARB_TIME_SLOT_6=18'b101100011010001000,ARB_TIME_SLOT_7=18'b0101100011010001,ARB_TIME_SLOT_8=18'b01000101100011010,ARB_TIME_SLOT_9=18'b010001000101100011,ARB_TIME_SLOT_10=18'b011010001000101100,ARB_TIME_SLOT_11=18'b100011010001000101)>.

Elaborating module <mcb_soft_calibration_top(C_MEM_TZQINIT_MAXCNT=10'b1000000000,C_MC_CALIBRATION_MODE="CALIBRATION",SKIP_IN_TERM_CAL=0,SKIP_DYNAMIC_CAL=0,SKIP_DYN_IN_TERM=1'b1,C_SIMULATION="FALSE",C_MEM_TYPE="DDR2")>.

Elaborating module <mcb_soft_calibration(C_MEM_TZQINIT_MAXCNT=10'b1000000000,C_MC_CALIBRATION_MODE="CALIBRATION",SKIP_IN_TERM_CAL=0,SKIP_DYNAMIC_CAL=0,SKIP_DYN_IN_TERM=1'b1,C_SIMULATION="FALSE",C_MEM_TYPE="DDR2")>.
WARNING:HDLCompiler:872 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" Line 312: Using initial value of START_BROADCAST since it is never assigned
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" Line 373: Assignment to Half_MV_DU ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" Line 375: Assignment to Half_MV_DD ignored, since the identifier is never used

Elaborating module <iodrp_controller>.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/iodrp_controller.v" Line 186: Result of 4-bit expression is truncated to fit in 3-bit target.

Elaborating module <iodrp_mcb_controller>.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/iodrp_mcb_controller.v" Line 301: Result of 4-bit expression is truncated to fit in 3-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/iodrp_mcb_controller.v" Line 312: Result of 9-bit expression is truncated to fit in 8-bit target.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" Line 408: Assignment to MCB_READ_DATA ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" Line 654: Assignment to MCB_UODATAVALID_U ignored, since the identifier is never used
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" Line 809: Result of 7-bit expression is truncated to fit in 6-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" Line 813: Result of 8-bit expression is truncated to fit in 6-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" Line 859: Result of 8-bit expression is truncated to fit in 7-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" Line 863: Result of 8-bit expression is truncated to fit in 6-bit target.
WARNING:HDLCompiler:413 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" Line 864: Result of 8-bit expression is truncated to fit in 7-bit target.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" Line 700: Assignment to IODRPCTRLR_USE_BKST ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration_top.v" Line 216: Assignment to Max_Value ignored, since the identifier is never used

Elaborating module <IOBUF>.

Elaborating module <IODRP2>.

Elaborating module <OSERDES2(BYPASS_GCLK_FF="TRUE",DATA_RATE_OQ="SDR",DATA_RATE_OT="SDR",OUTPUT_MODE="SINGLE_ENDED",SERDES_MODE="MASTER",DATA_WIDTH=2)>.

Elaborating module <OSERDES2(BYPASS_GCLK_FF="TRUE",DATA_RATE_OQ="SDR",DATA_RATE_OT="SDR",OUTPUT_MODE="SINGLE_ENDED",SERDES_MODE="MASTER",DATA_WIDTH=2,TRAIN_PATTERN=15)>.

Elaborating module <OSERDES2(BYPASS_GCLK_FF="TRUE",DATA_RATE_OQ="SDR",DATA_RATE_OT="SDR",OUTPUT_MODE="SINGLE_ENDED",SERDES_MODE="MASTER",DATA_WIDTH=2,TRAIN_PATTERN=5)>.

Elaborating module <OSERDES2(BYPASS_GCLK_FF="TRUE",DATA_RATE_OQ="SDR",DATA_RATE_OT="SDR",OUTPUT_MODE="SINGLE_ENDED",SERDES_MODE="SLAVE",DATA_WIDTH=2)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=7,ODELAY_VALUE=0,SERDES_MODE="MASTER",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=7,ODELAY_VALUE=0,SERDES_MODE="SLAVE",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=6,ODELAY_VALUE=0,SERDES_MODE="MASTER",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=6,ODELAY_VALUE=0,SERDES_MODE="SLAVE",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=14,ODELAY_VALUE=0,SERDES_MODE="MASTER",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=14,ODELAY_VALUE=0,SERDES_MODE="SLAVE",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=5,ODELAY_VALUE=0,SERDES_MODE="MASTER",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=5,ODELAY_VALUE=0,SERDES_MODE="SLAVE",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=4,ODELAY_VALUE=0,SERDES_MODE="MASTER",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=4,ODELAY_VALUE=0,SERDES_MODE="SLAVE",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=0,ODELAY_VALUE=0,SERDES_MODE="MASTER",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=0,ODELAY_VALUE=0,SERDES_MODE="SLAVE",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=1,ODELAY_VALUE=0,SERDES_MODE="MASTER",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=1,ODELAY_VALUE=0,SERDES_MODE="SLAVE",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=15,ODELAY_VALUE=0,SERDES_MODE="MASTER",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=15,ODELAY_VALUE=0,SERDES_MODE="SLAVE",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=3,ODELAY_VALUE=0,SERDES_MODE="MASTER",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=3,ODELAY_VALUE=0,SERDES_MODE="SLAVE",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=2,ODELAY_VALUE=0,SERDES_MODE="MASTER",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=2,ODELAY_VALUE=0,SERDES_MODE="SLAVE",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=8,ODELAY_VALUE=0,SERDES_MODE="MASTER",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <IODRP2_MCB(DATA_RATE="SDR",IDELAY_VALUE=0,MCB_ADDRESS=8,ODELAY_VALUE=0,SERDES_MODE="SLAVE",SIM_TAPDELAY_VALUE=10)>.

Elaborating module <OBUFT>.

Elaborating module <IOBUFDS>.

Elaborating module <PULLDOWN>.

Elaborating module <PULLUP>.
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" Line 524: Assignment to uo_data ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" Line 525: Assignment to uo_data_valid ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" Line 527: Assignment to uo_cmd_ready_in ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" Line 528: Assignment to uo_refrsh_flag ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" Line 529: Assignment to uo_cal_start ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" Line 530: Assignment to uo_sdo ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" Line 531: Assignment to status ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1756: Assignment to c3_p1_cmd_empty ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1757: Assignment to c3_p1_cmd_full ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1762: Assignment to c3_p1_wr_full ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1763: Assignment to c3_p1_wr_empty ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1764: Assignment to c3_p1_wr_count ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1765: Assignment to c3_p1_wr_underrun ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1766: Assignment to c3_p1_wr_error ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1769: Assignment to c3_p1_rd_data ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1770: Assignment to c3_p1_rd_full ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1771: Assignment to c3_p1_rd_empty ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1772: Assignment to c3_p1_rd_count ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1773: Assignment to c3_p1_rd_overflow ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1774: Assignment to c3_p1_rd_error ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1796: Assignment to c3_p3_cmd_empty ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1797: Assignment to c3_p3_cmd_full ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1802: Assignment to c3_p3_wr_full ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1803: Assignment to c3_p3_wr_empty ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1804: Assignment to c3_p3_wr_count ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1805: Assignment to c3_p3_wr_underrun ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1806: Assignment to c3_p3_wr_error ignored, since the identifier is never used
WARNING:HDLCompiler:1127 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1838: Assignment to selfrefresh_mode ignored, since the identifier is never used
WARNING:HDLCompiler:634 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 199: Net <mig2_cmd_en> does not have a driver.
WARNING:HDLCompiler:634 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 200: Net <mig2_cmd_instr[2]> does not have a driver.
WARNING:HDLCompiler:634 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 201: Net <mig2_cmd_bl[5]> does not have a driver.
WARNING:HDLCompiler:634 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 202: Net <mig2_cmd_byte_addr[29]> does not have a driver.
WARNING:HDLCompiler:634 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 205: Net <mig2_wr_en> does not have a driver.
WARNING:HDLCompiler:634 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 206: Net <mig2_wr_mask[3]> does not have a driver.
WARNING:HDLCompiler:634 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 207: Net <mig2_wr_data[31]> does not have a driver.
WARNING:HDLCompiler:634 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 1837: Net <selfrefresh_enter> does not have a driver.
WARNING:HDLCompiler:552 - "\PROJECT\EXP6T_PCIE3F\xise\../exp6t_disp.v" Line 430: Input port cfg_miso_i is not connected on this instance

=========================================================================
*                           HDL Synthesis                               *
=========================================================================

Synthesizing Unit <exp6t_disp>.
    Related source file is "/project/exp6t_pcie3f/exp6t_disp.v".
        FAST_TRAIN = "FALSE"
        GTP_RESET_SPEEDUP = 0
        GTP_SIMULATION = 0
        DEBUG_EN = 0
        C3_SIMULATION = "FALSE"
WARNING:Xst:2898 - Port 'cfg_miso_i', unconnected in block instance 'inst_sp6wrap', is tied to GND.
WARNING:Xst:647 - Input <dipsw<3:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <pushsw<2:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cpcie_rxp> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cpcie_rxn> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cpcie_refclkn> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cpcie_refclkp> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cpcie_perst> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <TMDS_HPD> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <DP_RSV1> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <DP_RSV2> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <USB_FLAGA> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <USB_FLAGB> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <USB_FLAGC> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <USB_CLKOUT> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <CFG_MISO> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <CFG_RESET_N> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <CFG_RESET> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <gpio_out> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <user_addr_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <user_length_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <dma_rddata_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <dma_addr_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <dma_remain_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <dma_pktsize_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <xio_diag_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <debug_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <cfg_clk_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <cfg_cs_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <cfg_mosi_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <cfg_busy_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <user_dreq_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <bar0_rdreq_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <bar1_wr_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <bar1_rdreq_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <bar2_wr_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <bar2_rdreq_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <dma_wr_ack_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <dma_rd_ack_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <dma_dvalid_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <dma_dreq_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <dma_corebusy_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <int_available_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 430: Output port <int_ack_o> of the instance <inst_sp6wrap> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 641: Output port <crtc_io_rdata> of the instance <crtc1> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 641: Output port <crtc_io_ack> of the instance <crtc1> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 711: Output port <crtc_io_rdata> of the instance <crtc2> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 711: Output port <crtc_io_ack> of the instance <crtc2> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 864: Output port <TX_LANE1> of the instance <dp_main> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 864: Output port <TX_LANE2> of the instance <dp_main> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 864: Output port <TX_LANE3> of the instance <dp_main> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 864: Output port <TX_STAT_TR1> of the instance <dp_main> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 864: Output port <TX_STAT_TR2> of the instance <dp_main> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 864: Output port <REF_HS> of the instance <dp_main> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 864: Output port <REF_VS> of the instance <dp_main> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 864: Output port <REF_DE> of the instance <dp_main> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXCHARISCOMMA0_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXCHARISK0_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXCHARISK1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXDISPERR0_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXDISPERR1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXNOTINTABLE0_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXNOTINTABLE1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXCLKCORCNT0_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXDATA0_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXDATA1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXBUFSTATUS1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXSTATUS0_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXLOSSOFSYNC1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_GTPCLKOUT0_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_TXKERR1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_TXBUFSTATUS1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_PLLLKDET0_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_REFCLKOUT1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RESETDONE0_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXBYTEISALIGNED1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXPRBSERR1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXELECIDLE0_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_RXELECIDLE1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 996: Output port <TILE0_TXOUTCLK1_OUT> of the instance <xil_s6_gtpwizard_v1_6_dp_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1605: Output port <rst0> of the instance <memc3_infrastructure_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_wr_count> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_rd_data> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_rd_count> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p2_wr_count> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p3_wr_count> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_cmd_empty> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_cmd_full> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_wr_full> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_wr_empty> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_wr_underrun> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_wr_error> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_rd_full> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_rd_empty> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_rd_overflow> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p1_rd_error> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p2_cmd_empty> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p2_cmd_full> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p2_wr_full> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p2_wr_empty> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p2_wr_underrun> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p2_wr_error> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p3_cmd_empty> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p3_cmd_full> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p3_wr_full> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p3_wr_empty> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p3_wr_underrun> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <p3_wr_error> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/exp6t_disp.v" line 1699: Output port <selfrefresh_mode> of the instance <memc3_wrapper_inst> is unconnected or connected to loadless signal.
Always blocking tristate driving signal <TMDS_CEC> is removed.
Always blocking tristate driving signal <TMDS_SCL> is removed.
Always blocking tristate driving signal <TMDS_SDA> is removed.
Always blocking tristate driving signal <GPIO9C<29>> is removed.
Always blocking tristate driving signal <GPIO9C<28>> is removed.
Always blocking tristate driving signal <GPIO9C<27>> is removed.
Always blocking tristate driving signal <GPIO9C<26>> is removed.
Always blocking tristate driving signal <GPIO9C<25>> is removed.
Always blocking tristate driving signal <GPIO9C<24>> is removed.
Always blocking tristate driving signal <GPIO9C<23>> is removed.
Always blocking tristate driving signal <GPIO9C<22>> is removed.
Always blocking tristate driving signal <GPIO9C<21>> is removed.
Always blocking tristate driving signal <GPIO9C<20>> is removed.
Always blocking tristate driving signal <GPIO9C<19>> is removed.
Always blocking tristate driving signal <GPIO9C<18>> is removed.
Always blocking tristate driving signal <GPIO9C<17>> is removed.
Always blocking tristate driving signal <GPIO9C<16>> is removed.
Always blocking tristate driving signal <GPIO9C<15>> is removed.
Always blocking tristate driving signal <GPIO9C<14>> is removed.
Always blocking tristate driving signal <GPIO9C<13>> is removed.
Always blocking tristate driving signal <GPIO9C<12>> is removed.
Always blocking tristate driving signal <GPIO9C<11>> is removed.
Always blocking tristate driving signal <GPIO9C<10>> is removed.
Always blocking tristate driving signal <GPIO9C<9>> is removed.
Always blocking tristate driving signal <GPIO9C<8>> is removed.
Always blocking tristate driving signal <GPIO9C<7>> is removed.
Always blocking tristate driving signal <GPIO9C<6>> is removed.
Always blocking tristate driving signal <GPIO9C<5>> is removed.
Always blocking tristate driving signal <GPIO9C<4>> is removed.
Always blocking tristate driving signal <GPIO9C<3>> is removed.
Always blocking tristate driving signal <GPIO9C<2>> is removed.
Always blocking tristate driving signal <GPIO9C<1>> is removed.
Always blocking tristate driving signal <GPIO9C<0>> is removed.
Always blocking tristate driving signal <USB_FD<15>> is removed.
Always blocking tristate driving signal <USB_FD<14>> is removed.
Always blocking tristate driving signal <USB_FD<13>> is removed.
Always blocking tristate driving signal <USB_FD<12>> is removed.
Always blocking tristate driving signal <USB_FD<11>> is removed.
Always blocking tristate driving signal <USB_FD<10>> is removed.
Always blocking tristate driving signal <USB_FD<9>> is removed.
Always blocking tristate driving signal <USB_FD<8>> is removed.
Always blocking tristate driving signal <USB_FD<7>> is removed.
Always blocking tristate driving signal <USB_FD<6>> is removed.
Always blocking tristate driving signal <USB_FD<5>> is removed.
Always blocking tristate driving signal <USB_FD<4>> is removed.
Always blocking tristate driving signal <USB_FD<3>> is removed.
Always blocking tristate driving signal <USB_FD<2>> is removed.
Always blocking tristate driving signal <USB_FD<1>> is removed.
Always blocking tristate driving signal <USB_FD<0>> is removed.
WARNING:Xst:653 - Signal <mig2_cmd_instr> is used but never assigned. This sourceless signal will be automatically connected to value GND.
WARNING:Xst:653 - Signal <mig2_cmd_bl> is used but never assigned. This sourceless signal will be automatically connected to value GND.
WARNING:Xst:653 - Signal <mig2_cmd_byte_addr> is used but never assigned. This sourceless signal will be automatically connected to value GND.
WARNING:Xst:653 - Signal <mig2_wr_mask> is used but never assigned. This sourceless signal will be automatically connected to value GND.
WARNING:Xst:653 - Signal <mig2_wr_data> is used but never assigned. This sourceless signal will be automatically connected to value GND.
WARNING:Xst:653 - Signal <mig2_cmd_en> is used but never assigned. This sourceless signal will be automatically connected to value GND.
WARNING:Xst:653 - Signal <mig2_wr_en> is used but never assigned. This sourceless signal will be automatically connected to value GND.
WARNING:Xst:653 - Signal <selfrefresh_enter> is used but never assigned. This sourceless signal will be automatically connected to value GND.
    Found 32-bit register for signal <bar0_rdata_r>.
    Found 1-bit register for signal <aux_hpd_r>.
    Found 2-bit register for signal <aux_hpd_in_r>.
    Found 16-bit register for signal <aux_hpd_count_r>.
    Found 16-bit adder for signal <aux_hpd_count_r[15]_GND_1_o_add_60_OUT> created at line 830.
    Summary:
	inferred   1 Adder/Subtractor(s).
	inferred  51 D-type flip-flop(s).
	inferred  10 Multiplexer(s).
Unit <exp6t_disp> synthesized.

Synthesizing Unit <xil_clk_wiz_v1_6_50x200>.
    Related source file is "/project/exp6t_pcie3f/xil_clk_wiz_v1_6_50x200.v".
    Summary:
	no macro.
Unit <xil_clk_wiz_v1_6_50x200> synthesized.

Synthesizing Unit <xil_clk_wiz_v1_6_50x62x312>.
    Related source file is "/project/exp6t_pcie3f/xil_clk_wiz_v1_6_50x62x312.v".
    Summary:
	no macro.
Unit <xil_clk_wiz_v1_6_50x62x312> synthesized.

Synthesizing Unit <xil_clk_wiz_v1_6_27x162>.
    Related source file is "/project/exp6t_pcie3f/xil_clk_wiz_v1_6_27x162.v".
    Summary:
	no macro.
Unit <xil_clk_wiz_v1_6_27x162> synthesized.

Synthesizing Unit <sp6wrap>.
    Related source file is "/project/exp6t_pcie3f/pciesample/sp6wrap.v".
        FAST_TRAIN = "FALSE"
        USE_PCIE_CABLE = "FALSE"
WARNING:Xst:647 - Input <customize_c<259:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <keycode_c<63:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <gpio_in<31:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <sw_i<7:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <bar2_rdata_i<31:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <dma_cfg_c<15:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <dma_sysaddr_i<31:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <dma_lcladdr_i<31:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <dma_length_i<9:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <dma_wrdata_i<31:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_miso_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <bar2_rdack_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <dma_wr_req_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <dma_rd_req_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <dma_userrun_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <int_reqline_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
INFO:Xst:3010 - "/project/exp6t_pcie3f/pciesample/sp6wrap.v" line 229: Output port <bar0_wend> of the instance <app> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/pciesample/sp6wrap.v" line 229: Output port <bar1_wend> of the instance <app> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/pciesample/sp6wrap.v" line 359: Output port <received_hot_reset> of the instance <eptest_i> is unconnected or connected to loadless signal.
    Summary:
	no macro.
Unit <sp6wrap> synthesized.

Synthesizing Unit <xt_pcie_app_s6>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/example_design/xt_pcie_app_s6.v".
WARNING:Xst:647 - Input <bar1_rdata<31:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <trn_tbuf_av<5:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <trn_fc_cpld<11:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <trn_fc_cplh<7:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <trn_fc_npd<11:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <trn_fc_nph<7:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <trn_fc_pd<11:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <trn_fc_ph<7:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_do<31:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_interrupt_do<7:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_interrupt_mmenable<2:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_status<15:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_command<15:3>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_command<1:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_dstatus<15:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_dcommand<15:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_lstatus<15:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_lcommand<15:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_pcie_link_state_n<2:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <bar1_burst> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <bar1_wbusy> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <bar1_rdack> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <trn_tcfg_req_n> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <trn_terr_drop_n> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <trn_rerrfwd_n> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_rd_wr_done_n> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_err_cpl_rdy_n> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_interrupt_rdy_n> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_interrupt_msienable> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/example_design/xt_pcie_app_s6.v" line 286: Output port <user_rreq> of the instance <PIO> is unconnected or connected to loadless signal.
    Found 10-bit register for signal <buff_wr_addr_r>.
    Found 32-bit register for signal <buff_wr_data_r>.
    Found 1-bit register for signal <buff_wr_req_r>.
    Summary:
	inferred  43 D-type flip-flop(s).
	inferred   6 Multiplexer(s).
Unit <xt_pcie_app_s6> synthesized.

Synthesizing Unit <xt_PIO>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/example_design/xt_pio.v".
    Summary:
	no macro.
Unit <xt_PIO> synthesized.

Synthesizing Unit <xt_PIO_EP>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/example_design/xt_pio_ep.v".
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/example_design/xt_pio_ep.v" line 203: Output port <rd_be_o> of the instance <EP_TX> is unconnected or connected to loadless signal.
    Summary:
	no macro.
Unit <xt_PIO_EP> synthesized.

Synthesizing Unit <xt_PIO_32_RX_ENGINE>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/example_design/xt_pio_32_rx_engine.v".
    Set property "fsm_encoding = one-hot" for signal <state>.
WARNING:Xst:647 - Input <trn_rsrc_dsc_n> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <compl_rdy_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <usr_rbusy_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
    Found 8-bit register for signal <be_in_r>.
    Found 32-bit register for signal <addr_r>.
    Found 8-bit register for signal <be_r>.
    Found 10-bit register for signal <len_r>.
    Found 1-bit register for signal <len_end_r>.
    Found 1-bit register for signal <tlp_type_rd_r>.
    Found 1-bit register for signal <tlp_type_iowr_r>.
    Found 1-bit register for signal <tlp_type_cmpl_r>.
    Found 1-bit register for signal <rdst_rdy_n_r>.
    Found 1-bit register for signal <compl_r>.
    Found 1-bit register for signal <compl_with_data_r>.
    Found 1-bit register for signal <req_r>.
    Found 1-bit register for signal <wen_r>.
    Found 1-bit register for signal <wr_r>.
    Found 1-bit register for signal <wend_r>.
    Found 1-bit register for signal <ren_r>.
    Found 1-bit register for signal <rd_r>.
    Found 4-bit register for signal <state>.
    Found 32-bit register for signal <TLP_HDR1_r>.
    Found 32-bit register for signal <TLP_HDR2_r>.
    Found 32-bit register for signal <TLP_HDR3_r>.
    Found 32-bit register for signal <wdata_r>.
    Found 7-bit register for signal <bar_r>.
    Found 10-bit subtractor for signal <len_r[9]_GND_65_o_sub_154_OUT>.
    Found 12-bit adder for signal <addr_r[11]_GND_65_o_add_82_OUT> created at line 257.
    Summary:
	inferred   2 Adder/Subtractor(s).
	inferred 210 D-type flip-flop(s).
	inferred  94 Multiplexer(s).
Unit <xt_PIO_32_RX_ENGINE> synthesized.

Synthesizing Unit <xt_PIO_32_TX_ENGINE>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/example_design/xt_pio_32_tx_engine.v".
WARNING:Xst:647 - Input <req_addr_i<1:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <usr_rack_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <usr_rbusy_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <usr_burst_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <usr_rd_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <cfg_bus_mstr_enable_i> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
    Found 1-bit register for signal <req_compl_q>.
    Found 1-bit register for signal <req_compl_with_data_q>.
    Found 1-bit register for signal <rdy_o>.
    Found 1-bit register for signal <done_o>.
    Found 10-bit register for signal <length_r>.
    Found 1-bit register for signal <ren_r>.
    Found 1-bit register for signal <rd_end_r>.
    Found 32-bit register for signal <addr_r>.
    Found 8-bit register for signal <be_r>.
    Found 4-bit register for signal <mask_r<3:0>>.
    Found 1-bit register for signal <tsof_n>.
    Found 1-bit register for signal <teof_n>.
    Found 1-bit register for signal <tsrc_rdy_n>.
    Found 1-bit register for signal <tsrc_dsc_n>.
    Found 32-bit register for signal <td_r>.
    Found 1-bit register for signal <cpl_w_data>.
    Found 3-bit register for signal <state>.
    Found 12-bit register for signal <byte_count>.
    Found 12-bit subtractor for signal <length>.
    Found 10-bit subtractor for signal <length_r[9]_GND_66_o_sub_144_OUT>.
    Found 12-bit adder for signal <n0439> created at line 183.
    Found 12-bit adder for signal <byte_count_be_low[11]_length[11]_add_99_OUT> created at line 183.
    Found 12-bit adder for signal <addr_r[11]_GND_66_o_add_208_OUT> created at line 347.
    Summary:
	inferred   5 Adder/Subtractor(s).
	inferred 112 D-type flip-flop(s).
	inferred  47 Multiplexer(s).
Unit <xt_PIO_32_TX_ENGINE> synthesized.

Synthesizing Unit <xt_PIO_TO_CTRL>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/example_design/xt_pio_to_ctrl.v".
    Found 1-bit register for signal <turnoff_ok_n>.
    Found 1-bit register for signal <trn_pending>.
    Summary:
	inferred   2 D-type flip-flop(s).
Unit <xt_PIO_TO_CTRL> synthesized.

Synthesizing Unit <xt_mem>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/example_design/xt_mem.v".
WARNING:Xst:647 - Input <mig_wr_count<6:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_rd_count<6:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <sys_addr<1:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_clk> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_cmd_full> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_wr_full> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_wr_empty> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_wr_underrun> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_wr_error> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_rd_full> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_rd_overflow> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_rd_error> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
    Found 1-bit register for signal <mem_busy_r>.
    Found 1-bit register for signal <mem_init_done_r>.
    Found 4-bit register for signal <mem_wr_mask0_r>.
    Found 4-bit register for signal <mem_wr_mask1_r>.
    Found 4-bit register for signal <mem_wr_mask2_r>.
    Found 4-bit register for signal <mem_wr_mask3_r>.
    Found 4-bit register for signal <mem_wr_mask_out0_r>.
    Found 4-bit register for signal <mem_wr_mask_out1_r>.
    Found 4-bit register for signal <mem_wr_mask_out2_r>.
    Found 4-bit register for signal <mem_wr_mask_out3_r>.
    Found 5-bit register for signal <mem_wait_full_r>.
    Found 5-bit register for signal <mem_wait_empt_r>.
    Found 4-bit register for signal <mem_state_r>.
    Found 4-bit register for signal <mem_wr_req_out_r>.
    Found 6-bit register for signal <mem_cmd_len_r>.
    Found 3-bit register for signal <mem_cmd_wr_r<2:0>>.
    Found 3-bit register for signal <mem_cmd_instr_r>.
    Found 32-bit register for signal <mem_cmd_addr_r>.
    Found 32-bit register for signal <mem_cmd_addr_out_r>.
    Found 32-bit register for signal <mem_wr_data0_r>.
    Found 32-bit register for signal <mem_wr_data1_r>.
    Found 32-bit register for signal <mem_wr_data2_r>.
    Found 32-bit register for signal <mem_wr_data3_r>.
    Found 32-bit register for signal <mem_wr_data_out0_r>.
    Found 32-bit register for signal <mem_wr_data_out1_r>.
    Found 32-bit register for signal <mem_wr_data_out2_r>.
    Found 32-bit register for signal <mem_wr_data_out3_r>.
    Found 32-bit register for signal <mem_rd_data_out_r>.
    Found 10-bit register for signal <mem_cmd_addr_count_r>.
    Found 10-bit register for signal <mem_rd_addr_r>.
    Found 10-bit register for signal <mem_rd_addr_count_r>.
    Found 10-bit register for signal <mem_rd_addr_out_r>.
    Found 1-bit register for signal <mem_cmd_req_r>.
    Found 1-bit register for signal <mem_wr_end_r>.
    Found 1-bit register for signal <mem_rd_ack_r>.
    Found 1-bit register for signal <mem_rd_addr_end_r>.
    Found 1-bit register for signal <mem_rd_out_r>.
INFO:Xst:1799 - State 0101 is never reached in FSM <mem_state_r>.
    Found finite state machine <FSM_0> for signal <mem_state_r>.
    -----------------------------------------------------------------------
    | States             | 9                                              |
    | Transitions        | 23                                             |
    | Inputs             | 12                                             |
    | Outputs            | 10                                             |
    | Clock              | sys_clk (rising_edge)                          |
    | Reset              | sys_rst_n (negative)                           |
    | Reset type         | asynchronous                                   |
    | Reset State        | 0000                                           |
    | Encoding           | auto                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found 10-bit subtractor for signal <mem_cmd_addr_count_r[9]_GND_68_o_sub_304_OUT>.
    Found 10-bit subtractor for signal <mem_cmd_addr_count_r[9]_GND_68_o_sub_308_OUT>.
    Found 10-bit subtractor for signal <mem_rd_addr_count_r[9]_GND_68_o_sub_539_OUT>.
    Found 2-bit adder for signal <mem_wait_full_r[3]_GND_68_o_add_47_OUT> created at line 308.
    Found 2-bit adder for signal <mem_wait_empt_r[3]_GND_68_o_add_61_OUT> created at line 320.
    Found 12-bit adder for signal <n0636> created at line 432.
    Found 12-bit adder for signal <mem_cmd_addr_r[11]_GND_68_o_add_260_OUT> created at line 432.
    Found 10-bit adder for signal <mem_rd_addr_r[9]_GND_68_o_add_529_OUT> created at line 542.
    Summary:
	inferred   8 Adder/Subtractor(s).
	inferred 457 D-type flip-flop(s).
	inferred  89 Multiplexer(s).
	inferred   1 Finite State Machine(s).
Unit <xt_mem> synthesized.

Synthesizing Unit <eptest>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v".
        TL_TX_RAM_RADDR_LATENCY = 1'b0
        TL_TX_RAM_RDATA_LATENCY = 2'b10
        TL_RX_RAM_RADDR_LATENCY = 1'b0
        TL_RX_RAM_RDATA_LATENCY = 2'b10
        TL_RX_RAM_WRITE_LATENCY = 1'b0
        VC0_TX_LASTPACKET = 5'b01100
        VC0_RX_RAM_LIMIT = 12'b000111111111
        VC0_TOTAL_CREDITS_PH = 7'b0010000
        VC0_TOTAL_CREDITS_PD = 11'b00000101001
        VC0_TOTAL_CREDITS_NPH = 7'b0001000
        VC0_TOTAL_CREDITS_CH = 7'b0010000
        VC0_TOTAL_CREDITS_CD = 11'b00000101001
        VC0_CPL_INFINITE = "TRUE"
        BAR0 = 32'b11111111111111110000000000000000
        BAR1 = 32'b11111110000000000000000000000000
        BAR2 = 32'b00000000000000000000000000000000
        BAR3 = 32'b00000000000000000000000000000000
        BAR4 = 32'b00000000000000000000000000000000
        BAR5 = 32'b00000000000000000000000000000000
        EXPANSION_ROM = 22'b0000000000000000000000
        DISABLE_BAR_FILTERING = "FALSE"
        DISABLE_ID_CHECK = "FALSE"
        TL_TFC_DISABLE = "FALSE"
        TL_TX_CHECKS_DISABLE = "FALSE"
        USR_CFG = "FALSE"
        USR_EXT_CFG = "FALSE"
        DEV_CAP_MAX_PAYLOAD_SUPPORTED = 3'b000
        CLASS_CODE = 24'b000001000000000000000000
        CARDBUS_CIS_POINTER = 32'b00000000000000000000000000000000
        PCIE_CAP_CAPABILITY_VERSION = 4'b0001
        PCIE_CAP_DEVICE_PORT_TYPE = 4'b0001
        PCIE_CAP_SLOT_IMPLEMENTED = "FALSE"
        PCIE_CAP_INT_MSG_NUM = 5'b00000
        DEV_CAP_PHANTOM_FUNCTIONS_SUPPORT = 2'b00
        DEV_CAP_EXT_TAG_SUPPORTED = "FALSE"
        DEV_CAP_ENDPOINT_L0S_LATENCY = 3'b111
        DEV_CAP_ENDPOINT_L1_LATENCY = 3'b111
        SLOT_CAP_ATT_BUTTON_PRESENT = "FALSE"
        SLOT_CAP_ATT_INDICATOR_PRESENT = "FALSE"
        SLOT_CAP_POWER_INDICATOR_PRESENT = "FALSE"
        DEV_CAP_ROLE_BASED_ERROR = "TRUE"
        LINK_CAP_ASPM_SUPPORT = 2'b01
        LINK_CAP_L0S_EXIT_LATENCY = 3'b111
        LINK_CAP_L1_EXIT_LATENCY = 3'b111
        LL_ACK_TIMEOUT = 15'b000000000000000
        LL_ACK_TIMEOUT_EN = "FALSE"
        LL_REPLAY_TIMEOUT = 15'b000000000000000
        LL_REPLAY_TIMEOUT_EN = "FALSE"
        MSI_CAP_MULTIMSGCAP = 3'b000
        MSI_CAP_MULTIMSG_EXTENSION = 1'b0
        LINK_STATUS_SLOT_CLOCK_CONFIG = "FALSE"
        PLM_AUTO_CONFIG = "FALSE"
        FAST_TRAIN = "FALSE"
        ENABLE_RX_TD_ECRC_TRIM = "FALSE"
        DISABLE_SCRAMBLING = "FALSE"
        PM_CAP_VERSION = 3'b011
        PM_CAP_PME_CLOCK = "FALSE"
        PM_CAP_DSI = "FALSE"
        PM_CAP_AUXCURRENT = 3'b000
        PM_CAP_D1SUPPORT = "TRUE"
        PM_CAP_D2SUPPORT = "TRUE"
        PM_CAP_PMESUPPORT = 5'b01111
        PM_DATA0 = 8'b00000000
        PM_DATA_SCALE0 = 2'b00
        PM_DATA1 = 8'b00000000
        PM_DATA_SCALE1 = 2'b00
        PM_DATA2 = 8'b00000000
        PM_DATA_SCALE2 = 2'b00
        PM_DATA3 = 8'b00000000
        PM_DATA_SCALE3 = 2'b00
        PM_DATA4 = 8'b00000000
        PM_DATA_SCALE4 = 2'b00
        PM_DATA5 = 8'b00000000
        PM_DATA_SCALE5 = 2'b00
        PM_DATA6 = 8'b00000000
        PM_DATA_SCALE6 = 2'b00
        PM_DATA7 = 8'b00000000
        PM_DATA_SCALE7 = 2'b00
        PCIE_GENERIC = 12'b000011101111
        GTP_SEL = 1'b1
        CFG_VEN_ID = 16'b0110100000001001
        CFG_DEV_ID = 16'b1000001000100000
        CFG_REV_ID = 8'b00000001
        CFG_SUBSYS_VEN_ID = 16'b0110100000001001
        CFG_SUBSYS_ID = 16'b1000001000100000
        REF_CLK_FREQ = 0
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXCHARISK0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXDISPERR0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXDISPERR1_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXNOTINTABLE0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXNOTINTABLE1_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXCLKCORCNT0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXCLKCORCNT1_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXDATA0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXSTATUS0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_GTPCLKOUT0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_PLLLKDET0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RESETDONE0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXELECIDLE0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_PHYSTATUS0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXVALID0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_RXVALID1_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_TXN0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/eptest/source/eptest.v" line 481: Output port <TILE0_TXP0_OUT> of the instance <GT_i> is unconnected or connected to loadless signal.
    Summary:
	no macro.
Unit <eptest> synthesized.

Synthesizing Unit <pcie_bram_top_s6>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/source/pcie_bram_top_s6.v".
        DEV_CAP_MAX_PAYLOAD_SUPPORTED = 3'b000
        VC0_TX_LASTPACKET = 5'b01100
        TLM_TX_OVERHEAD = 20
        TL_TX_RAM_RADDR_LATENCY = 1'b0
        TL_TX_RAM_RDATA_LATENCY = 2'b10
        TL_TX_RAM_WRITE_LATENCY = 1'b0
        VC0_RX_LIMIT = 12'b000111111111
        TL_RX_RAM_RADDR_LATENCY = 1'b0
        TL_RX_RAM_RDATA_LATENCY = 2'b10
        TL_RX_RAM_WRITE_LATENCY = 1'b0
    Summary:
	no macro.
Unit <pcie_bram_top_s6> synthesized.

Synthesizing Unit <pcie_brams_s6>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/source/pcie_brams_s6.v".
        NUM_BRAMS = 1
        RAM_RADDR_LATENCY = 1'b0
        RAM_RDATA_LATENCY = 2'b10
        RAM_WRITE_LATENCY = 1'b0
    Summary:
	no macro.
Unit <pcie_brams_s6> synthesized.

Synthesizing Unit <pcie_bram_s6>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/source/pcie_bram_s6.v".
        DOB_REG = 1
        WIDTH = 7'b0100100
WARNING:Xst:647 - Input <waddr_i<11:9>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <raddr_i<11:9>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
    Summary:
	no macro.
Unit <pcie_bram_s6> synthesized.

Synthesizing Unit <GTPA1_DUAL_WRAPPER>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/source/gtpa1_dual_wrapper.v".
        WRAPPER_SIM_GTPRESET_SPEEDUP = 1
        WRAPPER_CLK25_DIVIDER_0 = 4
        WRAPPER_CLK25_DIVIDER_1 = 4
        WRAPPER_PLL_DIVSEL_FB_0 = 5
        WRAPPER_PLL_DIVSEL_FB_1 = 5
        WRAPPER_PLL_DIVSEL_REF_0 = 2
        WRAPPER_PLL_DIVSEL_REF_1 = 2
        WRAPPER_SIMULATION = 0
    Summary:
	no macro.
Unit <GTPA1_DUAL_WRAPPER> synthesized.

Synthesizing Unit <GTPA1_DUAL_WRAPPER_TILE>.
    Related source file is "/project/exp6t_pcie3f/coregen/eptest/source/gtpa1_dual_wrapper_tile.v".
        TILE_SIM_GTPRESET_SPEEDUP = 1
        TILE_CLK25_DIVIDER_0 = 4
        TILE_CLK25_DIVIDER_1 = 4
        TILE_PLL_DIVSEL_FB_0 = 5
        TILE_PLL_DIVSEL_FB_1 = 5
        TILE_PLL_DIVSEL_REF_0 = 2
        TILE_PLL_DIVSEL_REF_1 = 2
        TILE_PLL_SOURCE_0 = "PLL0"
        TILE_PLL_SOURCE_1 = "PLL1"
    Summary:
	no macro.
Unit <GTPA1_DUAL_WRAPPER_TILE> synthesized.

Synthesizing Unit <xil_dvi>.
    Related source file is "/project/exp6t_pcie3f/lynx/xil_dvi.v".
        DVI_TX0 = 0
        DVI_TX1 = 0
        DVI_TX2 = 0
        DVI_TXC = 0
    Found 1-bit register for signal <ch_de_r>.
    Found 8-bit register for signal <ch1_in_r>.
    Found 8-bit register for signal <ch2_in_r>.
    Found 10-bit register for signal <ch1_enc_r>.
    Found 10-bit register for signal <ch2_enc_r>.
    Found 10-bit register for signal <ch0_in_r>.
    Found 10-bit register for signal <tx0_r>.
    Found 10-bit register for signal <tx1_r>.
    Found 10-bit register for signal <tx2_r>.
    Found 10-bit register for signal <tx3_r>.
    Found 10-bit register for signal <ch0_enc_r>.
    Found 4-bit register for signal <tx_req_r>.
    Found 2-bit register for signal <tx0_out_r>.
    Found 2-bit register for signal <tx1_out_r>.
    Found 2-bit register for signal <tx2_out_r>.
    Found 2-bit register for signal <tx3_out_r>.
    WARNING:Xst:2404 -  FFs/Latches <ch1_in_r<9:8>> (without init value) have a constant value of 0 in block <xil_dvi>.
    WARNING:Xst:2404 -  FFs/Latches <ch2_in_r<9:8>> (without init value) have a constant value of 0 in block <xil_dvi>.
    Summary:
	inferred 109 D-type flip-flop(s).
	inferred   4 Multiplexer(s).
Unit <xil_dvi> synthesized.

Synthesizing Unit <dvi_data_enc>.
    Related source file is "/project/exp6t_pcie3f/lynx/dvi_data_enc.v".
    Found 10-bit register for signal <st0_qm_r>.
    Found 10-bit register for signal <st1_qm_r>.
    Found 8-bit register for signal <st1_cnt_r>.
    Found 1-bit register for signal <st0_abort_r>.
    Found 8-bit subtractor for signal <n0387>.
    Found 8-bit subtractor for signal <st1_cnt_r[7]_GND_82_o_sub_218_OUT>.
    Found 4-bit adder for signal <st0_cnt1> created at line 119.
    Found 4-bit adder for signal <st1_cnt1> created at line 207.
    Found 8-bit adder for signal <st1_cnt_r[7]_GND_82_o_add_199_OUT> created at line 231.
    Found 8-bit adder for signal <st1_cnt_r[7]_GND_82_o_add_216_OUT> created at line 234.
    Found 8-bit subtractor for signal <_n0421>.
    Found 8-bit adder for signal <st1_cnt_r[7]_GND_82_o_add_224_OUT> created at line 235.
    Found 8-bit subtractor for signal <_n0423>.
    Found 8-bit adder for signal <st1_cnt_r[7]_GND_82_o_add_231_OUT> created at line 236.
    Found 8-bit subtractor for signal <_n0425>.
    Found 8-bit adder for signal <st1_cnt_r[7]_GND_82_o_sub_212_OUT> created at line 233.
    Found 16x4-bit Read Only RAM for signal <st1_cnt1_hi>
    Found 16x4-bit Read Only RAM for signal <st1_cnt1_low>
    Summary:
	inferred   2 RAM(s).
	inferred  12 Adder/Subtractor(s).
	inferred  29 D-type flip-flop(s).
	inferred  20 Multiplexer(s).
Unit <dvi_data_enc> synthesized.

Synthesizing Unit <xt_crtc>.
    Related source file is "/project/exp6t_pcie3f/xt_crtc.v".
        init_mode = 32'b00000000000000000000000000000000
        init_addr = 32'b00000000000000000000000000000000
        init_hdisp = 32'b00000000000000000000001111111111
        init_hsync = 32'b00000000000000000000010000100111
        init_hbp = 32'b00000000000000000000010010010111
        init_htotal = 32'b00000000000000000000010100101111
        init_vdisp = 32'b00000000000000000000001011111111
        init_vsync = 32'b00000000000000000000001100000010
        init_vbp = 32'b00000000000000000000001100000110
        init_vtotal = 32'b00000000000000000000001100011101
WARNING:Xst:647 - Input <mig_rd_count<6:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_cmd_full> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_rd_overflow> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_rd_error> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
    Found 16-bit register for signal <crtc_reg00_r>.
    Found 16-bit register for signal <crtc_reg05_r>.
    Found 16-bit register for signal <crtc_reg02_r>.
    Found 16-bit register for signal <crtc_reg01_r>.
    Found 16-bit register for signal <crtc_reg04_r>.
    Found 16-bit register for signal <crtc_reg03_r>.
    Found 16-bit register for signal <crtc_reg07_r>.
    Found 16-bit register for signal <crtc_reg06_r>.
    Found 1-bit register for signal <crtc_vblank_r>.
    Found 1-bit register for signal <mem_init_done_r>.
    Found 32-bit register for signal <io_wdata_r>.
    Found 32-bit register for signal <crtc_reg10_r>.
    Found 32-bit register for signal <crtc_reg11_r>.
    Found 32-bit register for signal <crtc_data_dl1_r>.
    Found 32-bit register for signal <crtc_data_dl2_r>.
    Found 32-bit register for signal <mem_cmd_addr_r>.
    Found 4-bit register for signal <io_be_r>.
    Found 12-bit register for signal <crtc_hcount_r<11:0>>.
    Found 12-bit register for signal <crtc_vcount_r<11:0>>.
    Found 12-bit register for signal <crtc_dcount_r<11:0>>.
    Found 12-bit register for signal <crtc_rd_addr_r>.
    Found 12-bit register for signal <crtc_rd_len_r>.
    Found 2-bit register for signal <crtc_rd_req_d_r>.
    Found 16-bit register for signal <crtc_rd_vpos_r>.
    Found 16-bit register for signal <fb_rd_addr_r>.
    Found 16-bit register for signal <fb_rd_len_r>.
    Found 16-bit register for signal <mem_rd_addr_r>.
    Found 3-bit register for signal <crtc_cclk_div_r<2:0>>.
    Found 3-bit register for signal <crtc_ctrl_dl0_r>.
    Found 3-bit register for signal <crtc_ctrl_dl1_r>.
    Found 3-bit register for signal <crtc_ctrl_dl2_r>.
    Found 3-bit register for signal <crtc_ctrl_dl3_r>.
    Found 3-bit register for signal <mem_state_r>.
    Found 24-bit register for signal <crtc_data_dl3_r<23:0>>.
    Found 8-bit register for signal <d_red_r>.
    Found 8-bit register for signal <d_grn_r>.
    Found 8-bit register for signal <d_blu_r>.
    Found 5-bit register for signal <fb_rd_req_r>.
    Found 7-bit register for signal <mem_rd_count8_r>.
    Found 1-bit register for signal <io_req_r>.
    Found 1-bit register for signal <io_wr_r>.
    Found 1-bit register for signal <io_ack_r>.
    Found 1-bit register for signal <crtc_hsync_r>.
    Found 1-bit register for signal <crtc_vsync_r>.
    Found 1-bit register for signal <crtc_de_r>.
    Found 1-bit register for signal <crtc_dhs_r>.
    Found 1-bit register for signal <crtc_dvs_r>.
    Found 1-bit register for signal <crtc_rd_reqf_r>.
    Found 1-bit register for signal <crtc_cclk_r>.
    Found 1-bit register for signal <d_de_r>.
    Found 1-bit register for signal <d_hsync_n_r>.
    Found 1-bit register for signal <d_vsync_n_r>.
    Found 1-bit register for signal <mem_cmd_req_r>.
    Found 1-bit register for signal <mem_cmd_addr_pre_r>.
    Found 1-bit register for signal <mem_cmd_addr_end_r>.
    Found 1-bit register for signal <mem_rd_req_r>.
    Found finite state machine <FSM_1> for signal <mem_state_r>.
    -----------------------------------------------------------------------
    | States             | 7                                              |
    | Transitions        | 14                                             |
    | Inputs             | 7                                              |
    | Outputs            | 7                                              |
    | Clock              | mig_clk (rising_edge)                          |
    | Reset              | rst_n (negative)                               |
    | Reset type         | asynchronous                                   |
    | Reset State        | 000                                            |
    | Encoding           | auto                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found 12-bit adder for signal <crtc_hcount_r[11]_GND_85_o_add_135_OUT> created at line 436.
    Found 12-bit adder for signal <crtc_vcount_r[11]_GND_85_o_add_142_OUT> created at line 440.
    Found 12-bit adder for signal <crtc_dcount_r[11]_GND_85_o_add_174_OUT> created at line 472.
    Found 3-bit adder for signal <crtc_cclk_div_r[2]_GND_85_o_add_209_OUT> created at line 558.
    Found 12-bit adder for signal <crtc_rd_addr_r[11]_GND_85_o_add_214_OUT> created at line 562.
    Found 13-bit adder for signal <n0761[12:0]> created at line 785.
    Found 7-bit adder for signal <mem_rd_count8_r[6]_GND_85_o_add_407_OUT> created at line 821.
    Found 16-bit adder for signal <mem_rd_addr_r[15]_GND_85_o_add_426_OUT> created at line 834.
    Found 12-bit comparator equal for signal <crtc_hsync_end> created at line 425
    Found 12-bit comparator equal for signal <crtc_hsync_sfp> created at line 426
    Found 12-bit comparator equal for signal <crtc_hsync_sync> created at line 427
    Found 12-bit comparator not equal for signal <crtc_hsync_sbp> created at line 428
    Found 12-bit comparator equal for signal <crtc_vsync_end> created at line 430
    Found 12-bit comparator equal for signal <crtc_vsync_sfp> created at line 431
    Found 12-bit comparator equal for signal <crtc_vsync_sync> created at line 432
    Found 12-bit comparator equal for signal <crtc_vsync_sbp> created at line 433
    Found 12-bit comparator equal for signal <crtc_dcount_r[11]_hpos_sfp[11]_equal_179_o> created at line 476
    Found 10-bit comparator equal for signal <mem_cmd_addr_r[11]_fb_rd_len[9]_equal_385_o> created at line 801
    WARNING:Xst:2404 -  FFs/Latches <io_addr_r<7:2>> (without init value) have a constant value of 0 in block <xt_crtc>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_rd_len_r<15:12>> (without init value) have a constant value of 0 in block <xt_crtc>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg00_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg05_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg02_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg01_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg04_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg03_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg07_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg06_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc>.
    Summary:
	inferred   8 Adder/Subtractor(s).
	inferred 547 D-type flip-flop(s).
	inferred  10 Comparator(s).
	inferred  83 Multiplexer(s).
	inferred   1 Finite State Machine(s).
Unit <xt_crtc> synthesized.

Synthesizing Unit <xt_crtc2>.
    Related source file is "/project/exp6t_pcie3f/xt_crtc2.v".
        init_mode = 32'b00000000000000000000000000000000
        init_addr = 32'b00000000010000000000000000000000
        init_hdisp = 32'b00000000000000000000001001111111
        init_hsync = 32'b00000000000000000000001010001111
        init_hbp = 32'b00000000000000000000001011101111
        init_htotal = 32'b00000000000000000000001100011111
        init_vdisp = 32'b00000000000000000000000111011111
        init_vsync = 32'b00000000000000000000000111101001
        init_vbp = 32'b00000000000000000000000111101011
        init_vtotal = 32'b00000000000000000000001000001100
WARNING:Xst:647 - Input <mig_rd_count<6:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_cmd_full> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_rd_overflow> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <mig_rd_error> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
    Found 16-bit register for signal <crtc_reg06_r>.
    Found 16-bit register for signal <crtc_reg05_r>.
    Found 16-bit register for signal <crtc_reg00_r>.
    Found 16-bit register for signal <crtc_reg04_r>.
    Found 16-bit register for signal <crtc_reg07_r>.
    Found 16-bit register for signal <crtc_reg02_r>.
    Found 16-bit register for signal <crtc_reg01_r>.
    Found 16-bit register for signal <crtc_reg03_r>.
    Found 1-bit register for signal <crtc_vblank_r>.
    Found 1-bit register for signal <mem_init_done_r>.
    Found 32-bit register for signal <io_wdata_r>.
    Found 32-bit register for signal <crtc_reg10_r>.
    Found 32-bit register for signal <crtc_data_dl1_r>.
    Found 32-bit register for signal <crtc_data_dl2_r>.
    Found 32-bit register for signal <crtc_data_dl3_r>.
    Found 32-bit register for signal <mem_cmd_addr_r>.
    Found 4-bit register for signal <io_be_r>.
    Found 4-bit register for signal <crtc_cclk_div_r>.
    Found 16-bit register for signal <crtc_hcount_r>.
    Found 16-bit register for signal <crtc_vcount_r>.
    Found 16-bit register for signal <crtc_dcount_r>.
    Found 16-bit register for signal <crtc_rd_vpos_r>.
    Found 16-bit register for signal <crtc_rd_len_r>.
    Found 16-bit register for signal <fb_rd_addr_r>.
    Found 16-bit register for signal <fb_rd_len_r>.
    Found 16-bit register for signal <mem_rd_addr_r>.
    Found 2-bit register for signal <crtc_rd_req_d_r>.
    Found 12-bit register for signal <crtc_rd_addr_r>.
    Found 3-bit register for signal <crtc_ctrl_dl0_r>.
    Found 3-bit register for signal <crtc_ctrl_dl1_r>.
    Found 3-bit register for signal <crtc_ctrl_dl2_r>.
    Found 3-bit register for signal <crtc_ctrl_dl3_r>.
    Found 3-bit register for signal <mem_state_r>.
    Found 8-bit register for signal <d_red_r>.
    Found 8-bit register for signal <d_grn_r>.
    Found 8-bit register for signal <d_blu_r>.
    Found 5-bit register for signal <fb_rd_req_r>.
    Found 7-bit register for signal <mem_rd_count8_r>.
    Found 32-bit register for signal <crtc_reg11_r>.
    Found 1-bit register for signal <io_req_r>.
    Found 1-bit register for signal <io_wr_r>.
    Found 1-bit register for signal <io_ack_r>.
    Found 1-bit register for signal <crtc_hsync_r>.
    Found 1-bit register for signal <crtc_vsync_r>.
    Found 1-bit register for signal <crtc_de_r>.
    Found 1-bit register for signal <crtc_dhs_r>.
    Found 1-bit register for signal <crtc_dvs_r>.
    Found 1-bit register for signal <crtc_rd_reqf_r>.
    Found 1-bit register for signal <crtc_cclk_r>.
    Found 1-bit register for signal <d_de_r>.
    Found 1-bit register for signal <d_hsync_n_r>.
    Found 1-bit register for signal <d_vsync_n_r>.
    Found 1-bit register for signal <mem_cmd_req_r>.
    Found 1-bit register for signal <mem_cmd_addr_pre_r>.
    Found 1-bit register for signal <mem_cmd_addr_end_r>.
    Found 1-bit register for signal <mem_rd_req_r>.
    Found finite state machine <FSM_3> for signal <mem_state_r>.
    -----------------------------------------------------------------------
    | States             | 7                                              |
    | Transitions        | 14                                             |
    | Inputs             | 7                                              |
    | Outputs            | 7                                              |
    | Clock              | mig_clk (rising_edge)                          |
    | Reset              | rst_n (negative)                               |
    | Reset type         | asynchronous                                   |
    | Reset State        | 000                                            |
    | Encoding           | auto                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found 12-bit adder for signal <crtc_hcount_r[11]_GND_87_o_add_155_OUT> created at line 438.
    Found 12-bit adder for signal <crtc_vcount_r[11]_GND_87_o_add_162_OUT> created at line 442.
    Found 12-bit adder for signal <crtc_dcount_r[11]_GND_87_o_add_194_OUT> created at line 474.
    Found 3-bit adder for signal <crtc_cclk_div_r[2]_GND_87_o_add_248_OUT> created at line 560.
    Found 12-bit adder for signal <crtc_rd_addr_r[11]_GND_87_o_add_253_OUT> created at line 564.
    Found 13-bit adder for signal <n0816[12:0]> created at line 787.
    Found 7-bit adder for signal <mem_rd_count8_r[6]_GND_87_o_add_455_OUT> created at line 823.
    Found 16-bit adder for signal <mem_rd_addr_r[15]_GND_87_o_add_474_OUT> created at line 836.
    Found 12-bit comparator equal for signal <crtc_hsync_end> created at line 427
    Found 12-bit comparator equal for signal <crtc_hsync_sfp> created at line 428
    Found 12-bit comparator equal for signal <crtc_hsync_sync> created at line 429
    Found 12-bit comparator not equal for signal <crtc_hsync_sbp> created at line 430
    Found 12-bit comparator equal for signal <crtc_vsync_end> created at line 432
    Found 12-bit comparator equal for signal <crtc_vsync_sfp> created at line 433
    Found 12-bit comparator equal for signal <crtc_vsync_sync> created at line 434
    Found 12-bit comparator equal for signal <crtc_vsync_sbp> created at line 435
    Found 12-bit comparator equal for signal <crtc_dcount_r[11]_hpos_sfp[11]_equal_199_o> created at line 478
    Found 10-bit comparator equal for signal <mem_cmd_addr_r[11]_fb_rd_len[9]_equal_433_o> created at line 803
    WARNING:Xst:2404 -  FFs/Latches <io_addr_r<7:2>> (without init value) have a constant value of 0 in block <xt_crtc2>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg06_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc2>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg05_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc2>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg00_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc2>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg04_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc2>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg07_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc2>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg02_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc2>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg01_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc2>.
    WARNING:Xst:2404 -  FFs/Latches <crtc_reg03_r<31:16>> (without init value) have a constant value of 0 in block <xt_crtc2>.
    Summary:
	inferred   8 Adder/Subtractor(s).
	inferred 572 D-type flip-flop(s).
	inferred  10 Comparator(s).
	inferred  84 Multiplexer(s).
	inferred   1 Finite State Machine(s).
Unit <xt_crtc2> synthesized.

Synthesizing Unit <dp_main_640x480>.
    Related source file is "/project/exp6t_pcie3f/lynx/dp_main_640x480.v".
        dp_mvid = 24'b000000000001010101010100
        dp_nvid = 24'b000000001000000000000000
        dp_maud = 8'b00000000
        dp_htotal = 16'b0000001100100000
        dp_vtotal = 16'b0000001000001101
        dp_hstart = 16'b0000000010010000
        dp_vstart = 16'b0000000000100011
        dp_hwidth = 16'b0000001010000000
        dp_vheight = 16'b0000000111100000
        dp_hsync = 16'b0000000001100000
        dp_vsync = 16'b0000000000000010
        dp_misc0 = 8'b00100000
        dp_misc1 = 8'b00000000
        dp_link = 1
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 173: Output port <link_unit> of the instance <dp_main_linkup> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 173: Output port <link_aux_cmd> of the instance <dp_main_linkup> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 173: Output port <link_timeout> of the instance <dp_main_linkup> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 173: Output port <link_aux_cmd_req> of the instance <dp_main_linkup> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 173: Output port <link_aux_cmd_done> of the instance <dp_main_linkup> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 173: Output port <link_aux_stat_irq1> of the instance <dp_main_linkup> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 291: Output port <aux_select> of the instance <aux_tx> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 291: Output port <aux_data_req> of the instance <aux_tx> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 308: Output port <aux_sync> of the instance <aux_rx> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 308: Output port <aux_stop> of the instance <aux_rx> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 331: Output port <TX_RED> of the instance <dp_main_crtc> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 331: Output port <TX_GRN> of the instance <dp_main_crtc> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 331: Output port <TX_BLU> of the instance <dp_main_crtc> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 331: Output port <tbc_data0> of the instance <dp_main_crtc> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 331: Output port <tbc_data1> of the instance <dp_main_crtc> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 331: Output port <tbc_data2> of the instance <dp_main_crtc> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 331: Output port <tbc_data3> of the instance <dp_main_crtc> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 569: Output port <sc_enc0> of the instance <dp_main_scramble> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 569: Output port <sc_enc1> of the instance <dp_main_scramble> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 569: Output port <sc_enc2> of the instance <dp_main_scramble> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 569: Output port <sc_enc3> of the instance <dp_main_scramble> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 569: Output port <sc_raw0> of the instance <dp_main_scramble> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 569: Output port <sc_raw1> of the instance <dp_main_scramble> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 569: Output port <sc_raw2> of the instance <dp_main_scramble> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/lynx/dp_main_640x480.v" line 569: Output port <sc_raw3> of the instance <dp_main_scramble> is unconnected or connected to loadless signal.
    Summary:
	no macro.
Unit <dp_main_640x480> synthesized.

Synthesizing Unit <dp_main_linkup1>.
    Related source file is "/project/exp6t_pcie3f/lynx/dp_main_linkup1.v".
        link_aux_cmd_init_wr = 4'b1000
        link_aux_cmd_idle_wr = 4'b1001
        link_aux_cmd_tr1_wr = 4'b1010
        link_aux_stat_tr1_rd = 4'b1011
        link_aux_cmd_tr2_wr = 4'b1100
        link_aux_stat_tr2_rd = 4'b1101
        link_aux_cmd_rsv1 = 4'b1110
        link_aux_cmd_rsv2 = 4'b1111
WARNING:Xst:647 - Input <link_aux_rx_data<2:3>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <link_aux_rx_data<6:7>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
    Found 12-bit register for signal <link_wait100us_count_r>.
    Found 5-bit register for signal <link_state_r>.
    Found 8-bit register for signal <link_wait400us_r>.
    Found 8-bit register for signal <aux_cmd_ack_r>.
    Found 8-bit register for signal <aux_wait_r>.
    Found 8-bit register for signal <aux_stat_irq_r>.
    Found 8-bit register for signal <aux_unit_r>.
    Found 8-bit register for signal <hpd_r>.
    Found 4-bit register for signal <link_main_mode_r>.
    Found 4-bit register for signal <link_aux_cmd_req_r>.
    Found 4-bit register for signal <aux_wait100us_r>.
    Found 4-bit register for signal <aux_stat_tr1_r<3:0>>.
    Found 4-bit register for signal <aux_stat_tr2_r<3:0>>.
    Found 3-bit register for signal <aux_state_r>.
    Found 3-bit register for signal <aux_retry_r>.
    Found 36-bit register for signal <aux_cmd_code_r>.
    Found 6-bit register for signal <aux_cmd_code_addr_r>.
    Found 1-bit register for signal <link_done_r>.
    Found 1-bit register for signal <link_err_r>.
    Found 1-bit register for signal <link_wait100us_r>.
    Found 1-bit register for signal <aux_wait2unit_r>.
    Found 1-bit register for signal <aux_timeout_r>.
    Found 1-bit register for signal <aux_tx_req_r>.
    Found 1-bit register for signal <aux_done_r>.
    Found 1-bit register for signal <aux_stat_algn_r>.
    Found finite state machine <FSM_6> for signal <aux_state_r>.
    -----------------------------------------------------------------------
    | States             | 8                                              |
    | Transitions        | 17                                             |
    | Inputs             | 8                                              |
    | Outputs            | 12                                             |
    | Clock              | clk27 (rising_edge)                            |
    | Reset              | rst_n (negative)                               |
    | Reset type         | asynchronous                                   |
    | Reset State        | 000                                            |
    | Encoding           | auto                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
INFO:Xst:1799 - State 00111 is never reached in FSM <link_state_r>.
    Found finite state machine <FSM_5> for signal <link_state_r>.
    -----------------------------------------------------------------------
    | States             | 16                                             |
    | Transitions        | 31                                             |
    | Inputs             | 9                                              |
    | Outputs            | 19                                             |
    | Clock              | clk27 (rising_edge)                            |
    | Reset              | rst_n (negative)                               |
    | Reset type         | asynchronous                                   |
    | Reset State        | 00000                                          |
    | Encoding           | auto                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found 12-bit adder for signal <link_wait100us_count_r[11]_GND_91_o_add_21_OUT> created at line 185.
    Found 4-bit adder for signal <hpd_r[3]_GND_91_o_add_44_OUT> created at line 204.
    Found 8-bit adder for signal <link_wait400us_r[7]_GND_91_o_add_213_OUT> created at line 275.
    Found 3-bit adder for signal <aux_cmd_code_addr_r[2]_GND_91_o_add_623_OUT> created at line 693.
    Found 8-bit adder for signal <aux_wait_r[7]_GND_91_o_add_652_OUT> created at line 708.
    Found 4-bit adder for signal <aux_wait100us_r[3]_GND_91_o_add_675_OUT> created at line 728.
    Found 3-bit adder for signal <aux_retry_r[2]_GND_91_o_add_694_OUT> created at line 737.
    Found 64x36-bit Read Only RAM for signal <aux_cmd_code>
    Summary:
	inferred   1 RAM(s).
	inferred   7 Adder/Subtractor(s).
	inferred 141 D-type flip-flop(s).
	inferred 155 Multiplexer(s).
	inferred   2 Finite State Machine(s).
Unit <dp_main_linkup1> synthesized.

Synthesizing Unit <dp_aux_tx>.
    Related source file is "/project/exp6t_pcie3f/lynx/dp_aux_tx.v".
    Found 20-bit register for signal <aux_addr_r>.
    Found 20-bit register for signal <aux_tx_data_r>.
    Found 20-bit register for signal <aux_select_r>.
    Found 5-bit register for signal <aux_clk_r>.
    Found 5-bit register for signal <aux_count_r>.
    Found 3-bit register for signal <aux_tx_out_r>.
    Found 4-bit register for signal <aux_state_r>.
    Found 4-bit register for signal <aux_cmd_r>.
    Found 8-bit register for signal <aux_len_r>.
    Found 1-bit register for signal <aux_clk_one_r>.
    Found 1-bit register for signal <aux_clk_edge_r>.
    Found 1-bit register for signal <aux_tx_oe_r>.
    Found 1-bit register for signal <aux_ack_r>.
    Found 1-bit register for signal <aux_done_r>.
    Found 1-bit register for signal <aux_data_req_r>.
    Found 1-bit register for signal <aux_sync_count10_r>.
    Found 1-bit register for signal <aux_sync4_r>.
    Found 1-bit register for signal <aux_cmd4_r>.
    Found 1-bit register for signal <aux_addr20_r>.
    Found 1-bit register for signal <aux_len8_r>.
    Found 1-bit register for signal <aux_data8_r>.
    Found 1-bit register for signal <aux_len0_r>.
    Found 1-bit register for signal <aux_stop4_r>.
INFO:Xst:1799 - State 1110 is never reached in FSM <aux_state_r>.
INFO:Xst:1799 - State 1000 is never reached in FSM <aux_state_r>.
INFO:Xst:1799 - State 1001 is never reached in FSM <aux_state_r>.
INFO:Xst:1799 - State 1010 is never reached in FSM <aux_state_r>.
INFO:Xst:1799 - State 1011 is never reached in FSM <aux_state_r>.
    Found finite state machine <FSM_9> for signal <aux_state_r>.
    -----------------------------------------------------------------------
    | States             | 16                                             |
    | Transitions        | 39                                             |
    | Inputs             | 13                                             |
    | Outputs            | 16                                             |
    | Clock              | clk27 (rising_edge)                            |
    | Reset              | rst_n (negative)                               |
    | Reset type         | asynchronous                                   |
    | Reset State        | 0000                                           |
    | Encoding           | auto                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found 8-bit subtractor for signal <aux_len_r[7]_GND_96_o_sub_725_OUT>.
    Found 5-bit adder for signal <aux_clk_r[4]_GND_96_o_add_40_OUT> created at line 198.
    Found 5-bit adder for signal <aux_count_r[4]_GND_96_o_add_638_OUT> created at line 432.
    Found 20-bit adder for signal <aux_select_r[19]_GND_96_o_add_809_OUT> created at line 490.
    Found 21-bit 3-to-1 multiplexer for signal <_n0881> created at line 204.
    Summary:
	inferred   4 Adder/Subtractor(s).
	inferred  99 D-type flip-flop(s).
	inferred 204 Multiplexer(s).
	inferred   1 Finite State Machine(s).
Unit <dp_aux_tx> synthesized.

Synthesizing Unit <dp_aux_rx>.
    Related source file is "/project/exp6t_pcie3f/lynx/dp_aux_rx.v".
    Found 6-bit register for signal <aux_clk_r>.
    Found 3-bit register for signal <aux_state_r>.
    Found 3-bit register for signal <aux_count_r>.
    Found 3-bit register for signal <aux_rx_in_r<2:0>>.
    Found 4-bit register for signal <aux_sync_count_r>.
    Found 4-bit register for signal <aux_sync_r>.
    Found 4-bit register for signal <aux_stop_r>.
    Found 8-bit register for signal <aux_cmd_r>.
    Found 8-bit register for signal <aux_data_r>.
    Found 1-bit register for signal <aux_rx_edge_r>.
    Found 1-bit register for signal <aux_rx_zero_r>.
    Found 1-bit register for signal <aux_clk8_r>.
    Found 1-bit register for signal <aux_sync_count10_r>.
    Found 1-bit register for signal <aux_sync4_r>.
    Found 1-bit register for signal <aux_sync_err_r>.
    Found 1-bit register for signal <aux_cmd8_r>.
    Found 1-bit register for signal <aux_data8_r>.
    Found 1-bit register for signal <aux_stop4_r>.
    Found 1-bit register for signal <aux_cmd_ack_r>.
    Found 1-bit register for signal <aux_data_ack_r>.
    Found 1-bit register for signal <aux_done_r>.
    Found finite state machine <FSM_11> for signal <fsmfake10>.
    -----------------------------------------------------------------------
    | States             | 5                                              |
    | Transitions        | 58                                             |
    | Inputs             | 12                                             |
    | Outputs            | 1                                              |
    | Clock              | clk27 (rising_edge)                            |
    | Reset              | rst_n (negative)                               |
    | Reset type         | asynchronous                                   |
    | Reset State        | 000                                            |
    | Encoding           | auto                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found finite state machine <FSM_10> for signal <aux_state_r>.
    -----------------------------------------------------------------------
    | States             | 5                                              |
    | Transitions        | 16                                             |
    | Inputs             | 8                                              |
    | Outputs            | 8                                              |
    | Clock              | clk27 (rising_edge)                            |
    | Reset              | rst_n (negative)                               |
    | Reset type         | asynchronous                                   |
    | Reset State        | 000                                            |
    | Encoding           | auto                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found 5-bit adder for signal <aux_clk_r[4]_GND_97_o_add_55_OUT> created at line 205.
    Found 4-bit adder for signal <aux_sync_count_r[3]_GND_97_o_add_130_OUT> created at line 232.
    Found 3-bit adder for signal <aux_count_r[2]_GND_97_o_add_174_OUT> created at line 268.
    Summary:
	inferred   3 Adder/Subtractor(s).
	inferred  52 D-type flip-flop(s).
	inferred  46 Multiplexer(s).
	inferred   2 Finite State Machine(s).
Unit <dp_aux_rx> synthesized.

Synthesizing Unit <dp_main_crtc1>.
    Related source file is "/project/exp6t_pcie3f/lynx/dp_main_crtc1.v".
        dp_vbid_vs = 8'b00010001
        dp_vbid_hs = 8'b00010000
        dp_vbid_idle = 8'b00010000
        K237 = 9'b111110111
        K277 = 9'b111111011
        K280 = 9'b100011100
        K281 = 9'b100111100
        K282 = 9'b101011100
        K283 = 9'b101111100
        K284 = 9'b110011100
        K285 = 9'b110111100
        K286 = 9'b111011100
        K287 = 9'b111111100
        K297 = 9'b111111101
        K307 = 9'b111111110
        D102 = 9'b001001010
        D116 = 9'b011001011
    Register <disp_reg_dclk_r_dummy_dummy_dummy_dummy_dummy> equivalent to <disp_reg_dclk_r> has been removed
    Register <disp_reg_dclk_r_dummy_dummy_dummy_dummy> equivalent to <disp_reg_dclk_r> has been removed
    Register <disp_reg_dclk_r_dummy_dummy_dummy> equivalent to <disp_reg_dclk_r> has been removed
    Register <disp_reg_dclk_r_dummy_dummy> equivalent to <disp_reg_dclk_r> has been removed
    Register <disp_reg_dclk_r_dummy> equivalent to <disp_reg_dclk_r> has been removed
    Found 1-bit register for signal <disp_dclk_sync_r>.
    Found 1-bit register for signal <disp_hsync_n_r>.
    Found 1-bit register for signal <disp_vsync_n_r>.
    Found 1-bit register for signal <disp_hblank_n_r>.
    Found 1-bit register for signal <disp_vblank_n_r>.
    Found 1-bit register for signal <disp_blank_n_r>.
    Found 1-bit register for signal <tbc_clr_r>.
    Found 1-bit register for signal <tbc_sync_ss_r>.
    Found 1-bit register for signal <tbc_count_sync_r>.
    Found 1-bit register for signal <tbc_de1_r>.
    Found 1-bit register for signal <disp_reg_dclk_r>.
    Found 15-bit register for signal <disp_dclk_r>.
    Found 12-bit register for signal <disp_reg_hcount_sbp_r<11:0>>.
    Found 12-bit register for signal <disp_reg_hcount_sav_r<11:0>>.
    Found 12-bit register for signal <disp_reg_hcount_eav_r<11:0>>.
    Found 12-bit register for signal <disp_reg_hcount_end_r<11:0>>.
    Found 12-bit register for signal <disp_reg_vcount_sbp_r<11:0>>.
    Found 12-bit register for signal <disp_reg_vcount_sav_r<11:0>>.
    Found 12-bit register for signal <disp_reg_vcount_eav_r<11:0>>.
    Found 12-bit register for signal <disp_reg_vcount_end_r<11:0>>.
    Found 12-bit register for signal <disp_vcount_r>.
    Found 5-bit register for signal <disp_htiming_r>.
    Found 4-bit register for signal <disp_vtiming_r>.
    Found 4-bit register for signal <tbc_sync_r>.
    Found 8-bit register for signal <tbc_count_r>.
    Found 576-bit register for signal <tbc_data0_out_r>.
    Found 12-bit register for signal <disp_hcount_r>.
    Found 24-bit adder for signal <n0384> created at line 241.
    Found 12-bit adder for signal <disp_hcount_r[11]_GND_98_o_add_36_OUT> created at line 276.
    Found 12-bit adder for signal <disp_vcount_r[11]_GND_98_o_add_39_OUT> created at line 277.
    Found 8-bit adder for signal <tbc_count_r[7]_GND_98_o_add_330_OUT> created at line 703.
    Found 12-bit comparator equal for signal <disp_hcount_r[11]_disp_reg_hcount_sbp_r[11]_equal_68_o> created at line 297
    Found 12-bit comparator equal for signal <disp_hcount_r[11]_disp_reg_hcount_sav_r[11]_equal_74_o> created at line 303
    Found 12-bit comparator equal for signal <disp_hcount_r[11]_disp_reg_hcount_eav_r[11]_equal_79_o> created at line 308
    Found 12-bit comparator equal for signal <disp_hcount_r[11]_disp_reg_hcount_end_r[11]_equal_84_o> created at line 315
    Found 12-bit comparator equal for signal <disp_vcount_r[11]_disp_reg_vcount_sbp_r[11]_equal_89_o> created at line 322
    Found 12-bit comparator equal for signal <disp_vcount_r[11]_disp_reg_vcount_sav_r[11]_equal_94_o> created at line 328
    Found 12-bit comparator equal for signal <disp_vcount_r[11]_disp_reg_vcount_eav_r[11]_equal_99_o> created at line 333
    Found 12-bit comparator equal for signal <disp_vcount_r[11]_disp_reg_vcount_end_r[11]_equal_104_o> created at line 340
    WARNING:Xst:2404 -  FFs/Latches <disp_reg_dclk_r<23:13>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
    WARNING:Xst:2404 -  FFs/Latches <disp_reg_dclk_r<11:11>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
    WARNING:Xst:2404 -  FFs/Latches <disp_reg_dclk_r<10:10>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
    WARNING:Xst:2404 -  FFs/Latches <disp_reg_dclk_r<9:9>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
    WARNING:Xst:2404 -  FFs/Latches <disp_reg_dclk_r<8:8>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
    WARNING:Xst:2404 -  FFs/Latches <disp_reg_dclk_r<7:7>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
    WARNING:Xst:2404 -  FFs/Latches <disp_reg_dclk_r<6:5>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
    WARNING:Xst:2404 -  FFs/Latches <tbc_data1_out_r<8:0>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
    WARNING:Xst:2404 -  FFs/Latches <tbc_data2_out_r<8:0>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
    WARNING:Xst:2404 -  FFs/Latches <tbc_data3_out_r<8:0>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
    WARNING:Xst:2404 -  FFs/Latches <disp_dclk_r<23:15>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
    Summary:
	inferred   4 Adder/Subtractor(s).
	inferred 743 D-type flip-flop(s).
	inferred   8 Comparator(s).
	inferred  59 Multiplexer(s).
Unit <dp_main_crtc1> synthesized.

Synthesizing Unit <dp_main_tbc1>.
    Related source file is "/project/exp6t_pcie3f/lynx/dp_main_tbc1.v".
        device = "XILINX"
WARNING:Xst:647 - Input <TX_VS> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
    Found 1-bit register for signal <tx_hs_in_r>.
    Found 1-bit register for signal <tx_de_in_r>.
    Found 1-bit register for signal <tx_hs_req_r>.
    Found 1-bit register for signal <tx_vs_req_r>.
    Found 1-bit register for signal <tx_de_req_r>.
    Found 1-bit register for signal <tx_ss_req_r>.
    Found 1-bit register for signal <tbc_line_end_r>.
    Found 1-bit register for signal <tbc_count11_r>.
    Found 1-bit register for signal <tbc_count64_r>.
    Found 1-bit register for signal <tbc_rd_end_r>.
    Found 1-bit register for signal <tbc_blank_end_r>.
    Found 1-bit register for signal <tbc_data_req_r>.
    Found 8-bit register for signal <tx_red_in_r>.
    Found 8-bit register for signal <tx_grn_in_r>.
    Found 8-bit register for signal <tx_blu_in_r>.
    Found 8-bit register for signal <tx_hs_in0_r>.
    Found 8-bit register for signal <tx_hs_in1_r>.
    Found 8-bit register for signal <tx_de_in0_r>.
    Found 8-bit register for signal <tx_de_in1_r>.
    Found 8-bit register for signal <tbc_count_r>.
    Found 8-bit register for signal <tbc_rd_count_r>.
    Found 24-bit register for signal <tx_data00_in_r>.
    Found 24-bit register for signal <tx_data01_in_r>.
    Found 24-bit register for signal <tx_data02_in_r>.
    Found 24-bit register for signal <tx_data03_in_r>.
    Found 12-bit register for signal <tx_data_count_r>.
    Found 12-bit register for signal <tbc_line_r>.
    Found 9-bit register for signal <tx_data_wr_r>.
    Found 2-bit register for signal <tx_ss_in_r>.
    Found 2-bit register for signal <tbc_data_sel_r<1:0>>.
    Found 2-bit register for signal <tbc_de_count_r>.
    Found 4-bit register for signal <tbc_state_r>.
    Found 108-bit register for signal <tbc_rd_data00_r>.
    Found 108-bit register for signal <tbc_rd_data01_r>.
    Found 108-bit register for signal <tbc_rd_data02_r>.
    Found 108-bit register for signal <tbc_rd_data03_r>.
    Found 288-bit register for signal <tbc_disp00_r>.
    Found 576-bit register for signal <tbc_data00_r>.
    Found 576-bit register for signal <tbc_data00_out_r>.
    Found finite state machine <FSM_12> for signal <tbc_state_r>.
    -----------------------------------------------------------------------
    | States             | 9                                              |
    | Transitions        | 21                                             |
    | Inputs             | 8                                              |
    | Outputs            | 14                                             |
    | Clock              | CLK (rising_edge)                              |
    | Reset              | SYSRST_N (negative)                            |
    | Reset type         | asynchronous                                   |
    | Reset State        | 0000                                           |
    | Encoding           | auto                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found 12-bit adder for signal <tx_data_count_r[11]_GND_100_o_add_54_OUT> created at line 311.
    Found 7-bit adder for signal <tx_hs_in0_r[6]_GND_100_o_add_79_OUT> created at line 325.
    Found 7-bit adder for signal <tx_hs_in1_r[6]_GND_100_o_add_98_OUT> created at line 336.
    Found 7-bit adder for signal <tx_de_in0_r[6]_GND_100_o_add_155_OUT> created at line 369.
    Found 7-bit adder for signal <tx_de_in1_r[6]_GND_100_o_add_174_OUT> created at line 380.
    Found 12-bit adder for signal <tbc_line_r[11]_GND_100_o_add_363_OUT> created at line 626.
    Found 8-bit adder for signal <tbc_count_r[7]_GND_100_o_add_419_OUT> created at line 657.
    Found 8-bit adder for signal <tbc_rd_count_r[7]_GND_100_o_add_508_OUT> created at line 696.
    Found 2-bit adder for signal <tbc_de_count_r[1]_GND_100_o_add_568_OUT> created at line 727.
    Summary:
	inferred   9 Adder/Subtractor(s).
	inferred 2095 D-type flip-flop(s).
	inferred 110 Multiplexer(s).
	inferred   1 Finite State Machine(s).
Unit <dp_main_tbc1> synthesized.

Synthesizing Unit <dp_main_scramble>.
    Related source file is "/project/exp6t_pcie3f/lynx/dp_main_scramble.v".
        K237 = 9'b111110111
        K277 = 9'b111111011
        K280 = 9'b100011100
        K281 = 9'b100111100
        K282 = 9'b101011100
        K283 = 9'b101111100
        K284 = 9'b110011100
        K285 = 9'b110111100
        K286 = 9'b111011100
        K287 = 9'b111111100
        K297 = 9'b111111101
        K307 = 9'b111111110
        D102 = 9'b001001010
        D116 = 9'b011001011
    Register <sc_data0_out_r_dummy_dummy_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data0_out_r_dummy_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data0_out_r_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data0_out_r_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data0_out_r> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data3_out_r_dummy_dummy_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data3_out_r_dummy_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data3_out_r_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data3_out_r_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data3_out_r> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data2_out_r_dummy_dummy_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data2_out_r_dummy_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data2_out_r_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data2_out_r_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data2_out_r> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data1_out_r_dummy_dummy_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data1_out_r_dummy_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data1_out_r_dummy_dummy> equivalent to <sc_data1_out_r> has been removed
    Register <sc_data1_out_r_dummy> equivalent to <sc_data1_out_r> has been removed
    Found 1-bit register for signal <sc_lfsr_reset0>.
    Found 1-bit register for signal <pack_data0_in_bs_r>.
    Found 1-bit register for signal <sc_no_8k_r>.
    Found 1-bit register for signal <sc_no_8k512_r>.
    Found 1-bit register for signal <sc_op_512_r>.
    Found 1-bit register for signal <dp_main_scr_r>.
    Found 16-bit register for signal <scr_lfsr_r>.
    Found 8-bit register for signal <scr_lfsr_out_r>.
    Found 11-bit register for signal <sc_data0_out0_r>.
    Found 11-bit register for signal <sc_data1_out0_r>.
    Found 11-bit register for signal <sc_data2_out0_r>.
    Found 11-bit register for signal <sc_data3_out0_r>.
    Found 11-bit register for signal <sc_data0_out1_r>.
    Found 11-bit register for signal <sc_data1_out1_r>.
    Found 11-bit register for signal <sc_data2_out1_r>.
    Found 11-bit register for signal <sc_data3_out1_r>.
    Found 11-bit register for signal <sc_data0_out2_r>.
    Found 11-bit register for signal <sc_data1_out2_r>.
    Found 11-bit register for signal <sc_data2_out2_r>.
    Found 11-bit register for signal <sc_data3_out2_r>.
    Found 11-bit register for signal <sc_data1_dl1_r>.
    Found 11-bit register for signal <sc_data2_dl1_r>.
    Found 11-bit register for signal <sc_data3_dl1_r>.
    Found 11-bit register for signal <sc_data2_dl2_r>.
    Found 11-bit register for signal <sc_data3_dl2_r>.
    Found 11-bit register for signal <sc_data3_dl3_r>.
    Found 11-bit register for signal <sc_tr_data_out_r>.
    Found 11-bit register for signal <sc_no_data_out_r>.
    Found 11-bit register for signal <sc_op_data0_out_r>.
    Found 11-bit register for signal <sc_op_data1_out_r>.
    Found 11-bit register for signal <sc_op_data2_out_r>.
    Found 11-bit register for signal <sc_op_data3_out_r>.
    Found 4-bit register for signal <sc_tr_count_r>.
    Found 9-bit register for signal <pack_data0_in_r>.
    Found 9-bit register for signal <pack_data1_in_r>.
    Found 9-bit register for signal <pack_data2_in_r>.
    Found 9-bit register for signal <pack_data3_in_r>.
    Found 9-bit register for signal <sc_no_count_8k_r>.
    Found 9-bit register for signal <sc_op_count_512_r>.
    Found 13-bit register for signal <sc_no_count_r>.
    Found 1-bit register for signal <sc_data1_out_r>.
    Found 4-bit adder for signal <sc_tr_count_r[3]_GND_102_o_add_188_OUT> created at line 421.
    Found 13-bit adder for signal <sc_no_count_w> created at line 476.
    Found 9-bit adder for signal <sc_no_count_8k_r[8]_GND_102_o_add_231_OUT> created at line 477.
    Found 9-bit adder for signal <sc_op_count_512_r[8]_GND_102_o_add_236_OUT> created at line 480.
    Found 32x22-bit Read Only RAM for signal <n0324>
    Found 4x18-bit Read Only RAM for signal <n0326>
    Found 22-bit 3-to-1 multiplexer for signal <n0302> created at line 331.
    Found 22-bit 3-to-1 multiplexer for signal <n0303> created at line 340.
    Found 22-bit 3-to-1 multiplexer for signal <n0304> created at line 347.
    Found 22-bit 3-to-1 multiplexer for signal <n0305> created at line 354.
    WARNING:Xst:2404 -  FFs/Latches <sc_data1_out_r<9:9>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data1_out_r<8:8>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data1_out_r<7:7>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data1_out_r<6:6>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data1_out_r<5:5>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data2_out_r<9:9>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data2_out_r<8:8>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data2_out_r<7:7>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data2_out_r<6:6>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data2_out_r<5:5>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data3_out_r<9:9>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data3_out_r<8:8>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data3_out_r<7:7>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data3_out_r<6:6>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data3_out_r<5:5>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data0_out_r<9:9>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data0_out_r<8:8>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data0_out_r<7:7>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data0_out_r<6:6>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    WARNING:Xst:2404 -  FFs/Latches <sc_data0_out_r<5:5>> (without init value) have a constant value of 0 in block <dp_main_scramble>.
    Summary:
	inferred   2 RAM(s).
	inferred   4 Adder/Subtractor(s).
	inferred 366 D-type flip-flop(s).
	inferred  17 Multiplexer(s).
Unit <dp_main_scramble> synthesized.

Synthesizing Unit <XIL_S6_GTPWIZARD_V1_6_DP>.
    Related source file is "/project/exp6t_pcie3f/xil_s6_gtpwizard_v1_6_dp.v".
        WRAPPER_SIM_GTPRESET_SPEEDUP = 0
        WRAPPER_CLK25_DIVIDER_0 = 6
        WRAPPER_CLK25_DIVIDER_1 = 6
        WRAPPER_PLL_DIVSEL_FB_0 = 2
        WRAPPER_PLL_DIVSEL_FB_1 = 2
        WRAPPER_PLL_DIVSEL_REF_0 = 1
        WRAPPER_PLL_DIVSEL_REF_1 = 1
        WRAPPER_SIMULATION = 0
    Summary:
	no macro.
Unit <XIL_S6_GTPWIZARD_V1_6_DP> synthesized.

Synthesizing Unit <XIL_S6_GTPWIZARD_V1_6_DP_TILE>.
    Related source file is "/project/exp6t_pcie3f/xil_s6_gtpwizard_v1_6_dp_tile.v".
        TILE_SIM_GTPRESET_SPEEDUP = 0
        TILE_CLK25_DIVIDER_0 = 6
        TILE_CLK25_DIVIDER_1 = 6
        TILE_PLL_DIVSEL_FB_0 = 2
        TILE_PLL_DIVSEL_FB_1 = 2
        TILE_PLL_DIVSEL_REF_0 = 1
        TILE_PLL_DIVSEL_REF_1 = 1
        TILE_PLL_SOURCE_0 = "PLL0"
        TILE_PLL_SOURCE_1 = "PLL1"
    Summary:
	no macro.
Unit <XIL_S6_GTPWIZARD_V1_6_DP_TILE> synthesized.

Synthesizing Unit <memc3_infrastructure>.
    Related source file is "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_infrastructure.v".
        C_MEMCLK_PERIOD = 5000
        C_RST_ACT_LOW = 1
        C_INPUT_CLK_TYPE = "SINGLE_ENDED"
        C_CLKOUT0_DIVIDE = 1
        C_CLKOUT1_DIVIDE = 1
        C_CLKOUT2_DIVIDE = 2
        C_CLKOUT3_DIVIDE = 8
        C_CLKFBOUT_MULT = 2
        C_DIVCLK_DIVIDE = 1
    Set property "syn_maxfan = 10" for signal <rst0_sync_r>.
    Set property "MAX_FANOUT = 10" for signal <rst0_sync_r>.
    Set property "KEEP = TRUE" for signal <sys_clk_ibufg>.
WARNING:Xst:647 - Input <sys_clk_p> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <sys_clk_n> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
    Found 1-bit register for signal <powerup_pll_locked>.
    Found 25-bit register for signal <rst0_sync_r>.
    Summary:
	inferred  26 D-type flip-flop(s).
Unit <memc3_infrastructure> synthesized.

Synthesizing Unit <memc3_wrapper>.
    Related source file is "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v".
        C_MEMCLK_PERIOD = 5000
        C_P0_MASK_SIZE = 4
        C_P0_DATA_PORT_SIZE = 32
        C_P1_MASK_SIZE = 4
        C_P1_DATA_PORT_SIZE = 32
        C_ARB_NUM_TIME_SLOTS = 12
        C_ARB_TIME_SLOT_0 = 18'b000001010011100101
        C_ARB_TIME_SLOT_1 = 18'b001010011100101000
        C_ARB_TIME_SLOT_2 = 18'b010011100101000001
        C_ARB_TIME_SLOT_3 = 18'b011100101000001010
        C_ARB_TIME_SLOT_4 = 18'b100101000001010011
        C_ARB_TIME_SLOT_5 = 18'b101000001010011100
        C_ARB_TIME_SLOT_6 = 18'b000001010011100101
        C_ARB_TIME_SLOT_7 = 18'b001010011100101000
        C_ARB_TIME_SLOT_8 = 18'b010011100101000001
        C_ARB_TIME_SLOT_9 = 18'b011100101000001010
        C_ARB_TIME_SLOT_10 = 18'b100101000001010011
        C_ARB_TIME_SLOT_11 = 18'b101000001010011100
        C_MEM_TRAS = 40000
        C_MEM_TRCD = 15000
        C_MEM_TREFI = 7800000
        C_MEM_TRFC = 105000
        C_MEM_TRP = 15000
        C_MEM_TWR = 15000
        C_MEM_TRTP = 7500
        C_MEM_TWTR = 7500
        C_MEM_ADDR_ORDER = "ROW_BANK_COLUMN"
        C_NUM_DQ_PINS = 16
        C_MEM_TYPE = "DDR2"
        C_MEM_DENSITY = "512Mb"
        C_MEM_BURST_LEN = 4
        C_MEM_CAS_LATENCY = 3
        C_MEM_ADDR_WIDTH = 13
        C_MEM_BANKADDR_WIDTH = 2
        C_MEM_NUM_COL_BITS = 10
        C_MEM_DDR1_2_ODS = "FULL"
        C_MEM_DDR2_RTT = "50OHMS"
        C_MEM_DDR2_DIFF_DQS_EN = "YES"
        C_MEM_DDR2_3_PA_SR = "FULL"
        C_MEM_DDR2_3_HIGH_TEMP_SR = "NORMAL"
        C_MEM_DDR3_CAS_LATENCY = 6
        C_MEM_DDR3_ODS = "DIV6"
        C_MEM_DDR3_RTT = "DIV2"
        C_MEM_DDR3_CAS_WR_LATENCY = 5
        C_MEM_DDR3_AUTO_SR = "ENABLED"
        C_MEM_DDR3_DYN_WRT_ODT = "OFF"
        C_MEM_MOBILE_PA_SR = "FULL"
        C_MEM_MDDR_ODS = "FULL"
        C_MC_CALIB_BYPASS = "NO"
        C_SIMULATION = "FALSE"
        C_LDQSP_TAP_DELAY_VAL = 0
        C_UDQSP_TAP_DELAY_VAL = 0
        C_LDQSN_TAP_DELAY_VAL = 0
        C_UDQSN_TAP_DELAY_VAL = 0
        C_DQ0_TAP_DELAY_VAL = 0
        C_DQ1_TAP_DELAY_VAL = 0
        C_DQ2_TAP_DELAY_VAL = 0
        C_DQ3_TAP_DELAY_VAL = 0
        C_DQ4_TAP_DELAY_VAL = 0
        C_DQ5_TAP_DELAY_VAL = 0
        C_DQ6_TAP_DELAY_VAL = 0
        C_DQ7_TAP_DELAY_VAL = 0
        C_DQ8_TAP_DELAY_VAL = 0
        C_DQ9_TAP_DELAY_VAL = 0
        C_DQ10_TAP_DELAY_VAL = 0
        C_DQ11_TAP_DELAY_VAL = 0
        C_DQ12_TAP_DELAY_VAL = 0
        C_DQ13_TAP_DELAY_VAL = 0
        C_DQ14_TAP_DELAY_VAL = 0
        C_DQ15_TAP_DELAY_VAL = 0
        C_MC_CALIBRATION_MODE = "CALIBRATION"
        C_MC_CALIBRATION_DELAY = "HALF"
        C_CALIB_SOFT_IP = "TRUE"
        C_SKIP_IN_TERM_CAL = 0
        C_SKIP_DYNAMIC_CAL = 0
WARNING:Xst:647 - Input <selfrefresh_enter> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p2_rd_data> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p2_rd_count> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p3_rd_data> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p3_rd_count> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p4_wr_count> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p5_wr_count> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <uo_data> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <status> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p2_rd_full> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p2_rd_empty> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p2_rd_overflow> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p2_rd_error> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p3_rd_full> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p3_rd_empty> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p3_rd_overflow> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p3_rd_error> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p4_wr_full> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p4_wr_empty> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p4_wr_underrun> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p4_wr_error> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p5_wr_full> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p5_wr_empty> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p5_wr_underrun> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <p5_wr_error> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <mcbx_dram_ddr3_rst> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <uo_data_valid> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <uo_cmd_ready_in> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <uo_refrsh_flag> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <uo_cal_start> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/memc3_wrapper.v" line 475: Output port <uo_sdo> of the instance <memc3_mcb_raw_wrapper_inst> is unconnected or connected to loadless signal.
    Summary:
	no macro.
Unit <memc3_wrapper> synthesized.

Synthesizing Unit <mcb_raw_wrapper>.
    Related source file is "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_raw_wrapper.v".
        C_MEMCLK_PERIOD = 5000
        C_PORT_ENABLE = 6'b111111
        C_MEM_ADDR_ORDER = "ROW_BANK_COLUMN"
        C_ARB_NUM_TIME_SLOTS = 12
        C_ARB_TIME_SLOT_0 = 18'b101100011010001000
        C_ARB_TIME_SLOT_1 = 18'b000101100011010001
        C_ARB_TIME_SLOT_2 = 18'b001000101100011010
        C_ARB_TIME_SLOT_3 = 18'b010001000101100011
        C_ARB_TIME_SLOT_4 = 18'b011010001000101100
        C_ARB_TIME_SLOT_5 = 18'b100011010001000101
        C_ARB_TIME_SLOT_6 = 18'b101100011010001000
        C_ARB_TIME_SLOT_7 = 18'b000101100011010001
        C_ARB_TIME_SLOT_8 = 18'b001000101100011010
        C_ARB_TIME_SLOT_9 = 18'b010001000101100011
        C_ARB_TIME_SLOT_10 = 18'b011010001000101100
        C_ARB_TIME_SLOT_11 = 18'b100011010001000101
        C_PORT_CONFIG = "B32_B32_W32_W32_R32_R32"
        C_MEM_TRAS = 40000
        C_MEM_TRCD = 15000
        C_MEM_TREFI = 7800000
        C_MEM_TRFC = 105000
        C_MEM_TRP = 15000
        C_MEM_TWR = 15000
        C_MEM_TRTP = 7500
        C_MEM_TWTR = 7500
        C_NUM_DQ_PINS = 16
        C_MEM_TYPE = "DDR2"
        C_MEM_DENSITY = "512Mb"
        C_MEM_BURST_LEN = 4
        C_MEM_CAS_LATENCY = 3
        C_MEM_ADDR_WIDTH = 13
        C_MEM_BANKADDR_WIDTH = 2
        C_MEM_NUM_COL_BITS = 10
        C_MEM_DDR3_CAS_LATENCY = 6
        C_MEM_MOBILE_PA_SR = "FULL"
        C_MEM_DDR1_2_ODS = "FULL"
        C_MEM_DDR3_ODS = "DIV6"
        C_MEM_DDR2_RTT = "50OHMS"
        C_MEM_DDR3_RTT = "DIV2"
        C_MEM_MDDR_ODS = "FULL"
        C_MEM_DDR2_DIFF_DQS_EN = "YES"
        C_MEM_DDR2_3_PA_SR = "FULL"
        C_MEM_DDR3_CAS_WR_LATENCY = 5
        C_MEM_DDR3_AUTO_SR = "ENABLED"
        C_MEM_DDR2_3_HIGH_TEMP_SR = "NORMAL"
        C_MEM_DDR3_DYN_WRT_ODT = "OFF"
        C_MEM_TZQINIT_MAXCNT = 10'b1000000000
        C_MC_CALIB_BYPASS = "NO"
        C_MC_CALIBRATION_RA = 16'b0000000000000000
        C_MC_CALIBRATION_BA = 4'b0000
        C_CALIB_SOFT_IP = "TRUE"
        C_SKIP_IN_TERM_CAL = 0
        C_SKIP_DYNAMIC_CAL = 0
        C_SKIP_DYN_IN_TERM = 1'b1
        C_SIMULATION = "FALSE"
        LDQSP_TAP_DELAY_VAL = 0
        UDQSP_TAP_DELAY_VAL = 0
        LDQSN_TAP_DELAY_VAL = 0
        UDQSN_TAP_DELAY_VAL = 0
        DQ0_TAP_DELAY_VAL = 0
        DQ1_TAP_DELAY_VAL = 0
        DQ2_TAP_DELAY_VAL = 0
        DQ3_TAP_DELAY_VAL = 0
        DQ4_TAP_DELAY_VAL = 0
        DQ5_TAP_DELAY_VAL = 0
        DQ6_TAP_DELAY_VAL = 0
        DQ7_TAP_DELAY_VAL = 0
        DQ8_TAP_DELAY_VAL = 0
        DQ9_TAP_DELAY_VAL = 0
        DQ10_TAP_DELAY_VAL = 0
        DQ11_TAP_DELAY_VAL = 0
        DQ12_TAP_DELAY_VAL = 0
        DQ13_TAP_DELAY_VAL = 0
        DQ14_TAP_DELAY_VAL = 0
        DQ15_TAP_DELAY_VAL = 0
        C_MC_CALIBRATION_CA = 12'b000000000000
        C_MC_CALIBRATION_CLK_DIV = 1
        C_MC_CALIBRATION_MODE = "CALIBRATION"
        C_MC_CALIBRATION_DELAY = "HALF"
        C_P0_MASK_SIZE = 4
        C_P0_DATA_PORT_SIZE = 32
        C_P1_MASK_SIZE = 4
        C_P1_DATA_PORT_SIZE = 32
    Set property "syn_maxfan = 1" for signal <int_sys_rst>.
    Set property "MAX_FANOUT = 1" for signal <int_sys_rst>.
WARNING:Xst:647 - Input <p0_cmd_byte_addr<29:26>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p0_cmd_byte_addr<0:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p1_cmd_byte_addr<29:26>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p1_cmd_byte_addr<0:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p2_cmd_byte_addr<29:26>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p2_cmd_byte_addr<0:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p3_cmd_byte_addr<29:26>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p3_cmd_byte_addr<0:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p4_cmd_byte_addr<29:26>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p4_cmd_byte_addr<0:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p4_wr_mask<3:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p4_wr_data<31:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p5_cmd_byte_addr<29:26>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p5_cmd_byte_addr<0:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p5_wr_mask<3:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p5_wr_data<31:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_addr<4:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_dqcount<3:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p2_rd_clk> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p2_rd_en> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p3_rd_clk> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p3_rd_en> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p4_wr_clk> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p4_wr_en> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p5_wr_clk> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <p5_wr_en> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <calib_recal> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_read> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_add> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_cs> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_sdi> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_broadcast> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_drp_update> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_done_cal> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_cmd> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_cmd_in> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_cmd_en> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_dq_lower_dec> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_dq_lower_inc> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_dq_upper_dec> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_dq_upper_inc> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_udqs_inc> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_udqs_dec> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_ldqs_inc> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <ui_ldqs_dec> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:653 - Signal <mcbx_dram_ddr3_rst> is used but never assigned. This sourceless signal will be automatically connected to value GND.
    Found 1-bit register for signal <syn_uiclk_pll_lock>.
    Summary:
	inferred   1 D-type flip-flop(s).
Unit <mcb_raw_wrapper> synthesized.

Synthesizing Unit <mcb_soft_calibration_top>.
    Related source file is "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration_top.v".
        C_MEM_TZQINIT_MAXCNT = 10'b1000000000
        C_MC_CALIBRATION_MODE = "CALIBRATION"
        SKIP_IN_TERM_CAL = 0
        SKIP_DYNAMIC_CAL = 0
        SKIP_DYN_IN_TERM = 1'b1
        C_SIMULATION = "FALSE"
        C_MEM_TYPE = "DDR2"
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration_top.v" line 169: Output port <Max_Value> of the instance <mcb_soft_calibration_inst> is unconnected or connected to loadless signal.
    Summary:
	no macro.
Unit <mcb_soft_calibration_top> synthesized.

Synthesizing Unit <mcb_soft_calibration>.
    Related source file is "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v".
        C_MEM_TZQINIT_MAXCNT = 10'b1000000000
        C_MC_CALIBRATION_MODE = "CALIBRATION"
        C_SIMULATION = "FALSE"
        SKIP_IN_TERM_CAL = 0
        SKIP_DYNAMIC_CAL = 0
        SKIP_DYN_IN_TERM = 1'b1
        C_MEM_TYPE = "DDR2"
WARNING:Xst:3149 - Value "1" of property "syn_preserve" is not applicable.
WARNING:Xst:3149 - Value "1" of property "syn_preserve" is not applicable.
WARNING:Xst:3149 - Value "1" of property "syn_preserve" is not applicable.
WARNING:Xst:3149 - Value "1" of property "syn_preserve" is not applicable.
WARNING:Xst:3149 - Value "1" of property "syn_preserve" is not applicable.
WARNING:Xst:3149 - Value "1" of property "syn_preserve" is not applicable.
    Set property "syn_maxfan = 1" for signal <Active_IODRP>.
    Set property "MAX_FANOUT = 1" for signal <Active_IODRP>.
WARNING:Xst:3149 - Value "1" of property "syn_preserve" is not applicable.
WARNING:Xst:3149 - Value "1" of property "syn_preserve" is not applicable.
    Set property "IOB = FALSE" for signal <DONE_SOFTANDHARD_CAL>.
    Set property "syn_maxfan = 5" for signal <Pre_SYSRST>.
    Set property "MAX_FANOUT = 5" for signal <Pre_SYSRST>.
WARNING:Xst:647 - Input <MCB_UODATA<7:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <MCB_UODATAVALID> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <MCB_UOCMDREADY> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <MCB_UO_CAL_START> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" line 388: Output port <DRP_BKST> of the instance <iodrp_controller> is unconnected or connected to loadless signal.
INFO:Xst:3010 - "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/mcb_soft_calibration.v" line 405: Output port <read_data> of the instance <iodrp_mcb_controller> is unconnected or connected to loadless signal.
WARNING:Xst:2935 - Signal 'MCB_UIDQLOWERDEC', unconnected in block 'mcb_soft_calibration', is tied to its initial value (0).
WARNING:Xst:2935 - Signal 'MCB_UIDQLOWERINC', unconnected in block 'mcb_soft_calibration', is tied to its initial value (0).
WARNING:Xst:2935 - Signal 'MCB_UIDQUPPERDEC', unconnected in block 'mcb_soft_calibration', is tied to its initial value (0).
WARNING:Xst:2935 - Signal 'MCB_UIDQUPPERINC', unconnected in block 'mcb_soft_calibration', is tied to its initial value (0).
WARNING:Xst:2935 - Signal 'MCB_RECAL', unconnected in block 'mcb_soft_calibration', is tied to its initial value (0).
    Register <MCB_UIUDQSINC> equivalent to <MCB_UILDQSINC> has been removed
    Register <MCB_UIUDQSDEC> equivalent to <MCB_UILDQSDEC> has been removed
    Found 1-bit register for signal <CKE_Train>.
    Found 1-bit register for signal <Block_Reset>.
    Found 16-bit register for signal <WAIT_200us_COUNTER>.
    Found 10-bit register for signal <RstCounter>.
    Found 1-bit register for signal <Rst_condition1>.
    Found 1-bit register for signal <Rst_condition2>.
    Found 1-bit register for signal <SELFREFRESH_MCB_MODE_R1>.
    Found 1-bit register for signal <SELFREFRESH_MCB_MODE_R2>.
    Found 1-bit register for signal <SELFREFRESH_MCB_MODE_R3>.
    Found 1-bit register for signal <PLL_LOCK_R1>.
    Found 1-bit register for signal <PLL_LOCK_R2>.
    Found 1-bit register for signal <SELFREFRESH_MCB_REQ>.
    Found 1-bit register for signal <WAIT_SELFREFRESH_EXIT_DQS_CAL>.
    Found 1-bit register for signal <PERFORM_START_DYN_CAL_AFTER_SELFREFRESH>.
    Found 1-bit register for signal <START_DYN_CAL_STATE_R1>.
    Found 1-bit register for signal <PERFORM_START_DYN_CAL_AFTER_SELFREFRESH_R1>.
    Found 1-bit register for signal <SELFREFRESH_MODE>.
    Found 6-bit register for signal <count>.
    Found 1-bit register for signal <MCB_CMD_VALID>.
    Found 5-bit register for signal <MCB_UIADDR>.
    Found 1-bit register for signal <MCB_UICMDEN>.
    Found 1-bit register for signal <MCB_UIDONECAL>.
    Found 1-bit register for signal <MCB_USE_BKST>.
    Found 1-bit register for signal <MCB_UIDRPUPDATE>.
    Found 1-bit register for signal <Pre_SYSRST>.
    Found 1-bit register for signal <IODRPCTRLR_CMD_VALID>.
    Found 8-bit register for signal <IODRPCTRLR_MEMCELL_ADDR>.
    Found 8-bit register for signal <IODRPCTRLR_WRITE_DATA>.
    Found 1-bit register for signal <IODRPCTRLR_R_WB>.
    Found 6-bit register for signal <P_Term>.
    Found 7-bit register for signal <N_Term>.
    Found 6-bit register for signal <P_Term_Prev>.
    Found 7-bit register for signal <N_Term_Prev>.
    Found 2-bit register for signal <Active_IODRP>.
    Found 1-bit register for signal <MCB_UILDQSINC>.
    Found 1-bit register for signal <MCB_UILDQSDEC>.
    Found 1-bit register for signal <counter_en>.
    Found 1-bit register for signal <First_Dyn_Cal_Done>.
    Found 8-bit register for signal <Max_Value>.
    Found 8-bit register for signal <Max_Value_Previous>.
    Found 6-bit register for signal <STATE>.
    Found 8-bit register for signal <DQS_DELAY>.
    Found 8-bit register for signal <DQS_DELAY_INITIAL>.
    Found 8-bit register for signal <TARGET_DQS_DELAY>.
    Found 1-bit register for signal <First_In_Term_Done>.
    Found 1-bit register for signal <MCB_UICMD>.
    Found 4-bit register for signal <MCB_UIDQCOUNT>.
    Found 8-bit register for signal <counter_inc>.
    Found 8-bit register for signal <counter_dec>.
    Found 1-bit register for signal <DONE_SOFTANDHARD_CAL>.
    Found 1-bit register for signal <RST_reg>.
INFO:Xst:1799 - State 101010 is never reached in FSM <STATE>.
    Found finite state machine <FSM_14> for signal <STATE>.
    -----------------------------------------------------------------------
    | States             | 43                                             |
    | Transitions        | 102                                            |
    | Inputs             | 25                                             |
    | Outputs            | 29                                             |
    | Clock              | UI_CLK (rising_edge)                           |
    | Reset              | RST_reg (positive)                             |
    | Reset type         | synchronous                                    |
    | Reset State        | 000000                                         |
    | Power Up State     | 000000                                         |
    | Encoding           | auto                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found 8-bit subtractor for signal <Max_Value_Delta_Up>.
    Found 8-bit subtractor for signal <Max_Value_Delta_Dn>.
    Found 8-bit subtractor for signal <DQS_DELAY[7]_GND_116_o_sub_173_OUT>.
    Found 16-bit adder for signal <WAIT_200us_COUNTER[15]_GND_116_o_add_12_OUT> created at line 455.
    Found 10-bit adder for signal <RstCounter[9]_GND_116_o_add_17_OUT> created at line 519.
    Found 6-bit adder for signal <count[5]_GND_116_o_add_39_OUT> created at line 646.
    Found 6-bit adder for signal <P_Term[5]_GND_116_o_add_54_OUT> created at line 809.
    Found 7-bit adder for signal <N_Term[6]_GND_116_o_add_67_OUT> created at line 859.
    Found 8-bit adder for signal <n0586[7:0]> created at line 437.
    Found 9-bit adder for signal <n0589[8:0]> created at line 437.
    Found 10-bit adder for signal <n0592[9:0]> created at line 437.
    Found 11-bit adder for signal <n0595[10:0]> created at line 437.
    Found 12-bit adder for signal <n0598[11:0]> created at line 437.
    Found 9-bit adder for signal <n0610[8:0]> created at line 437.
    Found 10-bit adder for signal <n0613[9:0]> created at line 437.
    Found 11-bit adder for signal <n0616[10:0]> created at line 437.
    Found 10-bit adder for signal <n0628> created at line 437.
    Found 8-bit adder for signal <counter_inc[7]_GND_116_o_add_155_OUT> created at line 1189.
    Found 8-bit adder for signal <DQS_DELAY[7]_GND_116_o_add_158_OUT> created at line 1194.
    Found 8-bit adder for signal <counter_dec[7]_GND_116_o_add_169_OUT> created at line 1214.
    Found 13-bit adder for signal <_n0705> created at line 437.
    Found 13-bit adder for signal <n0414> created at line 437.
    Found 12-bit adder for signal <_n0715> created at line 437.
    Found 12-bit adder for signal <n0420> created at line 437.
    Found 1-bit 3-to-1 multiplexer for signal <IODRP_SDO> created at line 666.
    Found 10-bit comparator greater for signal <RstCounter[9]_PWR_61_o_LessThan_17_o> created at line 517
    Found 10-bit comparator greater for signal <RstCounter[9]_GND_116_o_LessThan_26_o> created at line 536
    Found 8-bit comparator greater for signal <Dec_Flag> created at line 634
    Found 8-bit comparator greater for signal <Inc_Flag> created at line 635
    Found 6-bit comparator equal for signal <n0132> created at line 871
    Found 7-bit comparator equal for signal <n0141> created at line 904
    Found 6-bit comparator greater for signal <count[5]_PWR_61_o_LessThan_133_o> created at line 1131
    Found 8-bit comparator greater for signal <Max_Value[7]_Max_Value_Previous[7]_LessThan_139_o> created at line 1163
    Found 8-bit comparator greater for signal <n0204> created at line 1163
    Found 8-bit comparator greater for signal <Max_Value_Previous[7]_Max_Value[7]_LessThan_143_o> created at line 1168
    Found 8-bit comparator greater for signal <n0208> created at line 1168
    Found 8-bit comparator greater for signal <DQS_DELAY[7]_DQS_DELAY_UPPER_LIMIT[7]_LessThan_157_o> created at line 1191
    Found 8-bit comparator lessequal for signal <n0222> created at line 1191
    Found 8-bit comparator greater for signal <DQS_DELAY_LOWER_LIMIT[7]_DQS_DELAY[7]_LessThan_171_o> created at line 1216
    Found 8-bit comparator lessequal for signal <n0240> created at line 1216
INFO:Xst:2840 - Register <SELFREFRESH_REQ_R1<0:0>> in unit <mcb_soft_calibration> has a constant value of 0 during circuit operation. The register is replaced by logic.
    WARNING:Xst:2404 -  FFs/Latches <SELFREFRESH_REQ_R2<0:0>> (without init value) have a constant value of 0 in block <mcb_soft_calibration>.
    WARNING:Xst:2404 -  FFs/Latches <SELFREFRESH_REQ_R3<0:0>> (without init value) have a constant value of 0 in block <mcb_soft_calibration>.
    WARNING:Xst:2404 -  FFs/Latches <MCB_UICMDIN<0:0>> (without init value) have a constant value of 0 in block <mcb_soft_calibration>.
    Summary:
	inferred  23 Adder/Subtractor(s).
	inferred 171 D-type flip-flop(s).
	inferred  15 Comparator(s).
	inferred  43 Multiplexer(s).
	inferred   1 Finite State Machine(s).
Unit <mcb_soft_calibration> synthesized.

Synthesizing Unit <iodrp_controller>.
    Related source file is "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/iodrp_controller.v".
    Set property "FSM_ENCODING = one-hot" for signal <state>.
    Set property "FSM_ENCODING = one-hot" for signal <nextstate>.
    Found 8-bit register for signal <data_reg>.
    Found 1-bit register for signal <rd_not_write_reg>.
    Found 8-bit register for signal <shift_through_reg>.
    Found 3-bit register for signal <bit_cnt>.
    Found 8-bit register for signal <read_data>.
    Found 1-bit register for signal <AddressPhase>.
    Found 1-bit register for signal <DRP_ADD>.
    Found 1-bit register for signal <DRP_CS>.
    Found 1-bit register for signal <DRP_BKST>.
    Found 3-bit register for signal <state>.
    Found 8-bit register for signal <memcell_addr_reg>.
    Found finite state machine <FSM_15> for signal <state>.
    -----------------------------------------------------------------------
    | States             | 8                                              |
    | Transitions        | 13                                             |
    | Inputs             | 4                                              |
    | Outputs            | 8                                              |
    | Clock              | DRP_CLK (rising_edge)                          |
    | Reset              | sync_rst (positive)                            |
    | Reset type         | synchronous                                    |
    | Reset State        | 000                                            |
    | Encoding           | one-hot                                        |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found 3-bit adder for signal <bit_cnt[2]_GND_117_o_add_15_OUT> created at line 186.
    Summary:
	inferred   1 Adder/Subtractor(s).
	inferred  40 D-type flip-flop(s).
	inferred   3 Multiplexer(s).
	inferred   1 Finite State Machine(s).
Unit <iodrp_controller> synthesized.

Synthesizing Unit <iodrp_mcb_controller>.
    Related source file is "/project/exp6t_pcie3f/coregen/xil_mig_v3_5_ddr2/user_design/rtl/iodrp_mcb_controller.v".
    Set property "FSM_ENCODING = GRAY" for signal <state>.
    Set property "FSM_ENCODING = GRAY" for signal <nextstate>.
WARNING:Xst:647 - Input <drp_ioi_addr<4:0>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
    Found 8-bit register for signal <data_reg>.
    Found 1-bit register for signal <rd_not_write_reg>.
    Found 8-bit register for signal <shift_through_reg<7:0>>.
    Found 3-bit register for signal <bit_cnt>.
    Found 8-bit register for signal <read_data>.
    Found 1-bit register for signal <AddressPhase>.
    Found 1-bit register for signal <DRP_ADD>.
    Found 1-bit register for signal <DRP_CS>.
    Found 1-bit register for signal <MCB_UIREAD>.
    Found 1-bit register for signal <DRP_BKST>.
    Found 4-bit register for signal <state>.
    Found 8-bit register for signal <memcell_addr_reg>.
    Found finite state machine <FSM_16> for signal <state>.
    -----------------------------------------------------------------------
    | States             | 10                                             |
    | Transitions        | 15                                             |
    | Inputs             | 4                                              |
    | Outputs            | 9                                              |
    | Clock              | DRP_CLK (rising_edge)                          |
    | Reset              | sync_rst (positive)                            |
    | Reset type         | synchronous                                    |
    | Reset State        | 0000                                           |
    | Encoding           | GRAY                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found 3-bit adder for signal <bit_cnt[2]_GND_118_o_add_16_OUT> created at line 301.
    Summary:
	inferred   1 Adder/Subtractor(s).
	inferred  41 D-type flip-flop(s).
	inferred   5 Multiplexer(s).
	inferred   1 Finite State Machine(s).
Unit <iodrp_mcb_controller> synthesized.

=========================================================================
HDL Synthesis Report

Macro Statistics
# RAMs                                                 : 9
 16x4-bit single-port Read Only RAM                    : 6
 32x22-bit single-port Read Only RAM                   : 1
 4x18-bit single-port Read Only RAM                    : 1
 64x36-bit single-port Read Only RAM                   : 1
# Adders/Subtractors                                   : 124
 10-bit adder                                          : 5
 10-bit subtractor                                     : 5
 11-bit adder                                          : 2
 12-bit adder                                          : 22
 12-bit subtractor                                     : 1
 13-bit adder                                          : 5
 16-bit adder                                          : 4
 2-bit adder                                           : 3
 20-bit adder                                          : 1
 24-bit adder                                          : 1
 3-bit adder                                           : 7
 4-bit adder                                           : 10
 5-bit adder                                           : 3
 6-bit adder                                           : 2
 7-bit adder                                           : 7
 8-bit adder                                           : 23
 8-bit addsub                                          : 1
 8-bit subtractor                                      : 18
 9-bit adder                                           : 4
# Registers                                            : 473
 1-bit register                                        : 184
 10-bit register                                       : 22
 108-bit register                                      : 4
 11-bit register                                       : 24
 12-bit register                                       : 20
 13-bit register                                       : 1
 15-bit register                                       : 1
 16-bit register                                       : 31
 2-bit register                                        : 11
 20-bit register                                       : 3
 24-bit register                                       : 5
 25-bit register                                       : 1
 288-bit register                                      : 1
 3-bit register                                        : 21
 32-bit register                                       : 33
 36-bit register                                       : 1
 4-bit register                                        : 29
 5-bit register                                        : 9
 576-bit register                                      : 3
 6-bit register                                        : 6
 7-bit register                                        : 5
 8-bit register                                        : 51
 9-bit register                                        : 7
# Comparators                                          : 43
 10-bit comparator equal                               : 2
 10-bit comparator greater                             : 2
 12-bit comparator equal                               : 24
 12-bit comparator not equal                           : 2
 6-bit comparator equal                                : 1
 6-bit comparator greater                              : 1
 7-bit comparator equal                                : 1
 8-bit comparator greater                              : 8
 8-bit comparator lessequal                            : 2
# Multiplexers                                         : 1119
 1-bit 2-to-1 multiplexer                              : 263
 1-bit 3-to-1 multiplexer                              : 1
 10-bit 2-to-1 multiplexer                             : 94
 108-bit 2-to-1 multiplexer                            : 8
 11-bit 2-to-1 multiplexer                             : 4
 12-bit 2-to-1 multiplexer                             : 37
 16-bit 2-to-1 multiplexer                             : 14
 2-bit 2-to-1 multiplexer                              : 31
 20-bit 2-to-1 multiplexer                             : 66
 21-bit 2-to-1 multiplexer                             : 24
 21-bit 3-to-1 multiplexer                             : 1
 22-bit 3-to-1 multiplexer                             : 4
 3-bit 2-to-1 multiplexer                              : 63
 32-bit 2-to-1 multiplexer                             : 57
 36-bit 2-to-1 multiplexer                             : 43
 39-bit 2-to-1 multiplexer                             : 13
 4-bit 2-to-1 multiplexer                              : 72
 5-bit 2-to-1 multiplexer                              : 55
 6-bit 2-to-1 multiplexer                              : 9
 7-bit 2-to-1 multiplexer                              : 39
 8-bit 2-to-1 multiplexer                              : 218
 9-bit 2-to-1 multiplexer                              : 3
# FSMs                                                 : 12
# Xors                                                 : 56
 1-bit xor2                                            : 44
 1-bit xor3                                            : 2
 1-bit xor4                                            : 6
 8-bit xor2                                            : 4

=========================================================================

=========================================================================
*                       Advanced HDL Synthesis                          *
=========================================================================

Reading core <../xil_blk_mem_gen_v4_2_1024x32.ngc>.
Reading core <../xil_blk_mem_gen_v4_2_dp108x256.ngc>.
Loading core <xil_blk_mem_gen_v4_2_1024x32> for timing and area information for instance <rdbuff>.
Loading core <xil_blk_mem_gen_v4_2_dp108x256> for timing and area information for instance <ram00_dp108x256>.
Loading core <xil_blk_mem_gen_v4_2_1024x32> for timing and area information for instance <linebuf0>.
Loading core <xil_blk_mem_gen_v4_2_1024x32> for timing and area information for instance <linebuf0>.
INFO:Xst:2261 - The FF/Latch <mem_wait_full_r_0> in Unit <mem> is equivalent to the following FF/Latch, which will be removed : <mem_wait_empt_r_0> 
INFO:Xst:2261 - The FF/Latch <mem_wait_full_r_1> in Unit <mem> is equivalent to the following FF/Latch, which will be removed : <mem_wait_empt_r_1> 
INFO:Xst:2261 - The FF/Latch <IODRPCTRLR_MEMCELL_ADDR_2> in Unit <mcb_soft_calibration_inst> is equivalent to the following 3 FFs/Latches, which will be removed : <IODRPCTRLR_MEMCELL_ADDR_4> <IODRPCTRLR_MEMCELL_ADDR_5> <IODRPCTRLR_MEMCELL_ADDR_6> 
INFO:Xst:2261 - The FF/Latch <tbc_disp00_r_8> in Unit <dp_main_tbc> is equivalent to the following 279 FFs/Latches, which will be removed : <tbc_disp00_r_17> <tbc_disp00_r_26> <tbc_disp00_r_35> <tbc_disp00_r_44> <tbc_disp00_r_53> <tbc_disp00_r_62> <tbc_disp00_r_71> <tbc_disp00_r_80> <tbc_disp00_r_89> <tbc_disp00_r_98> <tbc_disp00_r_107> <tbc_disp00_r_116> <tbc_disp00_r_125> <tbc_disp00_r_134> <tbc_disp00_r_143> <tbc_disp00_r_152> <tbc_disp00_r_161> <tbc_disp00_r_170> <tbc_disp00_r_179> <tbc_disp00_r_188> <tbc_disp00_r_197> <tbc_disp00_r_206> <tbc_disp00_r_215> <tbc_disp00_r_224> <tbc_disp00_r_233> <tbc_disp00_r_242> <tbc_disp00_r_251> <tbc_disp00_r_260> <tbc_disp00_r_269> <tbc_disp00_r_278> <tbc_disp00_r_287> <tbc_data00_r_0> <tbc_data00_r_1> <tbc_data00_r_2> <tbc_data00_r_3> <tbc_data00_r_4> <tbc_data00_r_5> <tbc_data00_r_6> <tbc_data00_r_7> <tbc_data00_r_8> <tbc_data00_r_9> <tbc_data00_r_10> <tbc_data00_r_14> <tbc_data00_r_16> <tbc_data00_r_18> <tbc_data00_r_19> <tbc_data00_r_23> <tbc_data00_r_25>
   <tbc_data00_r_324> <tbc_data00_r_334> <tbc_data00_r_335> <tbc_data00_r_336> <tbc_data00_r_338> <tbc_data00_r_339> <tbc_data00_r_340> <tbc_data00_r_341> <tbc_data00_r_342> <tbc_data00_r_343> <tbc_data00_r_345> <tbc_data00_r_347> <tbc_data00_r_349> <tbc_data00_r_350> <tbc_data00_r_352> <tbc_data00_r_360> <tbc_data00_r_361> <tbc_data00_r_362> <tbc_data00_r_363> <tbc_data00_r_364> <tbc_data00_r_365> <tbc_data00_r_366> <tbc_data00_r_367> <tbc_data00_r_368> <tbc_data00_r_369> <tbc_data00_r_370> <tbc_data00_r_371> <tbc_data00_r_372> <tbc_data00_r_373> <tbc_data00_r_374> <tbc_data00_r_375> <tbc_data00_r_376> <tbc_data00_r_377> <tbc_data00_r_378> <tbc_data00_r_379> <tbc_data00_r_380> <tbc_data00_r_381> <tbc_data00_r_382> <tbc_data00_r_383> <tbc_data00_r_384> <tbc_data00_r_385> <tbc_data00_r_386> <tbc_data00_r_387> <tbc_data00_r_388> <tbc_data00_r_389> <tbc_data00_r_390> <tbc_data00_r_391> <tbc_data00_r_392> <tbc_data00_r_393> <tbc_data00_r_394> <tbc_data00_r_395> <tbc_data00_r_396> <tbc_data00_r_397>
   <tbc_data00_r_398> <tbc_data00_r_399> <tbc_data00_r_400> <tbc_data00_r_401> <tbc_data00_r_402> <tbc_data00_r_403> <tbc_data00_r_404> <tbc_data00_r_405> <tbc_data00_r_406> <tbc_data00_r_407> <tbc_data00_r_408> <tbc_data00_r_409> <tbc_data00_r_410> <tbc_data00_r_411> <tbc_data00_r_412> <tbc_data00_r_413> <tbc_data00_r_414> <tbc_data00_r_415> <tbc_data00_r_416> <tbc_data00_r_417> <tbc_data00_r_418> <tbc_data00_r_419> <tbc_data00_r_420> <tbc_data00_r_421> <tbc_data00_r_422> <tbc_data00_r_423> <tbc_data00_r_424> <tbc_data00_r_425> <tbc_data00_r_426> <tbc_data00_r_427> <tbc_data00_r_428> <tbc_data00_r_429> <tbc_data00_r_430> <tbc_data00_r_431> <tbc_data00_r_432> <tbc_data00_r_433> <tbc_data00_r_434> <tbc_data00_r_435> <tbc_data00_r_436> <tbc_data00_r_437> <tbc_data00_r_438> <tbc_data00_r_439> <tbc_data00_r_440> <tbc_data00_r_441> <tbc_data00_r_442> <tbc_data00_r_443> <tbc_data00_r_444> <tbc_data00_r_445> <tbc_data00_r_446> <tbc_data00_r_447> <tbc_data00_r_448> <tbc_data00_r_449> <tbc_data00_r_450>
   <tbc_data00_r_451> <tbc_data00_r_452> <tbc_data00_r_453> <tbc_data00_r_454> <tbc_data00_r_455> <tbc_data00_r_456> <tbc_data00_r_457> <tbc_data00_r_458> <tbc_data00_r_459> <tbc_data00_r_460> <tbc_data00_r_461> <tbc_data00_r_462> <tbc_data00_r_463> <tbc_data00_r_464> <tbc_data00_r_465> <tbc_data00_r_466> <tbc_data00_r_467> <tbc_data00_r_468> <tbc_data00_r_469> <tbc_data00_r_470> <tbc_data00_r_471> <tbc_data00_r_472> <tbc_data00_r_473> <tbc_data00_r_474> <tbc_data00_r_475> <tbc_data00_r_476> <tbc_data00_r_477> <tbc_data00_r_478> <tbc_data00_r_479> <tbc_data00_r_480> <tbc_data00_r_481> <tbc_data00_r_482> <tbc_data00_r_483> <tbc_data00_r_484> <tbc_data00_r_485> <tbc_data00_r_486> <tbc_data00_r_487> <tbc_data00_r_488> <tbc_data00_r_489> <tbc_data00_r_490> <tbc_data00_r_491> <tbc_data00_r_492> <tbc_data00_r_493> <tbc_data00_r_494> <tbc_data00_r_495> <tbc_data00_r_496> <tbc_data00_r_497> <tbc_data00_r_498> <tbc_data00_r_499> <tbc_data00_r_500> <tbc_data00_r_501> <tbc_data00_r_502> <tbc_data00_r_503>
   <tbc_data00_r_504> <tbc_data00_r_505> <tbc_data00_r_506> <tbc_data00_r_507> <tbc_data00_r_508> <tbc_data00_r_509> <tbc_data00_r_510> <tbc_data00_r_511> <tbc_data00_r_512> <tbc_data00_r_513> <tbc_data00_r_514> <tbc_data00_r_515> <tbc_data00_r_516> <tbc_data00_r_517> <tbc_data00_r_518> <tbc_data00_r_519> <tbc_data00_r_520> <tbc_data00_r_521> <tbc_data00_r_522> <tbc_data00_r_523> <tbc_data00_r_524> <tbc_data00_r_525> <tbc_data00_r_526> <tbc_data00_r_527> <tbc_data00_r_528> <tbc_data00_r_529> <tbc_data00_r_530> <tbc_data00_r_531> <tbc_data00_r_532> <tbc_data00_r_533> <tbc_data00_r_534> <tbc_data00_r_535> <tbc_data00_r_536> <tbc_data00_r_537> <tbc_data00_r_538> <tbc_data00_r_539> <tbc_data00_r_540> <tbc_data00_r_541> <tbc_data00_r_542> <tbc_data00_r_543> <tbc_data00_r_544> <tbc_data00_r_545> <tbc_data00_r_546> <tbc_data00_r_547> <tbc_data00_r_548> <tbc_data00_r_549> <tbc_data00_r_550> <tbc_data00_r_551> <tbc_data00_r_552> <tbc_data00_r_553> <tbc_data00_r_554> <tbc_data00_r_555> <tbc_data00_r_556>
   <tbc_data00_r_557> <tbc_data00_r_558> <tbc_data00_r_559> <tbc_data00_r_560> <tbc_data00_r_561> <tbc_data00_r_562> <tbc_data00_r_563> <tbc_data00_r_564> <tbc_data00_r_565> <tbc_data00_r_566> <tbc_data00_r_567> <tbc_data00_r_568> <tbc_data00_r_569> <tbc_data00_r_570> <tbc_data00_r_571> <tbc_data00_r_572> <tbc_data00_r_573> <tbc_data00_r_574> <tbc_data00_r_575>
INFO:Xst:2261 - The FF/Latch <tbc_data00_r_11> in Unit <dp_main_tbc> is equivalent to the following 17 FFs/Latches, which will be removed : <tbc_data00_r_12> <tbc_data00_r_13> <tbc_data00_r_15> <tbc_data00_r_17> <tbc_data00_r_20> <tbc_data00_r_21> <tbc_data00_r_22> <tbc_data00_r_24> <tbc_data00_r_26> <tbc_data00_r_351> <tbc_data00_r_353> <tbc_data00_r_354> <tbc_data00_r_355> <tbc_data00_r_356> <tbc_data00_r_357> <tbc_data00_r_358> <tbc_data00_r_359> 
INFO:Xst:2261 - The FF/Latch <mem_rd_count8_r_6> in Unit <crtc1> is equivalent to the following FF/Latch, which will be removed : <mem_rd_req_r> 
INFO:Xst:2261 - The FF/Latch <crtc_rd_vpos_r_12> in Unit <crtc1> is equivalent to the following 3 FFs/Latches, which will be removed : <crtc_rd_vpos_r_13> <crtc_rd_vpos_r_14> <crtc_rd_vpos_r_15> 
INFO:Xst:2261 - The FF/Latch <mem_rd_count8_r_6> in Unit <crtc2> is equivalent to the following FF/Latch, which will be removed : <mem_rd_req_r> 
INFO:Xst:2261 - The FF/Latch <crtc_rd_vpos_r_12> in Unit <crtc2> is equivalent to the following 3 FFs/Latches, which will be removed : <crtc_rd_vpos_r_13> <crtc_rd_vpos_r_14> <crtc_rd_vpos_r_15> 
INFO:Xst:2261 - The FF/Latch <crtc_rd_len_r_12> in Unit <crtc2> is equivalent to the following 3 FFs/Latches, which will be removed : <crtc_rd_len_r_13> <crtc_rd_len_r_14> <crtc_rd_len_r_15> 
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_3> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_4> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_5> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_6> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_7> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_8> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_9> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_10> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_11> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_12> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_13> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_14> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_15> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_16> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_17> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_18> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_19> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_20> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_21> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_22> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_14> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_15> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_0> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_1> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_2> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_3> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_4> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_5> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_6> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_7> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_8> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_9> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_10> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_11> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_12> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_13> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_14> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_15> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_0> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_1> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_2> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_12> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_13> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_14> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_15> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_16> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_17> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_18> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_19> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_20> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_21> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_22> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_23> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_24> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_25> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_26> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_27> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_28> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_29> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_30> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_31> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_23> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_24> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_25> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_26> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_27> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_28> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_29> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_30> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_31> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_0> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_1> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_2> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_3> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_4> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_5> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_6> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_7> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_8> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_9> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_10> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_11> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_0> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_1> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_2> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_3> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_4> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_5> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_6> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_7> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_8> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_9> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_10> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_11> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_12> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_13> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_14> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_15> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_0> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_1> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_2> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_3> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_11> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_12> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_13> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_14> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_15> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_0> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_1> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_2> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_3> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_4> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_5> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_6> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_7> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_8> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_9> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_10> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_11> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_12> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_13> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_14> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_15> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_9> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_10> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_11> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_12> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_13> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_14> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_15> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_0> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_1> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_2> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_3> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_4> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_5> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_6> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_7> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_8> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_9> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_10> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_11> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_12> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_13> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_4> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_5> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_6> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_7> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_8> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_9> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_10> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_11> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_12> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_13> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_14> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_15> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_0> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_1> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_2> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_3> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_4> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_5> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_6> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_7> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_8> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_3> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_4> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_5> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_6> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_7> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_8> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_9> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_10> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_11> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_12> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_13> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_14> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_15> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_0> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_1> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_2> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_3> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_4> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_5> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_6> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_14> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_15> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_0> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_1> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_2> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_3> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_4> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_5> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_6> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_7> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_8> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_9> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_10> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_11> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_12> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_13> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_14> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg07_r_15> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_0> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_1> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg01_r_2> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_12> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_13> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_14> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_15> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_16> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_17> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_18> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_19> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_20> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_21> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_22> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_23> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_24> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_25> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_26> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_27> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_28> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_29> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_30> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_31> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_7> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_8> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_9> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_10> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_11> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_12> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_13> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_14> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_15> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_0> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_1> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_2> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_3> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_4> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_5> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_6> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_7> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_8> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_9> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_10> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg10_r_11> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_0> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_1> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_2> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_3> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_4> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_5> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_6> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_7> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_8> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_9> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_10> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_11> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_12> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_13> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_14> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_15> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_0> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_1> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_2> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_3> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_be_r_0> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_be_r_1> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_be_r_2> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_be_r_3> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wr_r> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_0> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_1> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_2> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_3> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_4> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_5> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_6> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_7> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_8> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_9> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_10> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_11> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_12> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_13> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_14> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg06_r_15> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_9> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_10> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_11> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_12> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_13> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_14> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_15> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_0> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_1> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_2> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_3> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_4> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_5> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_6> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_7> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_8> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_9> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_10> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_11> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_12> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg04_r_13> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_4> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_5> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_6> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_7> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_8> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_9> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_10> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_11> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_12> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_13> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_14> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_15> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_0> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_1> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_2> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_3> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_4> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_5> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_6> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_7> (without init value) has a constant value of 1 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_8> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_414> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_415> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_416> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_417> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_418> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_419> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_420> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_421> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_422> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_423> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_424> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_425> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_426> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_427> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_428> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_429> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_430> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_431> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_432> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_433> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_393> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_394> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_395> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_396> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_397> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_398> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_399> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_400> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_401> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_402> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_403> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_404> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_405> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_406> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_407> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_408> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_409> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_410> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_411> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_412> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_413> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_455> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_456> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_457> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_458> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_459> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_460> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_461> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_462> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_463> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_464> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_465> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_466> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_467> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_468> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_469> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_470> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_471> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_472> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_473> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_474> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_434> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_435> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_436> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_437> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_438> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_439> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_440> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_441> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_442> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_443> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_444> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_445> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_446> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_447> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_448> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_449> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_450> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_451> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_452> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_453> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_454> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_89> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_98> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_107> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_116> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_125> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_134> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_143> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_152> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_161> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_170> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_179> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_197> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_206> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_215> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_224> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_233> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_242> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_251> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_260> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_269> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_2> (without init value) has a constant value of 0 in block <iodrp_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_4> (without init value) has a constant value of 0 in block <iodrp_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_5> (without init value) has a constant value of 0 in block <iodrp_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_6> (without init value) has a constant value of 0 in block <iodrp_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_2> (without init value) has a constant value of 0 in block <iodrp_mcb_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_4> (without init value) has a constant value of 0 in block <iodrp_mcb_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_5> (without init value) has a constant value of 0 in block <iodrp_mcb_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_6> (without init value) has a constant value of 0 in block <iodrp_mcb_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <MCB_UICMD> (without init value) has a constant value of 0 in block <mcb_soft_calibration_inst>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <MCB_UIDQCOUNT_0> (without init value) has a constant value of 0 in block <mcb_soft_calibration_inst>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <MCB_UIDQCOUNT_1> (without init value) has a constant value of 0 in block <mcb_soft_calibration_inst>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <MCB_UIDQCOUNT_2> (without init value) has a constant value of 0 in block <mcb_soft_calibration_inst>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <MCB_UIDQCOUNT_3> (without init value) has a constant value of 0 in block <mcb_soft_calibration_inst>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1293 - FF/Latch <DQS_DELAY_INITIAL_7> has a constant value of 0 in block <mcb_soft_calibration_inst>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <IODRPCTRLR_MEMCELL_ADDR_2> (without init value) has a constant value of 0 in block <mcb_soft_calibration_inst>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_disp00_r_8> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_44> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_53> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_62> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_71> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_80> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_372> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_373> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_374> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_375> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_376> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_377> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_378> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_379> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_380> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_381> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_382> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_383> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_384> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_385> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_386> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_387> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_388> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_389> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_390> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_391> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_392> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_278> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_287> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_296> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_305> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_314> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_r_323> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_334> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_343> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_352> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_360> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_361> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_362> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_363> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_364> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_365> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_366> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_367> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_368> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_369> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_370> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_371> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_3> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_4> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_5> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_6> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_7> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_8> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_9> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_10> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_11> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_12> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_13> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_14> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_15> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_16> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_17> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_18> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_19> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_20> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_21> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_22> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_558> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_559> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_560> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_561> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_562> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_563> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_564> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_565> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_566> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_567> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_568> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_569> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_570> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_571> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_572> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_573> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_574> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_575> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_0> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_1> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_2> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_7> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_8> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_9> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_10> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_11> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_12> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_13> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_14> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_15> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_0> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_1> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_2> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_3> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_4> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_5> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_6> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_7> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_8> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_9> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg05_r_10> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_23> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_24> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_25> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_26> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_27> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_28> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_29> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_30> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_31> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_be_r_0> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_be_r_1> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_be_r_2> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_be_r_3> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wr_r> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_0> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_1> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_2> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_3> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_4> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_5> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg00_r_6> (without init value) has a constant value of 1 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_496> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_497> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_498> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_499> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_500> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_501> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_502> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_503> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_504> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_505> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_506> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_507> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_508> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_509> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_510> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_511> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_512> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_513> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_514> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_515> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_475> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_476> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_477> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_478> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_479> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_480> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_481> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_482> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_483> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_484> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_485> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_486> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_487> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_488> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_489> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_490> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_491> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_492> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_493> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_494> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_495> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_537> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_538> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_539> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_540> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_541> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_542> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_543> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_544> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_545> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_546> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_547> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_548> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_549> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_550> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_551> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_552> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_553> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_554> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_555> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_556> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_557> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_516> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_517> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_518> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_519> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_520> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_521> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_522> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_523> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_524> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_525> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_526> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_527> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_528> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_529> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_530> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_531> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_532> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_533> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_534> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_535> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_536> (without init value) has a constant value of 0 in block <dp_main_tbc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_rd_len_r_7> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_rd_len_r_8> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <fb_rd_len_r_7> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <fb_rd_len_r_8> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_0> of sequential type is unconnected in block <mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_1> of sequential type is unconnected in block <mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_25> of sequential type is unconnected in block <mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_26> of sequential type is unconnected in block <mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_27> of sequential type is unconnected in block <mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_28> of sequential type is unconnected in block <mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_29> of sequential type is unconnected in block <mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_30> of sequential type is unconnected in block <mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_31> of sequential type is unconnected in block <mem>.
WARNING:Xst:2677 - Node <be_r_4> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <be_r_5> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <be_r_6> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <be_r_7> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_0> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_1> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_10> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_11> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_16> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_17> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_18> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_19> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_23> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_31> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <bar_r_2> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <bar_r_3> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <bar_r_4> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <bar_r_5> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <bar_r_6> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <be_in_r_0> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <be_in_r_1> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <be_in_r_2> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <be_in_r_3> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_96> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_97> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_98> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_99> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_100> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_101> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_102> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_103> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_104> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_105> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_106> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_107> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_96> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_97> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_98> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_99> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_100> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_101> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_102> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_103> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_104> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_105> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_106> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_107> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_96> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_97> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_98> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_99> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_100> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_101> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_102> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_103> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_104> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_105> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_106> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_107> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_96> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_97> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_98> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_99> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_100> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_101> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_102> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_103> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_104> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_105> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_106> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_107> of sequential type is unconnected in block <dp_main_tbc>.
WARNING:Xst:2677 - Node <aux_sync_r_3> of sequential type is unconnected in block <aux_rx>.
WARNING:Xst:2677 - Node <aux_data_r_7> of sequential type is unconnected in block <aux_rx>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_0> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_1> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_2> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_3> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_6> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_7> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_0> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_1> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_2> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_3> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_4> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_5> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_10> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_11> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_0> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_1> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_2> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_3> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_4> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_5> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_10> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_11> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_12> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_13> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_14> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_len_r_15> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_rd_vpos_r_12> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_addr_r_12> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_addr_r_13> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_addr_r_14> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <fb_rd_addr_r_15> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_vsync_r> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_hcount_r_12> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_hcount_r_13> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_hcount_r_14> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_hcount_r_15> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_vcount_r_12> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_vcount_r_13> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_vcount_r_14> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_vcount_r_15> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_0> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_1> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_2> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_3> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_4> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_5> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_10> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_11> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_12> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_0> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_1> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_2> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_3> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_4> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_5> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_10> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_11> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_12> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_13> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_14> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_15> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_vpos_r_12> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_addr_r_12> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_addr_r_13> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_addr_r_14> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <fb_rd_addr_r_15> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_cclk_div_r_3> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_dcount_r_12> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_dcount_r_13> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_dcount_r_14> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_dcount_r_15> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_ctrl_dl0_r_1> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_ctrl_dl1_r_1> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_ctrl_dl2_r_1> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_ctrl_dl3_r_1> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_24> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_25> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_26> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_27> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_28> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_29> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_30> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_31> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2404 -  FFs/Latches <TLP_HDR1_r<31:31>> (without init value) have a constant value of 0 in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2404 -  FFs/Latches <tbc_disp00_r<287:287>> (without init value) have a constant value of 0 in block <dp_main_tbc1>.
WARNING:Xst:2404 -  FFs/Latches <tbc_data00_r<575:360>> (without init value) have a constant value of 0 in block <dp_main_tbc1>.
WARNING:Xst:2404 -  FFs/Latches <disp_reg_hcount_sav_r<11:8>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
WARNING:Xst:2404 -  FFs/Latches <disp_reg_hcount_sbp_r<11:7>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
WARNING:Xst:2404 -  FFs/Latches <disp_reg_hcount_eav_r<11:10>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
WARNING:Xst:2404 -  FFs/Latches <disp_reg_vcount_sbp_r<11:1>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
WARNING:Xst:2404 -  FFs/Latches <disp_reg_hcount_end_r<11:10>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
WARNING:Xst:2404 -  FFs/Latches <disp_reg_vcount_sav_r<11:6>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
WARNING:Xst:2404 -  FFs/Latches <disp_reg_vcount_end_r<11:10>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
WARNING:Xst:2404 -  FFs/Latches <disp_reg_vcount_eav_r<11:10>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
WARNING:Xst:2404 -  FFs/Latches <tbc_data0_out_r<575:567>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
WARNING:Xst:2404 -  FFs/Latches <fb_rd_len_r<15:12>> (without init value) have a constant value of 0 in block <xt_crtc>.
WARNING:Xst:2404 -  FFs/Latches <crtc_rd_vpos_r<15:12>> (without init value) have a constant value of 0 in block <xt_crtc>.
WARNING:Xst:2404 -  FFs/Latches <crtc_rd_vpos_r<15:12>> (without init value) have a constant value of 0 in block <xt_crtc2>.
WARNING:Xst:2404 -  FFs/Latches <crtc_rd_len_r<15:12>> (without init value) have a constant value of 0 in block <xt_crtc2>.
WARNING:Xst:2404 -  FFs/Latches <tbc_data00_out_r<575:567>> (without init value) have a constant value of 0 in block <dp_main_tbc1>.
WARNING:Xst:2404 -  FFs/Latches <tbc_data0_out_r<566:558>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.
WARNING:Xst:2404 -  FFs/Latches <fb_rd_addr_r<15:12>> (without init value) have a constant value of 0 in block <xt_crtc>.
WARNING:Xst:2404 -  FFs/Latches <fb_rd_addr_r<15:12>> (without init value) have a constant value of 0 in block <xt_crtc2>.
WARNING:Xst:2404 -  FFs/Latches <fb_rd_len_r<15:12>> (without init value) have a constant value of 0 in block <xt_crtc2>.
WARNING:Xst:2404 -  FFs/Latches <tbc_data00_out_r<566:558>> (without init value) have a constant value of 0 in block <dp_main_tbc1>.
WARNING:Xst:2404 -  FFs/Latches <tbc_data0_out_r<557:549>> (without init value) have a constant value of 0 in block <dp_main_crtc1>.

Synthesizing (advanced) Unit <dp_aux_tx>.
The following registers are absorbed into counter <aux_clk_r>: 1 register on signal <aux_clk_r>.
Unit <dp_aux_tx> synthesized (advanced).

Synthesizing (advanced) Unit <dp_main_linkup1>.
The following registers are absorbed into counter <link_wait100us_count_r>: 1 register on signal <link_wait100us_count_r>.
INFO:Xst:3031 - HDL ADVISOR - The RAM <Mram_aux_cmd_code> will be implemented on LUTs either because you have described an asynchronous read or because of currently unsupported block RAM features. If you have described an asynchronous read, making it synchronous would allow you to take advantage of available block RAM resources, for optimized device usage and improved timings. Please refer to your documentation for coding guidelines.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 64-word x 36-bit                    |          |
    |     weA            | connected to signal <GND>           | high     |
    |     addrA          | connected to signal <(link_aux_cmd_req_r<2:0>,aux_cmd_code_addr_r<2:0>)> |          |
    |     diA            | connected to signal <GND>           |          |
    |     doA            | connected to signal <aux_cmd_code>  |          |
    -----------------------------------------------------------------------
Unit <dp_main_linkup1> synthesized (advanced).

Synthesizing (advanced) Unit <dp_main_scramble>.
The following registers are absorbed into counter <sc_tr_count_r>: 1 register on signal <sc_tr_count_r>.
The following registers are absorbed into counter <sc_no_count_8k_r>: 1 register on signal <sc_no_count_8k_r>.
The following registers are absorbed into counter <sc_no_count_r>: 1 register on signal <sc_no_count_r>.
The following registers are absorbed into counter <sc_op_count_512_r>: 1 register on signal <sc_op_count_512_r>.
INFO:Xst:3030 - HDL ADVISOR - Register <sc_tr_data_out_r> currently described with an asynchronous reset, could be combined with distributed RAM <Mram_n0324> for implementation on block RAM resources if you made this reset synchronous instead.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 32-word x 22-bit                    |          |
    |     weA            | connected to signal <GND>           | high     |
    |     addrA          | connected to signal <(dp_main_mode<0>,sc_tr_count_r)> |          |
    |     diA            | connected to signal <GND>           |          |
    |     doA            | connected to signal <sc_tr_data_out_w> |          |
    -----------------------------------------------------------------------
INFO:Xst:3030 - HDL ADVISOR - Register <sc_no_data_out_r> currently described with an asynchronous reset, could be combined with distributed RAM <Mram_n0326> for implementation on block RAM resources if you made this reset synchronous instead.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 4-word x 18-bit                     |          |
    |     weA            | connected to signal <GND>           | high     |
    |     addrA          | connected to signal <(sc_no_8k_r,sc_no_8k512_r)> |          |
    |     diA            | connected to signal <GND>           |          |
    |     doA            | connected to signal <sc_no_data_out_w> |          |
    -----------------------------------------------------------------------
Unit <dp_main_scramble> synthesized (advanced).

Synthesizing (advanced) Unit <dvi_data_enc>.
INFO:Xst:3031 - HDL ADVISOR - The RAM <Mram_st1_cnt1_hi> will be implemented on LUTs either because you have described an asynchronous read or because of currently unsupported block RAM features. If you have described an asynchronous read, making it synchronous would allow you to take advantage of available block RAM resources, for optimized device usage and improved timings. Please refer to your documentation for coding guidelines.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 16-word x 4-bit                     |          |
    |     weA            | connected to signal <GND>           | high     |
    |     addrA          | connected to signal <st0_qm_r<7:4>> |          |
    |     diA            | connected to signal <GND>           |          |
    |     doA            | connected to signal <st1_cnt1_hi>   |          |
    -----------------------------------------------------------------------
INFO:Xst:3031 - HDL ADVISOR - The RAM <Mram_st1_cnt1_low> will be implemented on LUTs either because you have described an asynchronous read or because of currently unsupported block RAM features. If you have described an asynchronous read, making it synchronous would allow you to take advantage of available block RAM resources, for optimized device usage and improved timings. Please refer to your documentation for coding guidelines.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 16-word x 4-bit                     |          |
    |     weA            | connected to signal <GND>           | high     |
    |     addrA          | connected to signal <st0_qm_r<3:0>> |          |
    |     diA            | connected to signal <GND>           |          |
    |     doA            | connected to signal <st1_cnt1_low>  |          |
    -----------------------------------------------------------------------
Unit <dvi_data_enc> synthesized (advanced).

Synthesizing (advanced) Unit <iodrp_controller>.
The following registers are absorbed into counter <bit_cnt>: 1 register on signal <bit_cnt>.
Unit <iodrp_controller> synthesized (advanced).

Synthesizing (advanced) Unit <iodrp_mcb_controller>.
The following registers are absorbed into counter <bit_cnt>: 1 register on signal <bit_cnt>.
Unit <iodrp_mcb_controller> synthesized (advanced).

Synthesizing (advanced) Unit <mcb_soft_calibration>.
The following registers are absorbed into counter <count>: 1 register on signal <count>.
The following registers are absorbed into counter <WAIT_200us_COUNTER>: 1 register on signal <WAIT_200us_COUNTER>.
The following registers are absorbed into counter <DQS_DELAY>: 1 register on signal <DQS_DELAY>.
The following registers are absorbed into counter <counter_inc>: 1 register on signal <counter_inc>.
The following registers are absorbed into counter <counter_dec>: 1 register on signal <counter_dec>.
	The following adders/subtractors are grouped into adder tree <Madd_n0420_Madd1> :
 	<Madd_n0610[8:0]> in block <mcb_soft_calibration>, 	<Madd_n0613[9:0]> in block <mcb_soft_calibration>, 	<Madd_n0616[10:0]_Madd> in block <mcb_soft_calibration>, 	<Madd__n0715_Madd> in block <mcb_soft_calibration>.
	The following adders/subtractors are grouped into adder tree <Madd_n0592[9:0]1> :
 	<Madd_n0586[7:0]> in block <mcb_soft_calibration>, 	<Madd_n0589[8:0]> in block <mcb_soft_calibration>, 	<Madd_n0592[9:0]> in block <mcb_soft_calibration>.
Unit <mcb_soft_calibration> synthesized (advanced).

Synthesizing (advanced) Unit <xt_crtc>.
The following registers are absorbed into counter <crtc_hcount_r>: 1 register on signal <crtc_hcount_r>.
The following registers are absorbed into counter <crtc_dcount_r>: 1 register on signal <crtc_dcount_r>.
The following registers are absorbed into counter <crtc_cclk_div_r>: 1 register on signal <crtc_cclk_div_r>.
Unit <xt_crtc> synthesized (advanced).
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_0> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_1> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_25> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_26> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_27> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_28> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_29> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_30> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_out_r_31> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <be_r_4> of sequential type is unconnected in block <xt_PIO_32_TX_ENGINE>.
WARNING:Xst:2677 - Node <be_r_5> of sequential type is unconnected in block <xt_PIO_32_TX_ENGINE>.
WARNING:Xst:2677 - Node <be_r_6> of sequential type is unconnected in block <xt_PIO_32_TX_ENGINE>.
WARNING:Xst:2677 - Node <be_r_7> of sequential type is unconnected in block <xt_PIO_32_TX_ENGINE>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_0> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_1> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_10> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_11> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_16> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_17> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_18> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_19> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <TLP_HDR1_r_23> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <be_in_r_0> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <be_in_r_1> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <be_in_r_2> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <be_in_r_3> of sequential type is unconnected in block <xt_PIO_32_RX_ENGINE>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_96> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_97> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_98> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_99> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_100> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_101> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_102> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_103> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_104> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_105> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_106> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data00_r_107> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_96> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_97> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_98> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_99> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_100> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_101> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_102> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_103> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_104> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_105> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_106> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data01_r_107> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_96> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_97> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_98> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_99> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_100> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_101> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_102> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_103> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_104> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_105> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_106> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data02_r_107> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_96> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_97> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_98> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_99> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_100> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_101> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_102> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_103> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_104> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_105> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_106> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_rd_data03_r_107> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <aux_sync_r_3> of sequential type is unconnected in block <dp_aux_rx>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_0> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_1> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_2> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_3> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_6> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_cmd_ack_r_7> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_stat_irq_r_0> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_stat_irq_r_2> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_stat_irq_r_3> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_stat_irq_r_4> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_stat_irq_r_5> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_stat_irq_r_6> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_stat_irq_r_7> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_cmd_code_addr_r_3> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_cmd_code_addr_r_4> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <aux_cmd_code_addr_r_5> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <disp_htiming_r_1> of sequential type is unconnected in block <dp_main_crtc1>.
WARNING:Xst:2677 - Node <crtc_reg07_r_12> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg07_r_13> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg07_r_14> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg07_r_15> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_0> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_1> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_2> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_3> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_4> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_5> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_10> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_11> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <fb_rd_len_r_0> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <fb_rd_len_r_1> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <fb_rd_len_r_2> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <fb_rd_len_r_3> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <fb_rd_len_r_4> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <fb_rd_len_r_5> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <fb_rd_len_r_10> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <fb_rd_len_r_11> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg07_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg07_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg07_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg07_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_hcount_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_hcount_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_hcount_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_hcount_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_vcount_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_vcount_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_vcount_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_vcount_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_0> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_1> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_2> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_3> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_4> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_5> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_10> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_len_r_11> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_0> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_1> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_2> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_3> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_4> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_5> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_10> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <fb_rd_len_r_11> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_cclk_div_r_3> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_dcount_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_dcount_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_dcount_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_dcount_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_24> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_25> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_26> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_27> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_28> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_29> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_30> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl3_r_31> of sequential type is unconnected in block <xt_crtc2>.

=========================================================================
Advanced HDL Synthesis Report

Macro Statistics
# RAMs                                                 : 9
 16x4-bit single-port distributed Read Only RAM        : 6
 32x22-bit single-port distributed Read Only RAM       : 1
 4x18-bit single-port distributed Read Only RAM        : 1
 64x36-bit single-port distributed Read Only RAM       : 1
# Adders/Subtractors                                   : 100
 10-bit adder                                          : 3
 10-bit subtractor                                     : 5
 12-bit adder                                          : 16
 12-bit subtractor                                     : 1
 13-bit adder                                          : 2
 16-bit adder                                          : 4
 2-bit adder                                           : 3
 20-bit adder                                          : 1
 3-bit adder                                           : 4
 4-bit adder                                           : 9
 5-bit adder                                           : 2
 6-bit adder                                           : 1
 7-bit adder                                           : 7
 8-bit adder                                           : 20
 8-bit subtractor                                      : 18
 9-bit adder                                           : 4
# Adder Trees                                          : 2
 10-bit / 4-inputs adder tree                          : 1
 10-bit / 6-inputs adder tree                          : 1
# Counters                                             : 16
 12-bit up counter                                     : 3
 13-bit up counter                                     : 1
 16-bit up counter                                     : 1
 3-bit up counter                                      : 3
 4-bit up counter                                      : 1
 5-bit up counter                                      : 1
 6-bit up counter                                      : 1
 8-bit up counter                                      : 2
 8-bit updown counter                                  : 1
 9-bit up counter                                      : 2
# Registers                                            : 5356
 Flip-Flops                                            : 5356
# Comparators                                          : 43
 10-bit comparator equal                               : 2
 10-bit comparator greater                             : 2
 12-bit comparator equal                               : 24
 12-bit comparator not equal                           : 2
 6-bit comparator equal                                : 1
 6-bit comparator greater                              : 1
 7-bit comparator equal                                : 1
 8-bit comparator greater                              : 8
 8-bit comparator lessequal                            : 2
# Multiplexers                                         : 1880
 1-bit 2-to-1 multiplexer                              : 1092
 1-bit 3-to-1 multiplexer                              : 1
 10-bit 2-to-1 multiplexer                             : 94
 108-bit 2-to-1 multiplexer                            : 8
 11-bit 2-to-1 multiplexer                             : 4
 12-bit 2-to-1 multiplexer                             : 34
 16-bit 2-to-1 multiplexer                             : 14
 2-bit 2-to-1 multiplexer                              : 31
 20-bit 2-to-1 multiplexer                             : 66
 21-bit 2-to-1 multiplexer                             : 24
 21-bit 3-to-1 multiplexer                             : 1
 22-bit 3-to-1 multiplexer                             : 4
 3-bit 2-to-1 multiplexer                              : 61
 32-bit 2-to-1 multiplexer                             : 41
 36-bit 2-to-1 multiplexer                             : 43
 39-bit 2-to-1 multiplexer                             : 13
 4-bit 2-to-1 multiplexer                              : 71
 5-bit 2-to-1 multiplexer                              : 54
 6-bit 2-to-1 multiplexer                              : 8
 7-bit 2-to-1 multiplexer                              : 39
 8-bit 2-to-1 multiplexer                              : 176
 9-bit 2-to-1 multiplexer                              : 1
# FSMs                                                 : 12
# Xors                                                 : 56
 1-bit xor2                                            : 44
 1-bit xor3                                            : 2
 1-bit xor4                                            : 6
 8-bit xor2                                            : 4

=========================================================================

=========================================================================
*                         Low Level Synthesis                           *
=========================================================================
WARNING:Xst:1710 - FF/Latch <MCB_UICMD> (without init value) has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <MCB_UIDQCOUNT_0> (without init value) has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <MCB_UIDQCOUNT_1> (without init value) has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <MCB_UIDQCOUNT_2> (without init value) has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <MCB_UIDQCOUNT_3> (without init value) has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <DQS_DELAY_INITIAL_7> has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <IODRPCTRLR_MEMCELL_ADDR_2> (without init value) has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <IODRPCTRLR_MEMCELL_ADDR_4> (without init value) has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <IODRPCTRLR_MEMCELL_ADDR_5> (without init value) has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <IODRPCTRLR_MEMCELL_ADDR_6> (without init value) has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <DRP_BKST> (without init value) has a constant value of 0 in block <iodrp_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data00_out_r_465> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_464> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_463> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_462> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_461> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_460> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_459> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_458> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_457> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_456> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_455> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_454> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_453> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_452> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_451> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_450> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_449> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_448> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_483> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_482> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_481> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_480> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_479> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_478> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_477> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_476> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_475> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_474> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_473> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_472> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_471> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_470> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_469> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_468> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_467> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_466> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_428> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_427> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_426> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_425> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_424> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_423> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_422> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_421> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_420> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_419> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_418> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_417> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_416> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_415> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_414> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_413> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_412> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_411> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_447> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_446> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_445> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_444> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_443> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_442> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_441> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_440> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_439> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_438> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_437> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_436> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_435> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_434> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_433> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_432> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_431> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_430> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_429> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_538> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_537> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_536> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_535> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_534> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_533> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_532> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_531> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_530> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_529> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_528> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_527> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_526> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_525> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_524> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_523> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_522> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_521> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_557> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_556> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_555> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_554> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_553> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_552> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_551> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_550> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_549> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_548> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_547> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_546> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_545> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_544> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_543> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_542> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_541> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_540> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_539> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_501> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_500> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_499> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_498> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_497> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_496> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_495> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_494> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_493> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_492> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_491> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_490> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_489> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_488> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_487> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_486> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_485> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_484> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_520> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_519> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_518> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_517> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_516> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_515> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_514> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_513> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_512> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_511> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_510> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_509> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_508> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_507> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_506> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_505> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_504> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_503> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_502> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_98> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_89> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_80> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_71> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_62> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_53> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_44> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_25> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_23> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_19> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_18> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_16> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_14> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_10> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_9> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_8> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_7> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_6> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_278> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_269> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_260> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_251> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_242> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_233> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_224> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_215> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_206> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_197> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_179> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_170> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_161> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_152> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_143> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_134> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_125> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_116> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_107> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_161> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_152> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_143> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_134> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_125> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_116> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_107> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_98> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_89> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_80> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_71> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_62> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_53> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_44> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_35> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_26> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_17> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_8> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_5> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_4> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_3> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_2> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_1> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_0> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_278> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_269> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_260> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_251> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_242> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_233> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_224> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_215> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_206> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_197> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_188> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_179> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_disp00_r_170> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_391> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_390> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_389> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_388> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_387> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_386> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_385> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_384> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_383> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_382> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_381> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_380> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_379> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_378> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_377> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_376> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_375> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_374> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_410> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_409> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_408> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_407> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_406> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_405> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_404> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_403> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_402> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_401> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_400> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_399> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_398> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_397> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_396> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_395> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_394> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_393> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_392> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_349> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_347> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_345> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_343> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_342> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_341> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_340> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_339> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_338> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_336> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_335> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_334> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_324> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_323> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_314> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_305> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_296> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_287> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_373> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_372> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_371> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_370> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_369> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_368> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_367> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_366> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_365> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_364> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_363> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_362> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_361> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_360> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_352> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_343> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_out_r_334> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_352> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data00_r_350> (without init value) has a constant value of 0 in block <dp_main_tbc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tbc_data0_out_r_481> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_482> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_483> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_484> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_485> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_486> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_487> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_488> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_489> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_490> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_491> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_492> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_493> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_494> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_495> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_496> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_497> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_498> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_499> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_500> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_501> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_502> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_503> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_504> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_505> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_506> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_507> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_453> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_454> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_455> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_456> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_457> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_458> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_459> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_460> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_461> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_462> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_463> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_464> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_465> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_466> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_467> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_468> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_469> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_470> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_471> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_472> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_473> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_474> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_475> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_476> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_477> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_478> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_479> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_480> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_536> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_537> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_538> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_539> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_540> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_541> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_542> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_543> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_544> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_545> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_546> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_547> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_548> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_end_r_0> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_end_r_1> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_end_r_4> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_end_r_5> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_end_r_6> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_end_r_7> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_end_r_8> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_eav_r_0> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_eav_r_2> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_eav_r_3> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_eav_r_4> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_eav_r_5> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_eav_r_6> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_eav_r_7> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_eav_r_8> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_508> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_509> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_510> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_511> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_512> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_513> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_514> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_515> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_516> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_517> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_518> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_519> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_520> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_521> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_522> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_523> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_524> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_525> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_526> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_527> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_528> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_529> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_530> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_531> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_532> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_533> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_534> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_535> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_370> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_371> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_372> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_373> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_374> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_375> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_376> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_377> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_378> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_379> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_380> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_381> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_382> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_383> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_384> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_385> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_386> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_387> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_388> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_389> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_390> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_391> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_392> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_393> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_394> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_395> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_396> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_hcount_eav_r_4> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_hcount_eav_r_5> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_hcount_eav_r_6> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_hcount_eav_r_7> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_hcount_sav_r_4> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_hcount_sav_r_5> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_hcount_sav_r_6> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_hcount_sbp_r_5> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_sav_r_0> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_sav_r_2> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_sav_r_3> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_vcount_sav_r_4> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_hcount_end_r_5> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_hcount_end_r_6> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <disp_reg_hcount_end_r_7> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_334> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_343> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_352> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_360> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_361> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_362> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_363> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_364> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_365> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_366> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_367> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_368> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_369> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_425> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_426> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_427> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_428> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_429> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_430> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_431> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_432> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_433> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_434> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_435> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_436> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_437> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_438> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_439> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_440> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_441> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_442> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_443> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_444> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_445> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_446> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_447> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_448> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_449> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_450> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_451> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_452> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_397> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_398> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_399> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_400> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_401> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_402> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_403> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_404> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_405> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_406> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_407> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_408> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_409> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_410> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_411> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_412> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_413> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_414> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_415> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_416> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_417> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_418> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_419> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_420> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_421> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_422> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_423> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tbc_data0_out_r_424> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
INFO:Xst:2261 - The FF/Latch <mem_wait_full_r_0> in Unit <xt_mem> is equivalent to the following FF/Latch, which will be removed : <mem_wait_empt_r_0> 
INFO:Xst:2261 - The FF/Latch <mem_wait_full_r_1> in Unit <xt_mem> is equivalent to the following FF/Latch, which will be removed : <mem_wait_empt_r_1> 
INFO:Xst:2261 - The FF/Latch <tbc_data00_r_325> in Unit <dp_main_tbc1> is equivalent to the following FF/Latch, which will be removed : <tbc_data00_r_330> 
INFO:Xst:2261 - The FF/Latch <tbc_data00_r_11> in Unit <dp_main_tbc1> is equivalent to the following 17 FFs/Latches, which will be removed : <tbc_data00_r_12> <tbc_data00_r_13> <tbc_data00_r_15> <tbc_data00_r_17> <tbc_data00_r_20> <tbc_data00_r_21> <tbc_data00_r_22> <tbc_data00_r_24> <tbc_data00_r_26> <tbc_data00_r_351> <tbc_data00_r_353> <tbc_data00_r_354> <tbc_data00_r_355> <tbc_data00_r_356> <tbc_data00_r_357> <tbc_data00_r_358> <tbc_data00_r_359> 
INFO:Xst:2261 - The FF/Latch <disp_reg_dclk_r> in Unit <dp_main_crtc1> is equivalent to the following 32 FFs/Latches, which will be removed : <disp_reg_hcount_eav_r_0> <disp_reg_hcount_eav_r_1> <disp_reg_hcount_eav_r_2> <disp_reg_hcount_eav_r_3> <disp_reg_hcount_eav_r_8> <disp_reg_hcount_eav_r_9> <disp_reg_hcount_sav_r_0> <disp_reg_hcount_sav_r_1> <disp_reg_hcount_sav_r_2> <disp_reg_hcount_sav_r_3> <disp_reg_hcount_sav_r_7> <disp_reg_hcount_sbp_r_0> <disp_reg_hcount_sbp_r_1> <disp_reg_hcount_sbp_r_2> <disp_reg_hcount_sbp_r_3> <disp_reg_hcount_sbp_r_4> <disp_reg_hcount_sbp_r_6> <disp_reg_vcount_sav_r_1> <disp_reg_vcount_sav_r_5> <disp_reg_vcount_sbp_r> <disp_reg_hcount_end_r_0> <disp_reg_hcount_end_r_1> <disp_reg_hcount_end_r_2> <disp_reg_hcount_end_r_3> <disp_reg_hcount_end_r_4> <disp_reg_hcount_end_r_8> <disp_reg_hcount_end_r_9> <disp_reg_vcount_end_r_2> <disp_reg_vcount_end_r_3> <disp_reg_vcount_end_r_9> <disp_reg_vcount_eav_r_1> <disp_reg_vcount_eav_r_9> 
INFO:Xst:2261 - The FF/Latch <mem_rd_count8_r_6> in Unit <xt_crtc> is equivalent to the following FF/Latch, which will be removed : <mem_rd_req_r> 
INFO:Xst:2261 - The FF/Latch <mem_rd_count8_r_6> in Unit <xt_crtc2> is equivalent to the following FF/Latch, which will be removed : <mem_rd_req_r> 
INFO:Xst:2261 - The FF/Latch <tbc_data00_r_337> in Unit <dp_main_tbc1> is equivalent to the following 3 FFs/Latches, which will be removed : <tbc_data00_r_344> <tbc_data00_r_346> <tbc_data00_r_348> 
INFO:Xst:2261 - The FF/Latch <tbc_data00_out_r_351> in Unit <dp_main_tbc1> is equivalent to the following 7 FFs/Latches, which will be removed : <tbc_data00_out_r_353> <tbc_data00_out_r_354> <tbc_data00_out_r_355> <tbc_data00_out_r_356> <tbc_data00_out_r_357> <tbc_data00_out_r_358> <tbc_data00_out_r_359> 
INFO:Xst:2261 - The FF/Latch <tbc_data00_r_27> in Unit <dp_main_tbc1> is equivalent to the following 11 FFs/Latches, which will be removed : <tbc_data00_r_28> <tbc_data00_r_31> <tbc_data00_r_32> <tbc_data00_r_33> <tbc_data00_r_34> <tbc_data00_r_35> <tbc_data00_r_326> <tbc_data00_r_327> <tbc_data00_r_328> <tbc_data00_r_331> <tbc_data00_r_332> 
INFO:Xst:2261 - The FF/Latch <tbc_data00_out_r_342> in Unit <dp_main_tbc1> is equivalent to the following 4 FFs/Latches, which will be removed : <tbc_data00_out_r_345> <tbc_data00_out_r_347> <tbc_data00_out_r_349> <tbc_data00_out_r_350> 
INFO:Xst:2261 - The FF/Latch <tbc_data00_out_r_344> in Unit <dp_main_tbc1> is equivalent to the following 2 FFs/Latches, which will be removed : <tbc_data00_out_r_346> <tbc_data00_out_r_348> 
INFO:Xst:2261 - The FF/Latch <tbc_data00_out_r_335> in Unit <dp_main_tbc1> is equivalent to the following FF/Latch, which will be removed : <tbc_data00_out_r_339> 
INFO:Xst:2261 - The FF/Latch <tbc_data00_out_r_336> in Unit <dp_main_tbc1> is equivalent to the following 3 FFs/Latches, which will be removed : <tbc_data00_out_r_338> <tbc_data00_out_r_340> <tbc_data00_out_r_341> 
INFO:Xst:2261 - The FF/Latch <tbc_data00_out_r_327> in Unit <dp_main_tbc1> is equivalent to the following 2 FFs/Latches, which will be removed : <tbc_data00_out_r_331> <tbc_data00_out_r_332> 
Analyzing FSM <MFsm> for best encoding.
Optimizing FSM <inst_sp6wrap/app/mem/FSM_0> on signal <mem_state_r[1:4]> with user encoding.
-------------------
 State | Encoding
-------------------
 0000  | 0000
 0100  | 0100
 0101  | unreached
 0111  | 0111
 0110  | 0110
 1000  | 1000
 1001  | 1001
 1011  | 1011
 1010  | 1010
-------------------
Analyzing FSM <MFsm> for best encoding.
Optimizing FSM <memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/gen_term_calib.mcb_soft_calibration_top_inst/mcb_soft_calibration_inst/FSM_14> on signal <STATE[1:6]> with gray encoding.
--------------------
 State  | Encoding
--------------------
 000000 | 000000
 000001 | 000001
 000010 | 000011
 000011 | 000010
 000100 | 000110
 000101 | 000111
 000110 | 000101
 000111 | 000100
 001000 | 001100
 001001 | 001101
 001010 | 001111
 001011 | 001110
 001100 | 001010
 001101 | 001011
 010010 | 001001
 010000 | 001000
 001110 | 011000
 001111 | 011001
 010001 | 011011
 010011 | 011010
 010100 | 011110
 010101 | 011111
 100010 | 011101
 100001 | 011100
 010111 | 010100
 010110 | 010101
 011000 | 010111
 011001 | 010110
 011010 | 010010
 011011 | 010011
 011100 | 010001
 011101 | 010000
 011110 | 110000
 011111 | 110001
 100000 | 110011
 100011 | 110010
 100100 | 110110
 100101 | 110111
 100110 | 110101
 101000 | 110100
 101001 | 111100
 100111 | 111101
 101010 | unreached
--------------------
Optimizing FSM <memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/gen_term_calib.mcb_soft_calibration_top_inst/mcb_soft_calibration_inst/iodrp_controller/FSM_15> on signal <state[1:8]> with one-hot encoding.
-------------------
 State | Encoding
-------------------
 000   | 00000001
 001   | 00000010
 010   | 00000100
 011   | 00001000
 111   | 00010000
 100   | 00100000
 101   | 01000000
 110   | 10000000
-------------------
Optimizing FSM <memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/gen_term_calib.mcb_soft_calibration_top_inst/mcb_soft_calibration_inst/iodrp_mcb_controller/FSM_16> on signal <state[1:4]> with GRAY encoding.
-------------------
 State | Encoding
-------------------
 0000  | 0000
 0001  | 0001
 0010  | 0011
 0011  | 0010
 0111  | 0110
 0100  | 0111
 0101  | 0101
 0110  | 0100
 1000  | 1100
 1001  | 1101
-------------------
Analyzing FSM <MFsm> for best encoding.
Optimizing FSM <dp_main/dp_main_tbc/FSM_12> on signal <tbc_state_r[1:4]> with user encoding.
-------------------
 State | Encoding
-------------------
 0000  | 0000
 0001  | 0001
 0010  | 0010
 0011  | 0011
 1000  | 1000
 1001  | 1001
 1010  | 1010
 1011  | 1011
 1100  | 1100
-------------------
Analyzing FSM <MFsm> for best encoding.
Optimizing FSM <dp_main/aux_rx/FSM_10> on signal <aux_state_r[1:3]> with user encoding.
-------------------
 State | Encoding
-------------------
 000   | 000
 001   | 001
 011   | 011
 010   | 010
 100   | 100
-------------------
Analyzing FSM <MFsm> for best encoding.
Optimizing FSM <dp_main/aux_rx/FSM_11> on signal <fsmfake10[1:5]> with one-hot encoding.
-------------------
 State | Encoding
-------------------
 000   | 00001
 001   | 00010
 100   | 00100
 010   | 01000
 011   | 10000
-------------------
Analyzing FSM <MFsm> for best encoding.
Optimizing FSM <dp_main/dp_main_linkup/FSM_6> on signal <aux_state_r[1:3]> with user encoding.
-------------------
 State | Encoding
-------------------
 000   | 000
 001   | 001
 011   | 011
 010   | 010
 100   | 100
 101   | 101
 111   | 111
 110   | 110
-------------------
Analyzing FSM <MFsm> for best encoding.
Optimizing FSM <dp_main/dp_main_linkup/FSM_5> on signal <link_state_r[1:5]> with user encoding.
-------------------
 State | Encoding
-------------------
 00000 | 00000
 00001 | 00001
 00011 | 00011
 00010 | 00010
 00100 | 00100
 00101 | 00101
 00110 | 00110
 00111 | unreached
 01000 | 01000
 01001 | 01001
 01011 | 01011
 01010 | 01010
 01100 | 01100
 01101 | 01101
 01110 | 01110
 01111 | 01111
-------------------
Analyzing FSM <MFsm> for best encoding.
Optimizing FSM <dp_main/aux_tx/FSM_9> on signal <aux_state_r[1:4]> with user encoding.
-------------------
 State | Encoding
-------------------
 0000  | 0000
 0001  | 0001
 0011  | 0011
 0010  | 0010
 0100  | 0100
 0101  | 0101
 0111  | 0111
 0110  | 0110
 1100  | 1100
 1101  | 1101
 1111  | 1111
 1110  | unreached
 1000  | unreached
 1001  | unreached
 1010  | unreached
 1011  | unreached
-------------------
Analyzing FSM <MFsm> for best encoding.
Optimizing FSM <crtc1/FSM_1> on signal <mem_state_r[1:3]> with user encoding.
-------------------
 State | Encoding
-------------------
 000   | 000
 001   | 001
 100   | 100
 101   | 101
 111   | 111
 110   | 110
 011   | 011
-------------------
Analyzing FSM <MFsm> for best encoding.
Optimizing FSM <crtc2/FSM_3> on signal <mem_state_r[1:3]> with user encoding.
-------------------
 State | Encoding
-------------------
 000   | 000
 001   | 001
 100   | 100
 101   | 101
 111   | 111
 110   | 110
 011   | 011
-------------------
WARNING:Xst:1710 - FF/Latch <sc_no_data_out_r_0> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <sc_no_data_out_r_1> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <sc_no_data_out_r_6> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <sc_no_data_out_r_9> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <sc_no_data_out_r_10> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <mem_cmd_instr_r_2> (without init value) has a constant value of 0 in block <xt_mem>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_len_r_2> (without init value) has a constant value of 0 in block <xt_mem>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_len_r_3> (without init value) has a constant value of 0 in block <xt_mem>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_len_r_4> (without init value) has a constant value of 0 in block <xt_mem>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_len_r_5> (without init value) has a constant value of 0 in block <xt_mem>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_0> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_1> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_25> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_26> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_27> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_28> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_29> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_30> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_31> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:1710 - FF/Latch <tsrc_dsc_n> (without init value) has a constant value of 1 in block <xt_PIO_32_TX_ENGINE>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <IODRPCTRLR_WRITE_DATA_7> (without init value) has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <TARGET_DQS_DELAY_7> (without init value) has a constant value of 0 in block <mcb_soft_calibration>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:2677 - Node <tx_data_count_r_10> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_data_count_r_11> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_de_in0_r_4> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_de_in0_r_5> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_de_in0_r_6> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_hs_in0_r_4> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_hs_in0_r_5> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_hs_in0_r_6> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_hs_in1_r_4> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_hs_in1_r_5> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_hs_in1_r_6> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_de_in1_r_4> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_de_in1_r_5> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tx_de_in1_r_6> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_count_r_6> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:2677 - Node <tbc_count_r_7> of sequential type is unconnected in block <dp_main_tbc1>.
WARNING:Xst:1710 - FF/Latch <fsmfake7_4> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_30> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_29> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_27> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_26> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_25> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_24> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_23> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_22> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_21> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_20> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_19> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_18> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_15> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_14> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_13> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_12> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_7> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_6> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_4> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <aux_cmd_code_r_3> (without init value) has a constant value of 0 in block <dp_main_linkup1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:2677 - Node <link_wait400us_r_5> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <link_wait400us_r_6> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:2677 - Node <link_wait400us_r_7> of sequential type is unconnected in block <dp_main_linkup1>.
WARNING:Xst:1710 - FF/Latch <tbc_sync_r_3> (without init value) has a constant value of 0 in block <dp_main_crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:2677 - Node <disp_dclk_r_0> of sequential type is unconnected in block <dp_main_crtc1>.
WARNING:Xst:2677 - Node <disp_dclk_r_1> of sequential type is unconnected in block <dp_main_crtc1>.
WARNING:Xst:2677 - Node <tbc_count_r_6> of sequential type is unconnected in block <dp_main_crtc1>.
WARNING:Xst:2677 - Node <tbc_count_r_7> of sequential type is unconnected in block <dp_main_crtc1>.
WARNING:Xst:1710 - FF/Latch <sc_op_data0_out_r_9> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <sc_op_data0_out_r_10> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <sc_op_data1_out_r_9> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <sc_op_data1_out_r_10> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <sc_op_data2_out_r_9> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <sc_op_data2_out_r_10> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <sc_op_data3_out_r_9> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <sc_op_data3_out_r_10> (without init value) has a constant value of 0 in block <dp_main_scramble>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <tx3_r_5> (without init value) has a constant value of 0 in block <xil_dvi>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tx3_r_6> (without init value) has a constant value of 0 in block <xil_dvi>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tx3_r_7> (without init value) has a constant value of 0 in block <xil_dvi>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tx3_r_8> (without init value) has a constant value of 0 in block <xil_dvi>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <tx3_r_9> (without init value) has a constant value of 0 in block <xil_dvi>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <crtc_reg03_r_3> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_2> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_1> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_0> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_11> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_10> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_9> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_8> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_7> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_6> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_5> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_4> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_3> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_2> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_1> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_0> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_11> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_10> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_9> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_8> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_7> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_6> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_5> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_4> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_3> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_29> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_28> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_27> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_26> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_25> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_24> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_11> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_10> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_9> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_8> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_7> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_6> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_5> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_4> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_3> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_2> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_1> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_0> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_11> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_10> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_9> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_8> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_7> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_6> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_5> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_4> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_0> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_11> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_10> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_9> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_8> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_7> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_6> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_5> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_4> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_3> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_2> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_1> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_0> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_11> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_10> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_9> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_8> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_7> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_6> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_5> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_4> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_3> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_2> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_1> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_0> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_2> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_1> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_0> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_11> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_10> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_9> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_8> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_7> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_6> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_5> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_4> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_3> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_2> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_1> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_0> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_11> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_10> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_9> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_8> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_7> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_6> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_5> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_4> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_3> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_2> (without init value) has a constant value of 0 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_1> (without init value) has a constant value of 1 in block <xt_crtc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:2677 - Node <crtc_reg02_r_12> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg02_r_13> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg02_r_14> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg02_r_15> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg00_r_12> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg00_r_13> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg00_r_14> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg00_r_15> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg05_r_12> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg05_r_13> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg05_r_14> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg05_r_15> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg01_r_12> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg01_r_13> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg01_r_14> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg01_r_15> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg04_r_12> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg04_r_13> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg04_r_14> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg04_r_15> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg06_r_12> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg06_r_13> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg06_r_14> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg06_r_15> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg03_r_12> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg03_r_13> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg03_r_14> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg03_r_15> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_0> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_1> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_2> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_3> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_4> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_5> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_6> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_7> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_8> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_9> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_10> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_11> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_12> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_13> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_14> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_15> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_16> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_17> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_18> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_19> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_20> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_21> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_22> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_23> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_24> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_25> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_26> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_27> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_28> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_29> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_30> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_reg11_r_31> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_rd_addr_r_10> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_rd_addr_r_11> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_10> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_11> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_12> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_13> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_14> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_15> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_0> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_1> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_2> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_3> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_4> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_5> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_6> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_7> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_30> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_31> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_28> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_29> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_30> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_31> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_28> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_29> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_30> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_31> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_cclk_div_r_1> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:2677 - Node <crtc_cclk_div_r_2> of sequential type is unconnected in block <xt_crtc>.
WARNING:Xst:1710 - FF/Latch <crtc_reg02_r_3> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_2> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_1> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_0> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_11> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_10> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_9> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_8> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_7> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_6> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_5> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_4> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_3> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_2> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_1> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg03_r_0> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_11> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_10> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_9> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_8> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_7> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_6> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_5> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_4> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_3> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_29> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_28> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_27> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_26> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_25> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <mem_cmd_addr_r_24> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_11> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_10> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_9> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_8> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_7> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_6> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_5> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_4> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_3> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_2> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_1> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg01_r_0> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_11> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_10> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_9> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_8> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_7> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_6> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_5> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg02_r_4> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_0> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_11> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_10> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_9> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_8> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_7> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_6> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_5> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_4> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_3> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_2> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_1> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg06_r_0> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_11> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_10> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_9> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_8> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_7> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_6> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_5> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_4> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_3> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_2> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_1> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg00_r_0> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_2> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_1> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg07_r_0> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_11> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_10> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_9> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_8> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_7> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_6> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_5> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_4> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_3> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_2> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_1> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_2> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_3> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_4> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_5> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_6> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_7> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_8> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_9> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_10> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg05_r_11> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_0> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg04_r_1> (without init value) has a constant value of 1 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_rd_len_r_7> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_rd_len_r_8> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <fb_rd_len_r_7> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <fb_rd_len_r_8> (without init value) has a constant value of 0 in block <xt_crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:2677 - Node <crtc_reg00_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg00_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg00_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg00_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg06_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg06_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg06_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg06_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg05_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg05_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg05_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg05_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg04_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg04_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg04_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg04_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg03_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg03_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg03_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg03_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg02_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg02_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg02_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg02_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg01_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg01_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg01_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg01_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_0> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_1> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_2> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_3> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_4> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_5> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_6> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_7> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_8> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_9> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_10> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_11> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_16> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_17> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_18> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_19> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_20> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_21> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_22> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_23> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_24> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_25> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_26> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_27> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_28> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_29> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_30> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_reg11_r_31> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_addr_r_10> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_rd_addr_r_11> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_10> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_11> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_12> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_13> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_14> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_rd_addr_r_15> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_cclk_div_r_1> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_cclk_div_r_2> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_0> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_1> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_2> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_3> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_4> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_5> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_6> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_7> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_30> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <mem_cmd_addr_r_31> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_28> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_29> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_30> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_31> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_28> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_29> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_30> of sequential type is unconnected in block <xt_crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_31> of sequential type is unconnected in block <xt_crtc2>.
INFO:Xst:1901 - Instance pll_base_i in unit pll_base_i of type PLL_BASE has been replaced by PLL_ADV
INFO:Xst:1901 - Instance pll_base_inst in unit pll_base_inst of type PLL_BASE has been replaced by PLL_ADV
INFO:Xst:2261 - The FF/Latch <mem_cmd_len_r_0> in Unit <xt_mem> is equivalent to the following FF/Latch, which will be removed : <mem_cmd_len_r_1> 
INFO:Xst:2261 - The FF/Latch <mem_wr_req_out_r_0> in Unit <xt_mem> is equivalent to the following FF/Latch, which will be removed : <mem_cmd_wr_r_0> 
INFO:Xst:2261 - The FF/Latch <MCB_UIADDR_0> in Unit <mcb_soft_calibration> is equivalent to the following 3 FFs/Latches, which will be removed : <MCB_UIADDR_2> <MCB_UIADDR_3> <MCB_UIADDR_4> 
INFO:Xst:2261 - The FF/Latch <link_main_mode_r_2> in Unit <dp_main_linkup1> is equivalent to the following FF/Latch, which will be removed : <link_done_r> 
INFO:Xst:2261 - The FF/Latch <tbc_data0_out_r_351> in Unit <dp_main_crtc1> is equivalent to the following 7 FFs/Latches, which will be removed : <tbc_data0_out_r_353> <tbc_data0_out_r_354> <tbc_data0_out_r_355> <tbc_data0_out_r_356> <tbc_data0_out_r_357> <tbc_data0_out_r_358> <tbc_data0_out_r_359> 
INFO:Xst:2261 - The FF/Latch <scr_lfsr_r_0> in Unit <dp_main_scramble> is equivalent to the following FF/Latch, which will be removed : <scr_lfsr_out_r_7> 
INFO:Xst:2261 - The FF/Latch <sc_data0_out0_r_9> in Unit <dp_main_scramble> is equivalent to the following 3 FFs/Latches, which will be removed : <sc_data1_out0_r_9> <sc_data2_out0_r_9> <sc_data3_out0_r_9> 
INFO:Xst:2261 - The FF/Latch <sc_data0_out0_r_10> in Unit <dp_main_scramble> is equivalent to the following 3 FFs/Latches, which will be removed : <sc_data1_out0_r_10> <sc_data2_out0_r_10> <sc_data3_out0_r_10> 
INFO:Xst:2261 - The FF/Latch <sc_tr_data_out_r_1> in Unit <dp_main_scramble> is equivalent to the following FF/Latch, which will be removed : <sc_tr_data_out_r_6> 
INFO:Xst:2261 - The FF/Latch <scr_lfsr_r_1> in Unit <dp_main_scramble> is equivalent to the following FF/Latch, which will be removed : <scr_lfsr_out_r_6> 
INFO:Xst:2261 - The FF/Latch <sc_no_data_out_r_2> in Unit <dp_main_scramble> is equivalent to the following 3 FFs/Latches, which will be removed : <sc_no_data_out_r_3> <sc_no_data_out_r_4> <sc_no_data_out_r_8> 
INFO:Xst:2261 - The FF/Latch <sc_no_data_out_r_5> in Unit <dp_main_scramble> is equivalent to the following FF/Latch, which will be removed : <sc_no_data_out_r_7> 
INFO:Xst:2261 - The FF/Latch <scr_lfsr_r_2> in Unit <dp_main_scramble> is equivalent to the following FF/Latch, which will be removed : <scr_lfsr_out_r_5> 
INFO:Xst:2261 - The FF/Latch <sc_tr_data_out_r_2> in Unit <dp_main_scramble> is equivalent to the following 4 FFs/Latches, which will be removed : <sc_tr_data_out_r_4> <sc_tr_data_out_r_5> <sc_tr_data_out_r_8> <sc_tr_data_out_r_10> 
INFO:Xst:2261 - The FF/Latch <sc_data0_out1_r_10> in Unit <dp_main_scramble> is equivalent to the following 3 FFs/Latches, which will be removed : <sc_data1_out1_r_10> <sc_data2_out1_r_10> <sc_data3_out1_r_10> 
INFO:Xst:2261 - The FF/Latch <sc_data0_out1_r_9> in Unit <dp_main_scramble> is equivalent to the following 3 FFs/Latches, which will be removed : <sc_data1_out1_r_9> <sc_data2_out1_r_9> <sc_data3_out1_r_9> 
INFO:Xst:2261 - The FF/Latch <tx3_r_3> in Unit <xil_dvi> is equivalent to the following FF/Latch, which will be removed : <tx3_r_4> 
INFO:Xst:2261 - The FF/Latch <crtc_rd_len_r_6> in Unit <xt_crtc> is equivalent to the following 3 FFs/Latches, which will be removed : <crtc_rd_len_r_7> <crtc_rd_len_r_8> <crtc_rd_len_r_9> 
INFO:Xst:2261 - The FF/Latch <fb_rd_len_r_6> in Unit <xt_crtc> is equivalent to the following 3 FFs/Latches, which will be removed : <fb_rd_len_r_7> <fb_rd_len_r_8> <fb_rd_len_r_9> 
INFO:Xst:2261 - The FF/Latch <crtc_rd_len_r_6> in Unit <xt_crtc2> is equivalent to the following FF/Latch, which will be removed : <crtc_rd_len_r_9> 
INFO:Xst:2261 - The FF/Latch <fb_rd_len_r_6> in Unit <xt_crtc2> is equivalent to the following FF/Latch, which will be removed : <fb_rd_len_r_9> 
WARNING:Xst:1710 - FF/Latch <addr_r_0> (without init value) has a constant value of 0 in block <xt_PIO_32_TX_ENGINE>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <addr_r_1> (without init value) has a constant value of 0 in block <xt_PIO_32_TX_ENGINE>. This FF/Latch will be trimmed during the optimization process.
INFO:Xst:2261 - The FF/Latch <sc_data1_out2_r_10> in Unit <dp_main_scramble> is equivalent to the following 3 FFs/Latches, which will be removed : <sc_data0_out2_r_10> <sc_data2_out2_r_10> <sc_data3_out2_r_10> 
INFO:Xst:2261 - The FF/Latch <sc_data1_out2_r_9> in Unit <dp_main_scramble> is equivalent to the following 3 FFs/Latches, which will be removed : <sc_data0_out2_r_9> <sc_data2_out2_r_9> <sc_data3_out2_r_9> 
INFO:Xst:2261 - The FF/Latch <sc_data1_dl1_r_10> in Unit <dp_main_scramble> is equivalent to the following 2 FFs/Latches, which will be removed : <sc_data2_dl1_r_10> <sc_data3_dl1_r_10> 
INFO:Xst:2261 - The FF/Latch <sc_data1_dl1_r_9> in Unit <dp_main_scramble> is equivalent to the following 2 FFs/Latches, which will be removed : <sc_data2_dl1_r_9> <sc_data3_dl1_r_9> 
INFO:Xst:2261 - The FF/Latch <sc_data2_dl2_r_9> in Unit <dp_main_scramble> is equivalent to the following FF/Latch, which will be removed : <sc_data3_dl2_r_9> 
INFO:Xst:2261 - The FF/Latch <sc_data2_dl2_r_10> in Unit <dp_main_scramble> is equivalent to the following FF/Latch, which will be removed : <sc_data3_dl2_r_10> 
INFO:Xst:2261 - The FF/Latch <tx3_r_1> in Unit <xil_dvi> is equivalent to the following FF/Latch, which will be removed : <tx3_r_2> 

Optimizing unit <exp6t_disp> ...

Optimizing unit <sp6wrap> ...

Optimizing unit <xt_pcie_app_s6> ...

Optimizing unit <xt_mem> ...
WARNING:Xst:2677 - Node <mem_wr_data3_r_0> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_1> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_2> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_3> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_4> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_5> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_6> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_7> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_8> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_9> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_10> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_11> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_12> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_13> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_14> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_15> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_16> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_17> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_18> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_19> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_20> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_21> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_22> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_23> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_24> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_25> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_26> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_27> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_28> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_29> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_30> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_data3_r_31> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_mask3_r_0> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_mask3_r_1> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_mask3_r_2> of sequential type is unconnected in block <xt_mem>.
WARNING:Xst:2677 - Node <mem_wr_mask3_r_3> of sequential type is unconnected in block <xt_mem>.

Optimizing unit <xt_PIO> ...

Optimizing unit <xt_PIO_EP> ...

Optimizing unit <xt_PIO_32_TX_ENGINE> ...

Optimizing unit <xt_PIO_32_RX_ENGINE> ...
WARNING:Xst:1710 - FF/Latch <addr_r_0> (without init value) has a constant value of 0 in block <xt_PIO_32_RX_ENGINE>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <addr_r_1> (without init value) has a constant value of 0 in block <xt_PIO_32_RX_ENGINE>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <addr_r_0> (without init value) has a constant value of 0 in block <xt_PIO_32_RX_ENGINE>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <addr_r_1> (without init value) has a constant value of 0 in block <xt_PIO_32_RX_ENGINE>. This FF/Latch will be trimmed during the optimization process.

Optimizing unit <xt_PIO_TO_CTRL> ...

Optimizing unit <eptest> ...

Optimizing unit <GTPA1_DUAL_WRAPPER> ...

Optimizing unit <GTPA1_DUAL_WRAPPER_TILE> ...

Optimizing unit <pcie_bram_top_s6> ...

Optimizing unit <pcie_brams_s6> ...

Optimizing unit <pcie_bram_s6> ...

Optimizing unit <XIL_S6_GTPWIZARD_V1_6_DP> ...

Optimizing unit <XIL_S6_GTPWIZARD_V1_6_DP_TILE> ...

Optimizing unit <xil_clk_wiz_v1_6_27x162> ...

Optimizing unit <xil_clk_wiz_v1_6_50x200> ...

Optimizing unit <xil_clk_wiz_v1_6_50x62x312> ...

Optimizing unit <memc3_wrapper> ...

Optimizing unit <mcb_raw_wrapper> ...

Optimizing unit <mcb_soft_calibration_top> ...

Optimizing unit <mcb_soft_calibration> ...

Optimizing unit <iodrp_controller> ...

Optimizing unit <iodrp_mcb_controller> ...

Optimizing unit <dp_main_640x480> ...

Optimizing unit <dp_main_tbc1> ...

Optimizing unit <dp_aux_rx> ...

Optimizing unit <dp_main_linkup1> ...

Optimizing unit <dp_main_crtc1> ...
INFO:Xst:2261 - The FF/Latch <tbc_data0_out_r_342> in Unit <dp_main_crtc1> is equivalent to the following 4 FFs/Latches, which will be removed : <tbc_data0_out_r_345> <tbc_data0_out_r_347> <tbc_data0_out_r_349> <tbc_data0_out_r_350> 
INFO:Xst:2261 - The FF/Latch <tbc_data0_out_r_344> in Unit <dp_main_crtc1> is equivalent to the following 2 FFs/Latches, which will be removed : <tbc_data0_out_r_346> <tbc_data0_out_r_348> 
INFO:Xst:2261 - The FF/Latch <tbc_data0_out_r_335> in Unit <dp_main_crtc1> is equivalent to the following FF/Latch, which will be removed : <tbc_data0_out_r_339> 
INFO:Xst:2261 - The FF/Latch <tbc_data0_out_r_336> in Unit <dp_main_crtc1> is equivalent to the following 3 FFs/Latches, which will be removed : <tbc_data0_out_r_338> <tbc_data0_out_r_340> <tbc_data0_out_r_341> 
INFO:Xst:2261 - The FF/Latch <tbc_data0_out_r_327> in Unit <dp_main_crtc1> is equivalent to the following 2 FFs/Latches, which will be removed : <tbc_data0_out_r_331> <tbc_data0_out_r_332> 
INFO:Xst:2261 - The FF/Latch <tbc_data0_out_r_318> in Unit <dp_main_crtc1> is equivalent to the following FF/Latch, which will be removed : <tbc_data0_out_r_322> 
INFO:Xst:2261 - The FF/Latch <tbc_data0_out_r_335> in Unit <dp_main_crtc1> is equivalent to the following FF/Latch, which will be removed : <tbc_data0_out_r_339> 
INFO:Xst:2261 - The FF/Latch <tbc_data0_out_r_336> in Unit <dp_main_crtc1> is equivalent to the following 3 FFs/Latches, which will be removed : <tbc_data0_out_r_338> <tbc_data0_out_r_340> <tbc_data0_out_r_341> 
INFO:Xst:2261 - The FF/Latch <tbc_data0_out_r_327> in Unit <dp_main_crtc1> is equivalent to the following 2 FFs/Latches, which will be removed : <tbc_data0_out_r_331> <tbc_data0_out_r_332> 
INFO:Xst:2261 - The FF/Latch <tbc_data0_out_r_318> in Unit <dp_main_crtc1> is equivalent to the following FF/Latch, which will be removed : <tbc_data0_out_r_322> 

Optimizing unit <dp_main_scramble> ...

Optimizing unit <dp_aux_tx> ...

Optimizing unit <memc3_infrastructure> ...

Optimizing unit <xil_dvi> ...

Optimizing unit <dvi_data_enc> ...
WARNING:Xst:1710 - FF/Latch <st1_cnt_r_0> (without init value) has a constant value of 0 in block <dvi_data_enc>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <st1_cnt_r_0> (without init value) has a constant value of 0 in block <dvi_data_enc>. This FF/Latch will be trimmed during the optimization process.

Optimizing unit <xt_crtc> ...

Optimizing unit <xt_crtc2> ...
WARNING:Xst:1710 - FF/Latch <io_wr_r> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_1> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_be_r_0> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wr_r> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_wdata_r_1> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <io_be_r_0> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_cmd_r_2> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_cmd_r_1> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_19> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_18> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_17> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_16> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_15> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_14> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_13> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_12> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_2> (without init value) has a constant value of 0 in block <iodrp_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_4> (without init value) has a constant value of 0 in block <iodrp_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_5> (without init value) has a constant value of 0 in block <iodrp_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_6> (without init value) has a constant value of 0 in block <iodrp_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <data_reg_7> (without init value) has a constant value of 0 in block <iodrp_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_2> (without init value) has a constant value of 0 in block <iodrp_mcb_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_4> (without init value) has a constant value of 0 in block <iodrp_mcb_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_5> (without init value) has a constant value of 0 in block <iodrp_mcb_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <memcell_addr_reg_6> (without init value) has a constant value of 0 in block <iodrp_mcb_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <data_reg_7> (without init value) has a constant value of 0 in block <iodrp_mcb_controller>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_4> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_5> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_6> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_7> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_10> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1710 - FF/Latch <aux_addr_r_11> (without init value) has a constant value of 0 in block <aux_tx>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg10_r_1> (without init value) has a constant value of 0 in block <crtc1>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch <crtc_reg10_r_1> (without init value) has a constant value of 0 in block <crtc2>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:2677 - Node <rdy_o> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <ren_r> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_12> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_13> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_14> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_15> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_16> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_17> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_18> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_19> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_20> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_21> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_22> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_23> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_24> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_25> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_26> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_27> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_28> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_29> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_30> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <addr_r_31> of sequential type is unconnected in block <EP_TX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_12> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_13> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_14> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_15> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_16> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_17> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_18> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_19> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_20> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_21> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_22> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_23> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_24> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_25> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_26> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_27> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_28> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_29> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_30> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <TLP_HDR3_r_31> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <bar_r_2> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <bar_r_3> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <bar_r_4> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <bar_r_5> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <bar_r_6> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <addr_r_25> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <addr_r_26> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <addr_r_27> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <addr_r_28> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <addr_r_29> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <addr_r_30> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <addr_r_31> of sequential type is unconnected in block <EP_RX>.
WARNING:Xst:2677 - Node <read_data_0> of sequential type is unconnected in block <iodrp_mcb_controller>.
WARNING:Xst:2677 - Node <read_data_1> of sequential type is unconnected in block <iodrp_mcb_controller>.
WARNING:Xst:2677 - Node <read_data_2> of sequential type is unconnected in block <iodrp_mcb_controller>.
WARNING:Xst:2677 - Node <read_data_3> of sequential type is unconnected in block <iodrp_mcb_controller>.
WARNING:Xst:2677 - Node <read_data_4> of sequential type is unconnected in block <iodrp_mcb_controller>.
WARNING:Xst:2677 - Node <read_data_5> of sequential type is unconnected in block <iodrp_mcb_controller>.
WARNING:Xst:2677 - Node <read_data_6> of sequential type is unconnected in block <iodrp_mcb_controller>.
WARNING:Xst:2677 - Node <read_data_7> of sequential type is unconnected in block <iodrp_mcb_controller>.
WARNING:Xst:2677 - Node <aux_data_r_2> of sequential type is unconnected in block <aux_rx>.
WARNING:Xst:2677 - Node <aux_data_r_3> of sequential type is unconnected in block <aux_rx>.
WARNING:Xst:2677 - Node <aux_data_r_4> of sequential type is unconnected in block <aux_rx>.
WARNING:Xst:2677 - Node <aux_data_r_5> of sequential type is unconnected in block <aux_rx>.
WARNING:Xst:2677 - Node <aux_data_r_6> of sequential type is unconnected in block <aux_rx>.
WARNING:Xst:2677 - Node <aux_data_r_7> of sequential type is unconnected in block <aux_rx>.
WARNING:Xst:2677 - Node <aux_cmd_r_6> of sequential type is unconnected in block <aux_rx>.
WARNING:Xst:2677 - Node <aux_cmd_r_7> of sequential type is unconnected in block <aux_rx>.
WARNING:Xst:2677 - Node <aux_unit_r_0> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_unit_r_1> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_unit_r_2> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_unit_r_3> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_unit_r_4> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_unit_r_5> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_unit_r_6> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_unit_r_7> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_stat_irq_r_1> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_timeout_r> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_stat_tr1_r_1> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_stat_tr1_r_2> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_stat_tr1_r_3> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_stat_tr2_r_1> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_stat_tr2_r_2> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <aux_stat_tr2_r_3> of sequential type is unconnected in block <dp_main_linkup>.
WARNING:Xst:2677 - Node <disp_blank_n_r> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_0> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_1> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_2> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_3> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_4> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_5> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_6> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_7> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_8> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_9> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_10> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_11> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_12> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_13> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_14> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_15> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_16> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_17> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_18> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_19> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_20> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_21> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_22> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_23> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_24> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_25> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_26> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_27> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_28> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_29> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_30> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_31> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_32> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_33> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_34> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_35> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_36> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_37> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_38> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_39> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_40> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_41> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_42> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_43> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_44> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_45> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_46> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_47> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_48> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_49> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_50> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_51> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_52> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_53> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_54> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_55> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_56> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_57> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_58> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_59> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_60> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_61> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_62> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_63> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_64> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_65> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_66> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_67> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_68> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_69> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_70> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_71> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_72> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_73> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_74> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_75> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_76> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_77> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_78> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_79> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_80> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_81> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_82> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_83> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_84> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_85> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_86> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_87> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_88> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_89> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_90> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_91> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_92> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_93> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_94> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_95> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_96> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_97> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_98> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_99> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_100> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_101> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_102> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_103> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_104> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_105> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_106> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_107> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_108> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_109> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_110> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_111> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_112> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_113> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_114> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_115> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_116> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_117> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_118> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_119> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_120> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_121> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_122> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_123> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_124> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_125> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_126> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_127> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_128> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_129> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_130> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_131> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_132> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_133> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_134> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_135> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_136> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_137> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_138> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_139> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_140> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_141> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_142> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_143> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_144> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_145> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_146> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_147> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_148> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_149> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_150> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_151> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_152> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_153> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_154> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_155> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_156> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_157> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_158> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_159> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_160> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_161> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_162> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_163> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_164> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_165> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_166> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_167> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_168> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_169> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_170> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_171> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_172> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_173> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_174> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_175> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_176> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_177> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_178> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_179> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_180> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_181> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_182> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_183> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_184> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_185> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_186> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_187> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_188> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_189> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_190> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_191> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_192> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_193> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_194> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_195> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_196> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_197> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_198> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_199> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_200> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_201> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_202> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_203> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_204> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_205> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_206> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_207> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_208> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_209> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_210> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_211> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_212> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_213> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_214> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_215> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_216> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_217> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_218> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_219> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_220> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_221> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_222> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_223> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_224> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_225> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_226> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_227> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_228> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_229> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_230> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_231> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_232> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_233> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_234> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_235> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_236> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_237> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_238> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_239> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_240> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_241> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_242> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_243> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_244> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_245> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_246> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_247> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_248> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_249> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_250> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_251> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_252> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_253> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_254> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_255> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_256> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_257> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_258> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_259> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_260> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_261> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_262> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_263> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_264> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_265> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_266> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_267> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_268> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_269> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_270> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_271> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_272> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_273> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_274> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_275> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_276> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_277> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_278> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_279> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_280> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_281> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_282> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_283> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_284> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_285> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_286> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_287> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_288> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_289> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_290> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_291> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_292> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_293> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_294> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_295> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_296> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_297> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_298> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_299> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_300> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_301> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_302> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_303> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_304> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_305> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_306> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_307> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_308> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_309> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_310> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_311> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_312> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_313> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_314> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_315> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_316> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_317> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_318> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_319> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_320> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_321> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_323> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_324> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_325> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_326> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_327> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_328> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_329> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_330> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_333> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_335> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_336> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_337> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_342> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_344> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_data0_out_r_351> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_count_sync_r> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hsync_n_r> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vsync_n_r> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_sync_ss_r> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_de1_r> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vtiming_r_0> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vtiming_r_1> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vtiming_r_2> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vtiming_r_3> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_0> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_1> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_2> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_3> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_4> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_5> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_6> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_7> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_8> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_9> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_10> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vcount_r_11> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_0> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_1> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_2> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_3> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_4> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_5> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_6> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_7> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_8> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_9> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_10> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hcount_r_11> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_hblank_n_r> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_htiming_r_0> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_htiming_r_2> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_htiming_r_3> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_htiming_r_4> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <disp_vblank_n_r> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_count_r_0> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_count_r_1> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_count_r_2> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_count_r_3> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_count_r_4> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_count_r_5> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_sync_r_0> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_sync_r_1> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_sync_r_2> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <tbc_clr_r> of sequential type is unconnected in block <dp_main_crtc>.
WARNING:Xst:2677 - Node <pack_data2_in_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data2_in_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data2_in_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data2_in_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data2_in_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data2_in_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data2_in_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data2_in_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data2_in_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data1_in_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data1_in_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data1_in_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data1_in_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data1_in_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data1_in_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data1_in_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data1_in_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data1_in_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data3_in_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data3_in_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data3_in_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data3_in_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data3_in_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data3_in_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data3_in_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data3_in_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <pack_data3_in_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out_r> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data1_out_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data1_out_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data1_out_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data1_out_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data1_out_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data1_out_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data1_out_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data1_out_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data1_out_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data2_out_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data2_out_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data2_out_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data2_out_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data2_out_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data2_out_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data2_out_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data2_out_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data2_out_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data3_out_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data3_out_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data3_out_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data3_out_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data3_out_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data3_out_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data3_out_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data3_out_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_op_data3_out_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out0_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out0_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out0_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out0_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out0_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out0_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out0_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out0_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out0_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out0_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out0_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out0_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out0_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out0_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out0_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out0_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out0_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out0_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out0_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out0_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out0_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out0_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out0_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out0_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out0_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out0_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out0_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out1_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out1_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out1_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out1_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out1_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out1_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out1_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out1_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out1_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out1_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out1_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out1_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out1_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out1_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out1_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out1_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out1_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out1_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out1_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out1_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out1_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out1_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out1_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out1_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out1_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out1_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out1_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out2_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out2_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out2_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out2_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out2_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out2_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out2_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out2_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_out2_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out2_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out2_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out2_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out2_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out2_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out2_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out2_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out2_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_out2_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out2_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out2_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out2_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out2_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out2_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out2_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out2_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out2_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_out2_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_dl1_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_dl1_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_dl1_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_dl1_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_dl1_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_dl1_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_dl1_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_dl1_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_dl1_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_dl1_r_9> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data1_dl1_r_10> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl1_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl1_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl1_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl1_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl1_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl1_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl1_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl1_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl1_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl1_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl1_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl1_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl1_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl1_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl1_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl1_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl1_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl1_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl2_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl2_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl2_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl2_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl2_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl2_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl2_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl2_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl2_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl2_r_9> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data2_dl2_r_10> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl2_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl2_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl2_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl2_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl2_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl2_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl2_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl2_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl2_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl3_r_0> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl3_r_1> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl3_r_2> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl3_r_3> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl3_r_4> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl3_r_5> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl3_r_6> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl3_r_7> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl3_r_8> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl3_r_9> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <sc_data3_dl3_r_10> of sequential type is unconnected in block <dp_main_scramble>.
WARNING:Xst:2677 - Node <aux_select_r_0> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_1> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_2> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_3> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_4> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_5> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_6> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_7> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_8> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_9> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_10> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_11> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_12> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_13> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_14> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_15> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_16> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_17> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_18> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_select_r_19> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <aux_data_req_r> of sequential type is unconnected in block <aux_tx>.
WARNING:Xst:2677 - Node <io_be_r_1> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_be_r_2> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_be_r_3> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_0> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_2> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_3> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_4> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_5> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_6> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_7> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_8> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_9> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_10> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_11> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_12> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_13> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_14> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_15> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_16> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_17> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_18> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_19> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_20> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_21> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_22> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_23> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_24> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_25> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_26> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_27> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_28> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_29> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_30> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_wdata_r_31> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_req_r> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_ack_r> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_0> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_2> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_3> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_4> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_5> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_6> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_7> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_8> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_9> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_10> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_11> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_12> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_13> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_14> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_15> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_16> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_17> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_18> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_19> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_20> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_21> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_22> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_23> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_24> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_25> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_26> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_27> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_28> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_29> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_30> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_reg10_r_31> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <io_be_r_1> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_be_r_2> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_be_r_3> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_0> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_2> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_3> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_4> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_5> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_6> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_7> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_8> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_9> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_10> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_11> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_12> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_13> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_14> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_15> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_16> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_17> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_18> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_19> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_20> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_21> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_22> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_23> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_24> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_25> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_26> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_27> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_28> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_29> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_30> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_wdata_r_31> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_req_r> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <d_vsync_n_r> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_vsync_r> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <io_ack_r> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_ctrl_dl0_r_1> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_ctrl_dl1_r_1> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_ctrl_dl2_r_1> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_ctrl_dl3_r_1> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_0> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_2> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_3> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_4> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_5> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_6> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_7> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_8> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_9> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_10> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_11> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_12> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_13> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_14> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_15> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_16> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_17> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_18> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_19> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_20> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_21> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_22> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_23> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_24> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_25> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_26> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_27> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_28> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_29> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_30> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_reg10_r_31> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_24> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_25> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_26> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_27> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_24> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_25> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_26> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_27> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_cclk_div_r_0> of sequential type is unconnected in block <crtc1>.
WARNING:Xst:2677 - Node <crtc_cclk_div_r_0> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_24> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_25> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_26> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl1_r_27> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_24> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_25> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_26> of sequential type is unconnected in block <crtc2>.
WARNING:Xst:2677 - Node <crtc_data_dl2_r_27> of sequential type is unconnected in block <crtc2>.

Mapping all equations...
Building and optimizing final netlist ...
INFO:Xst:2261 - The FF/Latch <crtc_cclk_r> in Unit <crtc1> is equivalent to the following FF/Latch, which will be removed : <crtc_rd_len_r_6> 
INFO:Xst:2261 - The FF/Latch <crtc_cclk_r> in Unit <crtc2> is equivalent to the following FF/Latch, which will be removed : <crtc_rd_len_r_6> 
Found area constraint ratio of 100 (+ 5) on block exp6t_disp, actual ratio is 5.
WARNING:Xst:387 - The KEEP property attached to the net <memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/int_sys_rst> may hinder timing optimization.
   You may achieve better results by removing this property
INFO:Xst:2261 - The FF/Latch <tx3_r_3> in Unit <tx_dvi> is equivalent to the following 7 FFs/Latches, which will be removed : <tx3_r_0_BRB0> <tx0_r_0_BRB0> <tx0_r_1_BRB0> <tx1_r_0_BRB0> <tx1_r_1_BRB0> <tx2_r_0_BRB0> <tx2_r_1_BRB0> 
INFO:Xst:2261 - The FF/Latch <tx3_out_r_1> in Unit <tx_dvi> is equivalent to the following FF/Latch, which will be removed : <tx3_r_0_BRB1> 
INFO:Xst:2261 - The FF/Latch <tx3_r_3> in Unit <tx_dvi> is equivalent to the following 7 FFs/Latches, which will be removed : <tx3_r_1_BRB0> <tx0_r_2_BRB0> <tx0_r_3_BRB0> <tx1_r_2_BRB0> <tx1_r_3_BRB0> <tx2_r_2_BRB0> <tx2_r_3_BRB0> 
INFO:Xst:2261 - The FF/Latch <tx3_r_3> in Unit <tx_dvi> is equivalent to the following 6 FFs/Latches, which will be removed : <tx0_r_4_BRB0> <tx0_r_5_BRB0> <tx1_r_4_BRB0> <tx1_r_5_BRB0> <tx2_r_4_BRB0> <tx2_r_5_BRB0> 
INFO:Xst:2261 - The FF/Latch <tx3_r_3> in Unit <tx_dvi> is equivalent to the following 6 FFs/Latches, which will be removed : <tx0_r_6_BRB0> <tx0_r_7_BRB0> <tx1_r_6_BRB0> <tx1_r_7_BRB0> <tx2_r_6_BRB0> <tx2_r_7_BRB0> 
INFO:Xst:2261 - The FF/Latch <tx3_r_3> in Unit <tx_dvi> is equivalent to the following 6 FFs/Latches, which will be removed : <tx0_r_8_BRB0> <tx0_r_9_BRB0> <tx1_r_8_BRB0> <tx1_r_9_BRB0> <tx2_r_8_BRB0> <tx2_r_9_BRB0> 

Pipelining and Register Balancing Report ...

Processing Unit <dp_main/aux_rx> :
	Register(s) aux_rx_in_r_0 has(ve) been backward balanced into : aux_rx_in_r_0_BRB0 aux_rx_in_r_0_BRB1.
Unit <dp_main/aux_rx> processed.

Processing Unit <crtc2> :
	Register(s) crtc_data_dl1_r_0 has(ve) been backward balanced into : crtc_data_dl1_r_0_BRB1 crtc_data_dl1_r_0_BRB2.
	Register(s) crtc_data_dl1_r_1 has(ve) been backward balanced into : crtc_data_dl1_r_1_BRB2.
	Register(s) crtc_data_dl1_r_10 has(ve) been backward balanced into : crtc_data_dl1_r_10_BRB2.
	Register(s) crtc_data_dl1_r_11 has(ve) been backward balanced into : crtc_data_dl1_r_11_BRB2.
	Register(s) crtc_data_dl1_r_12 has(ve) been backward balanced into : crtc_data_dl1_r_12_BRB2.
	Register(s) crtc_data_dl1_r_13 has(ve) been backward balanced into : crtc_data_dl1_r_13_BRB2.
	Register(s) crtc_data_dl1_r_14 has(ve) been backward balanced into : crtc_data_dl1_r_14_BRB2.
	Register(s) crtc_data_dl1_r_15 has(ve) been backward balanced into : crtc_data_dl1_r_15_BRB2.
	Register(s) crtc_data_dl1_r_16 has(ve) been backward balanced into : crtc_data_dl1_r_16_BRB2.
	Register(s) crtc_data_dl1_r_17 has(ve) been backward balanced into : crtc_data_dl1_r_17_BRB2.
	Register(s) crtc_data_dl1_r_18 has(ve) been backward balanced into : crtc_data_dl1_r_18_BRB2.
	Register(s) crtc_data_dl1_r_19 has(ve) been backward balanced into : crtc_data_dl1_r_19_BRB2.
	Register(s) crtc_data_dl1_r_2 has(ve) been backward balanced into : crtc_data_dl1_r_2_BRB2.
	Register(s) crtc_data_dl1_r_20 has(ve) been backward balanced into : crtc_data_dl1_r_20_BRB2.
	Register(s) crtc_data_dl1_r_21 has(ve) been backward balanced into : crtc_data_dl1_r_21_BRB2.
	Register(s) crtc_data_dl1_r_22 has(ve) been backward balanced into : crtc_data_dl1_r_22_BRB2.
	Register(s) crtc_data_dl1_r_23 has(ve) been backward balanced into : crtc_data_dl1_r_23_BRB2.
	Register(s) crtc_data_dl1_r_3 has(ve) been backward balanced into : crtc_data_dl1_r_3_BRB2.
	Register(s) crtc_data_dl1_r_4 has(ve) been backward balanced into : crtc_data_dl1_r_4_BRB2.
	Register(s) crtc_data_dl1_r_5 has(ve) been backward balanced into : crtc_data_dl1_r_5_BRB2.
	Register(s) crtc_data_dl1_r_6 has(ve) been backward balanced into : crtc_data_dl1_r_6_BRB2.
	Register(s) crtc_data_dl1_r_7 has(ve) been backward balanced into : crtc_data_dl1_r_7_BRB2.
	Register(s) crtc_data_dl1_r_8 has(ve) been backward balanced into : crtc_data_dl1_r_8_BRB2.
	Register(s) crtc_data_dl1_r_9 has(ve) been backward balanced into : crtc_data_dl1_r_9_BRB2.
	Register(s) crtc_data_dl2_r_0 has(ve) been backward balanced into : crtc_data_dl2_r_0_BRB0 crtc_data_dl2_r_0_BRB2 crtc_data_dl2_r_0_BRB3 crtc_data_dl2_r_0_BRB4.
	Register(s) crtc_data_dl2_r_1 has(ve) been backward balanced into : crtc_data_dl2_r_1_BRB3.
	Register(s) crtc_data_dl2_r_10 has(ve) been backward balanced into : crtc_data_dl2_r_10_BRB3.
	Register(s) crtc_data_dl2_r_11 has(ve) been backward balanced into : crtc_data_dl2_r_11_BRB3.
	Register(s) crtc_data_dl2_r_12 has(ve) been backward balanced into : crtc_data_dl2_r_12_BRB3.
	Register(s) crtc_data_dl2_r_13 has(ve) been backward balanced into : crtc_data_dl2_r_13_BRB3.
	Register(s) crtc_data_dl2_r_14 has(ve) been backward balanced into : crtc_data_dl2_r_14_BRB3.
	Register(s) crtc_data_dl2_r_15 has(ve) been backward balanced into : crtc_data_dl2_r_15_BRB3.
	Register(s) crtc_data_dl2_r_16 has(ve) been backward balanced into : crtc_data_dl2_r_16_BRB3.
	Register(s) crtc_data_dl2_r_17 has(ve) been backward balanced into : crtc_data_dl2_r_17_BRB3.
	Register(s) crtc_data_dl2_r_18 has(ve) been backward balanced into : crtc_data_dl2_r_18_BRB3.
	Register(s) crtc_data_dl2_r_19 has(ve) been backward balanced into : crtc_data_dl2_r_19_BRB3.
	Register(s) crtc_data_dl2_r_2 has(ve) been backward balanced into : crtc_data_dl2_r_2_BRB3.
	Register(s) crtc_data_dl2_r_20 has(ve) been backward balanced into : crtc_data_dl2_r_20_BRB3.
	Register(s) crtc_data_dl2_r_21 has(ve) been backward balanced into : crtc_data_dl2_r_21_BRB3.
	Register(s) crtc_data_dl2_r_22 has(ve) been backward balanced into : crtc_data_dl2_r_22_BRB3.
	Register(s) crtc_data_dl2_r_23 has(ve) been backward balanced into : crtc_data_dl2_r_23_BRB3.
	Register(s) crtc_data_dl2_r_3 has(ve) been backward balanced into : crtc_data_dl2_r_3_BRB3.
	Register(s) crtc_data_dl2_r_4 has(ve) been backward balanced into : crtc_data_dl2_r_4_BRB3.
	Register(s) crtc_data_dl2_r_5 has(ve) been backward balanced into : crtc_data_dl2_r_5_BRB3.
	Register(s) crtc_data_dl2_r_6 has(ve) been backward balanced into : crtc_data_dl2_r_6_BRB3.
	Register(s) crtc_data_dl2_r_7 has(ve) been backward balanced into : crtc_data_dl2_r_7_BRB3.
	Register(s) crtc_data_dl2_r_8 has(ve) been backward balanced into : crtc_data_dl2_r_8_BRB3.
	Register(s) crtc_data_dl2_r_9 has(ve) been backward balanced into : crtc_data_dl2_r_9_BRB3.
	Register(s) crtc_data_dl3_r_0 has(ve) been backward balanced into : crtc_data_dl3_r_0_BRB0 crtc_data_dl3_r_0_BRB1.
	Register(s) crtc_data_dl3_r_1 has(ve) been backward balanced into : crtc_data_dl3_r_1_BRB1.
	Register(s) crtc_data_dl3_r_10 has(ve) been backward balanced into : crtc_data_dl3_r_10_BRB1.
	Register(s) crtc_data_dl3_r_11 has(ve) been backward balanced into : crtc_data_dl3_r_11_BRB1.
	Register(s) crtc_data_dl3_r_12 has(ve) been backward balanced into : crtc_data_dl3_r_12_BRB1.
	Register(s) crtc_data_dl3_r_13 has(ve) been backward balanced into : crtc_data_dl3_r_13_BRB1.
	Register(s) crtc_data_dl3_r_14 has(ve) been backward balanced into : crtc_data_dl3_r_14_BRB1.
	Register(s) crtc_data_dl3_r_15 has(ve) been backward balanced into : crtc_data_dl3_r_15_BRB1.
	Register(s) crtc_data_dl3_r_16 has(ve) been backward balanced into : crtc_data_dl3_r_16_BRB1.
	Register(s) crtc_data_dl3_r_17 has(ve) been backward balanced into : crtc_data_dl3_r_17_BRB1.
	Register(s) crtc_data_dl3_r_18 has(ve) been backward balanced into : crtc_data_dl3_r_18_BRB1.
	Register(s) crtc_data_dl3_r_19 has(ve) been backward balanced into : crtc_data_dl3_r_19_BRB1.
	Register(s) crtc_data_dl3_r_2 has(ve) been backward balanced into : crtc_data_dl3_r_2_BRB1.
	Register(s) crtc_data_dl3_r_20 has(ve) been backward balanced into : crtc_data_dl3_r_20_BRB1.
	Register(s) crtc_data_dl3_r_21 has(ve) been backward balanced into : crtc_data_dl3_r_21_BRB1.
	Register(s) crtc_data_dl3_r_22 has(ve) been backward balanced into : crtc_data_dl3_r_22_BRB1.
	Register(s) crtc_data_dl3_r_23 has(ve) been backward balanced into : crtc_data_dl3_r_23_BRB1.
	Register(s) crtc_data_dl3_r_3 has(ve) been backward balanced into : crtc_data_dl3_r_3_BRB1.
	Register(s) crtc_data_dl3_r_4 has(ve) been backward balanced into : crtc_data_dl3_r_4_BRB1.
	Register(s) crtc_data_dl3_r_5 has(ve) been backward balanced into : crtc_data_dl3_r_5_BRB1.
	Register(s) crtc_data_dl3_r_6 has(ve) been backward balanced into : crtc_data_dl3_r_6_BRB1.
	Register(s) crtc_data_dl3_r_7 has(ve) been backward balanced into : crtc_data_dl3_r_7_BRB1.
	Register(s) crtc_data_dl3_r_8 has(ve) been backward balanced into : crtc_data_dl3_r_8_BRB1.
	Register(s) crtc_data_dl3_r_9 has(ve) been backward balanced into : crtc_data_dl3_r_9_BRB1.
Unit <crtc2> processed.

Processing Unit <dp_main/dp_main_linkup> :
	Register(s) hpd_r_4 has(ve) been backward balanced into : hpd_r_4_BRB0 hpd_r_4_BRB1.
	Register(s) hpd_r_5 has(ve) been backward balanced into : hpd_r_5_BRB0 hpd_r_5_BRB1.
Unit <dp_main/dp_main_linkup> processed.

Processing Unit <dp_main/dp_main_scramble> :
	Register(s) sc_data0_out0_r_0 has(ve) been backward balanced into : sc_data0_out0_r_0_BRB0 sc_data0_out0_r_0_BRB1 sc_data0_out0_r_0_BRB2 sc_data0_out0_r_0_BRB3.
	Register(s) sc_data0_out0_r_1 has(ve) been backward balanced into : sc_data0_out0_r_1_BRB2 sc_data0_out0_r_1_BRB3.
	Register(s) sc_data0_out0_r_10 has(ve) been backward balanced into : sc_data0_out0_r_10_BRB0 .
	Register(s) sc_data0_out0_r_2 has(ve) been backward balanced into : sc_data0_out0_r_2_BRB0 sc_data0_out0_r_2_BRB1 sc_data0_out0_r_2_BRB2 sc_data0_out0_r_2_BRB3 sc_data0_out0_r_2_BRB4.
	Register(s) sc_data0_out0_r_3 has(ve) been backward balanced into : sc_data0_out0_r_3_BRB2 sc_data0_out0_r_3_BRB4.
	Register(s) sc_data0_out0_r_4 has(ve) been backward balanced into : sc_data0_out0_r_4_BRB2 .
	Register(s) sc_data0_out0_r_5 has(ve) been backward balanced into : sc_data0_out0_r_5_BRB2 sc_data0_out0_r_5_BRB3 .
	Register(s) sc_data0_out0_r_6 has(ve) been backward balanced into : sc_data0_out0_r_6_BRB2 .
	Register(s) sc_data0_out0_r_7 has(ve) been backward balanced into : sc_data0_out0_r_7_BRB2 sc_data0_out0_r_7_BRB4.
	Register(s) sc_data0_out0_r_8 has(ve) been backward balanced into : sc_data0_out0_r_8_BRB2 .
	Register(s) sc_data0_out0_r_9 has(ve) been backward balanced into : sc_data0_out0_r_9_BRB1 sc_data0_out0_r_9_BRB2 sc_data0_out0_r_9_BRB3 sc_data0_out0_r_9_BRB4 sc_data0_out0_r_9_BRB5 sc_data0_out0_r_9_BRB6.
	Register(s) sc_data0_out1_r_10 has(ve) been backward balanced into : sc_data0_out1_r_10_BRB0 .
	Register(s) sc_data0_out1_r_9 has(ve) been backward balanced into : sc_data0_out1_r_9_BRB0 sc_data0_out1_r_9_BRB1.
	Register(s) sc_no_8k512_r has(ve) been backward balanced into : sc_no_8k512_r_BRB0 sc_no_8k512_r_BRB1 sc_no_8k512_r_BRB2 sc_no_8k512_r_BRB3 sc_no_8k512_r_BRB4 sc_no_8k512_r_BRB5.
	Register(s) sc_no_data_out_r_5 has(ve) been backward balanced into : sc_no_data_out_r_5_BRB0 sc_no_data_out_r_5_BRB1.
	Register(s) sc_tr_data_out_r_0 has(ve) been backward balanced into : sc_tr_data_out_r_0_BRB0 sc_tr_data_out_r_0_BRB2 .
	Register(s) sc_tr_data_out_r_1 has(ve) been backward balanced into : sc_tr_data_out_r_1_BRB0 sc_tr_data_out_r_1_BRB1 sc_tr_data_out_r_1_BRB2 sc_tr_data_out_r_1_BRB3.
	Register(s) sc_tr_data_out_r_7 has(ve) been backward balanced into : sc_tr_data_out_r_7_BRB1 sc_tr_data_out_r_7_BRB2.
	Register(s) sc_tr_data_out_r_9 has(ve) been backward balanced into : sc_tr_data_out_r_9_BRB2 .
Unit <dp_main/dp_main_scramble> processed.

Processing Unit <crtc1> :
	Register(s) crtc_ctrl_dl0_r_1 has(ve) been backward balanced into : crtc_ctrl_dl0_r_1_BRB0 crtc_ctrl_dl0_r_1_BRB1 crtc_ctrl_dl0_r_1_BRB2 crtc_ctrl_dl0_r_1_BRB3 crtc_ctrl_dl0_r_1_BRB5 crtc_ctrl_dl0_r_1_BRB6 crtc_ctrl_dl0_r_1_BRB7.
	Register(s) crtc_ctrl_dl1_r_1 has(ve) been backward balanced into : crtc_ctrl_dl1_r_1_BRB0 crtc_ctrl_dl1_r_1_BRB1 crtc_ctrl_dl1_r_1_BRB2 crtc_ctrl_dl1_r_1_BRB3 crtc_ctrl_dl1_r_1_BRB5 crtc_ctrl_dl1_r_1_BRB6 crtc_ctrl_dl1_r_1_BRB7.
	Register(s) crtc_ctrl_dl2_r_1 has(ve) been backward balanced into : crtc_ctrl_dl2_r_1_BRB0 crtc_ctrl_dl2_r_1_BRB1 crtc_ctrl_dl2_r_1_BRB2 crtc_ctrl_dl2_r_1_BRB3 crtc_ctrl_dl2_r_1_BRB4 crtc_ctrl_dl2_r_1_BRB5.
	Register(s) crtc_data_dl1_r_0 has(ve) been backward balanced into : crtc_data_dl1_r_0_BRB1 crtc_data_dl1_r_0_BRB2.
	Register(s) crtc_data_dl1_r_1 has(ve) been backward balanced into : crtc_data_dl1_r_1_BRB2.
	Register(s) crtc_data_dl1_r_10 has(ve) been backward balanced into : crtc_data_dl1_r_10_BRB2.
	Register(s) crtc_data_dl1_r_11 has(ve) been backward balanced into : crtc_data_dl1_r_11_BRB2.
	Register(s) crtc_data_dl1_r_12 has(ve) been backward balanced into : crtc_data_dl1_r_12_BRB2.
	Register(s) crtc_data_dl1_r_13 has(ve) been backward balanced into : crtc_data_dl1_r_13_BRB2.
	Register(s) crtc_data_dl1_r_14 has(ve) been backward balanced into : crtc_data_dl1_r_14_BRB2.
	Register(s) crtc_data_dl1_r_15 has(ve) been backward balanced into : crtc_data_dl1_r_15_BRB2.
	Register(s) crtc_data_dl1_r_16 has(ve) been backward balanced into : crtc_data_dl1_r_16_BRB2.
	Register(s) crtc_data_dl1_r_17 has(ve) been backward balanced into : crtc_data_dl1_r_17_BRB2.
	Register(s) crtc_data_dl1_r_18 has(ve) been backward balanced into : crtc_data_dl1_r_18_BRB2.
	Register(s) crtc_data_dl1_r_19 has(ve) been backward balanced into : crtc_data_dl1_r_19_BRB2.
	Register(s) crtc_data_dl1_r_2 has(ve) been backward balanced into : crtc_data_dl1_r_2_BRB2.
	Register(s) crtc_data_dl1_r_20 has(ve) been backward balanced into : crtc_data_dl1_r_20_BRB2.
	Register(s) crtc_data_dl1_r_21 has(ve) been backward balanced into : crtc_data_dl1_r_21_BRB2.
	Register(s) crtc_data_dl1_r_22 has(ve) been backward balanced into : crtc_data_dl1_r_22_BRB2.
	Register(s) crtc_data_dl1_r_23 has(ve) been backward balanced into : crtc_data_dl1_r_23_BRB2.
	Register(s) crtc_data_dl1_r_3 has(ve) been backward balanced into : crtc_data_dl1_r_3_BRB2.
	Register(s) crtc_data_dl1_r_4 has(ve) been backward balanced into : crtc_data_dl1_r_4_BRB2.
	Register(s) crtc_data_dl1_r_5 has(ve) been backward balanced into : crtc_data_dl1_r_5_BRB2.
	Register(s) crtc_data_dl1_r_6 has(ve) been backward balanced into : crtc_data_dl1_r_6_BRB2.
	Register(s) crtc_data_dl1_r_7 has(ve) been backward balanced into : crtc_data_dl1_r_7_BRB2.
	Register(s) crtc_data_dl1_r_8 has(ve) been backward balanced into : crtc_data_dl1_r_8_BRB2.
	Register(s) crtc_data_dl1_r_9 has(ve) been backward balanced into : crtc_data_dl1_r_9_BRB2.
	Register(s) crtc_data_dl2_r_0 has(ve) been backward balanced into : crtc_data_dl2_r_0_BRB0 crtc_data_dl2_r_0_BRB2 crtc_data_dl2_r_0_BRB3 crtc_data_dl2_r_0_BRB4.
	Register(s) crtc_data_dl2_r_1 has(ve) been backward balanced into : crtc_data_dl2_r_1_BRB3.
	Register(s) crtc_data_dl2_r_10 has(ve) been backward balanced into : crtc_data_dl2_r_10_BRB3.
	Register(s) crtc_data_dl2_r_11 has(ve) been backward balanced into : crtc_data_dl2_r_11_BRB3.
	Register(s) crtc_data_dl2_r_12 has(ve) been backward balanced into : crtc_data_dl2_r_12_BRB3.
	Register(s) crtc_data_dl2_r_13 has(ve) been backward balanced into : crtc_data_dl2_r_13_BRB3.
	Register(s) crtc_data_dl2_r_14 has(ve) been backward balanced into : crtc_data_dl2_r_14_BRB3.
	Register(s) crtc_data_dl2_r_15 has(ve) been backward balanced into : crtc_data_dl2_r_15_BRB3.
	Register(s) crtc_data_dl2_r_16 has(ve) been backward balanced into : crtc_data_dl2_r_16_BRB3.
	Register(s) crtc_data_dl2_r_17 has(ve) been backward balanced into : crtc_data_dl2_r_17_BRB3.
	Register(s) crtc_data_dl2_r_18 has(ve) been backward balanced into : crtc_data_dl2_r_18_BRB3.
	Register(s) crtc_data_dl2_r_19 has(ve) been backward balanced into : crtc_data_dl2_r_19_BRB3.
	Register(s) crtc_data_dl2_r_2 has(ve) been backward balanced into : crtc_data_dl2_r_2_BRB3.
	Register(s) crtc_data_dl2_r_20 has(ve) been backward balanced into : crtc_data_dl2_r_20_BRB3.
	Register(s) crtc_data_dl2_r_21 has(ve) been backward balanced into : crtc_data_dl2_r_21_BRB3.
	Register(s) crtc_data_dl2_r_22 has(ve) been backward balanced into : crtc_data_dl2_r_22_BRB3.
	Register(s) crtc_data_dl2_r_23 has(ve) been backward balanced into : crtc_data_dl2_r_23_BRB3.
	Register(s) crtc_data_dl2_r_3 has(ve) been backward balanced into : crtc_data_dl2_r_3_BRB3.
	Register(s) crtc_data_dl2_r_4 has(ve) been backward balanced into : crtc_data_dl2_r_4_BRB3.
	Register(s) crtc_data_dl2_r_5 has(ve) been backward balanced into : crtc_data_dl2_r_5_BRB3.
	Register(s) crtc_data_dl2_r_6 has(ve) been backward balanced into : crtc_data_dl2_r_6_BRB3.
	Register(s) crtc_data_dl2_r_7 has(ve) been backward balanced into : crtc_data_dl2_r_7_BRB3.
	Register(s) crtc_data_dl2_r_8 has(ve) been backward balanced into : crtc_data_dl2_r_8_BRB3.
	Register(s) crtc_data_dl2_r_9 has(ve) been backward balanced into : crtc_data_dl2_r_9_BRB3.
	Register(s) crtc_data_dl3_r_0 has(ve) been backward balanced into : crtc_data_dl3_r_0_BRB0 crtc_data_dl3_r_0_BRB1.
	Register(s) crtc_data_dl3_r_1 has(ve) been backward balanced into : crtc_data_dl3_r_1_BRB1.
	Register(s) crtc_data_dl3_r_10 has(ve) been backward balanced into : crtc_data_dl3_r_10_BRB1.
	Register(s) crtc_data_dl3_r_11 has(ve) been backward balanced into : crtc_data_dl3_r_11_BRB1.
	Register(s) crtc_data_dl3_r_12 has(ve) been backward balanced into : crtc_data_dl3_r_12_BRB1.
	Register(s) crtc_data_dl3_r_13 has(ve) been backward balanced into : crtc_data_dl3_r_13_BRB1.
	Register(s) crtc_data_dl3_r_14 has(ve) been backward balanced into : crtc_data_dl3_r_14_BRB1.
	Register(s) crtc_data_dl3_r_15 has(ve) been backward balanced into : crtc_data_dl3_r_15_BRB1.
	Register(s) crtc_data_dl3_r_16 has(ve) been backward balanced into : crtc_data_dl3_r_16_BRB1.
	Register(s) crtc_data_dl3_r_17 has(ve) been backward balanced into : crtc_data_dl3_r_17_BRB1.
	Register(s) crtc_data_dl3_r_18 has(ve) been backward balanced into : crtc_data_dl3_r_18_BRB1.
	Register(s) crtc_data_dl3_r_19 has(ve) been backward balanced into : crtc_data_dl3_r_19_BRB1.
	Register(s) crtc_data_dl3_r_2 has(ve) been backward balanced into : crtc_data_dl3_r_2_BRB1.
	Register(s) crtc_data_dl3_r_20 has(ve) been backward balanced into : crtc_data_dl3_r_20_BRB1.
	Register(s) crtc_data_dl3_r_21 has(ve) been backward balanced into : crtc_data_dl3_r_21_BRB1.
	Register(s) crtc_data_dl3_r_22 has(ve) been backward balanced into : crtc_data_dl3_r_22_BRB1.
	Register(s) crtc_data_dl3_r_23 has(ve) been backward balanced into : crtc_data_dl3_r_23_BRB1.
	Register(s) crtc_data_dl3_r_3 has(ve) been backward balanced into : crtc_data_dl3_r_3_BRB1.
	Register(s) crtc_data_dl3_r_4 has(ve) been backward balanced into : crtc_data_dl3_r_4_BRB1.
	Register(s) crtc_data_dl3_r_5 has(ve) been backward balanced into : crtc_data_dl3_r_5_BRB1.
	Register(s) crtc_data_dl3_r_6 has(ve) been backward balanced into : crtc_data_dl3_r_6_BRB1.
	Register(s) crtc_data_dl3_r_7 has(ve) been backward balanced into : crtc_data_dl3_r_7_BRB1.
	Register(s) crtc_data_dl3_r_8 has(ve) been backward balanced into : crtc_data_dl3_r_8_BRB1.
	Register(s) crtc_data_dl3_r_9 has(ve) been backward balanced into : crtc_data_dl3_r_9_BRB1.
	Register(s) crtc_vsync_r has(ve) been backward balanced into : crtc_vsync_r_BRB0 crtc_vsync_r_BRB1 crtc_vsync_r_BRB2 crtc_vsync_r_BRB3 crtc_vsync_r_BRB5 crtc_vsync_r_BRB6 crtc_vsync_r_BRB7.
Unit <crtc1> processed.

Processing Unit <tx_dvi> :
	Register(s) tx0_r_0 has(ve) been backward balanced into : tx0_r_0_BRB1 tx0_r_0_BRB2.
	Register(s) tx0_r_1 has(ve) been backward balanced into : tx0_r_1_BRB1 tx0_r_1_BRB2.
	Register(s) tx0_r_2 has(ve) been backward balanced into : tx0_r_2_BRB1 tx0_r_2_BRB2.
	Register(s) tx0_r_3 has(ve) been backward balanced into : tx0_r_3_BRB1 tx0_r_3_BRB2.
	Register(s) tx0_r_4 has(ve) been backward balanced into : tx0_r_4_BRB1 tx0_r_4_BRB2.
	Register(s) tx0_r_5 has(ve) been backward balanced into : tx0_r_5_BRB1 tx0_r_5_BRB2.
	Register(s) tx0_r_6 has(ve) been backward balanced into : tx0_r_6_BRB1 tx0_r_6_BRB2.
	Register(s) tx0_r_7 has(ve) been backward balanced into : tx0_r_7_BRB1 tx0_r_7_BRB2.
	Register(s) tx0_r_8 has(ve) been backward balanced into : tx0_r_8_BRB1.
	Register(s) tx0_r_9 has(ve) been backward balanced into : tx0_r_9_BRB1.
	Register(s) tx1_r_0 has(ve) been backward balanced into : tx1_r_0_BRB1 tx1_r_0_BRB2.
	Register(s) tx1_r_1 has(ve) been backward balanced into : tx1_r_1_BRB1 tx1_r_1_BRB2.
	Register(s) tx1_r_2 has(ve) been backward balanced into : tx1_r_2_BRB1 tx1_r_2_BRB2.
	Register(s) tx1_r_3 has(ve) been backward balanced into : tx1_r_3_BRB1 tx1_r_3_BRB2.
	Register(s) tx1_r_4 has(ve) been backward balanced into : tx1_r_4_BRB1 tx1_r_4_BRB2.
	Register(s) tx1_r_5 has(ve) been backward balanced into : tx1_r_5_BRB1 tx1_r_5_BRB2.
	Register(s) tx1_r_6 has(ve) been backward balanced into : tx1_r_6_BRB1 tx1_r_6_BRB2.
	Register(s) tx1_r_7 has(ve) been backward balanced into : tx1_r_7_BRB1 tx1_r_7_BRB2.
	Register(s) tx1_r_8 has(ve) been backward balanced into : tx1_r_8_BRB1.
	Register(s) tx1_r_9 has(ve) been backward balanced into : tx1_r_9_BRB1.
	Register(s) tx2_r_0 has(ve) been backward balanced into : tx2_r_0_BRB1 tx2_r_0_BRB2.
	Register(s) tx2_r_1 has(ve) been backward balanced into : tx2_r_1_BRB1 tx2_r_1_BRB2.
	Register(s) tx2_r_2 has(ve) been backward balanced into : tx2_r_2_BRB1 tx2_r_2_BRB2.
	Register(s) tx2_r_3 has(ve) been backward balanced into : tx2_r_3_BRB1 tx2_r_3_BRB2.
	Register(s) tx2_r_4 has(ve) been backward balanced into : tx2_r_4_BRB1 tx2_r_4_BRB2.
	Register(s) tx2_r_5 has(ve) been backward balanced into : tx2_r_5_BRB1 tx2_r_5_BRB2.
	Register(s) tx2_r_6 has(ve) been backward balanced into : tx2_r_6_BRB1 tx2_r_6_BRB2.
	Register(s) tx2_r_7 has(ve) been backward balanced into : tx2_r_7_BRB1 tx2_r_7_BRB2.
	Register(s) tx2_r_8 has(ve) been backward balanced into : tx2_r_8_BRB1.
	Register(s) tx2_r_9 has(ve) been backward balanced into : tx2_r_9_BRB1.
	Register(s) tx3_r_1 has(ve) been backward balanced into : tx3_r_1_BRB1.
	Register(s) tx_req_r_3 has(ve) been backward balanced into : tx_req_r_3_BRB0 tx_req_r_3_BRB1.
Unit <tx_dvi> processed.
FlipFlop memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/gen_term_calib.mcb_soft_calibration_top_inst/mcb_soft_calibration_inst/Pre_SYSRST has been replicated 2 time(s)

Final Macro Processing ...

Processing Unit <crtc1> :
	Found 4-bit shift register for signal <crtc_ctrl_dl3_r_0>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_0_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_0_BRB4>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_1_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_2_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_3_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_4_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_5_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_6_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_7_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_8_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_9_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_10_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_11_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_12_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_13_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_14_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_15_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_16_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_17_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_18_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_19_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_20_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_21_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_22_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_23_BRB3>.
	Found 3-bit shift register for signal <crtc_ctrl_dl2_r_1_BRB1>.
	Found 3-bit shift register for signal <crtc_ctrl_dl2_r_1_BRB2>.
	Found 3-bit shift register for signal <crtc_ctrl_dl2_r_1_BRB3>.
	Found 3-bit shift register for signal <crtc_ctrl_dl2_r_1_BRB5>.
	Found 2-bit shift register for signal <crtc_ctrl_dl1_r_1_BRB6>.
	Found 2-bit shift register for signal <crtc_ctrl_dl1_r_1_BRB7>.
Unit <crtc1> processed.

Processing Unit <crtc2> :
	Found 4-bit shift register for signal <crtc_ctrl_dl3_r_0>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_0_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_0_BRB4>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_1_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_2_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_3_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_4_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_5_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_6_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_7_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_8_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_9_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_10_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_11_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_12_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_13_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_14_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_15_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_16_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_17_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_18_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_19_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_20_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_21_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_22_BRB3>.
	Found 2-bit shift register for signal <crtc_data_dl2_r_23_BRB3>.
Unit <crtc2> processed.

Processing Unit <dp_main_linkup> :
	Found 2-bit shift register for signal <hpd_r_5_BRB1>.
Unit <dp_main_linkup> processed.

Processing Unit <dp_main_scramble> :
	Found 2-bit shift register for signal <sc_data0_out1_r_9_BRB1>.
	Found 2-bit shift register for signal <sc_data0_out0_r_9_BRB4>.
Unit <dp_main_scramble> processed.

Processing Unit <mcb_soft_calibration_inst> :
	Found 2-bit shift register for signal <SELFREFRESH_MCB_MODE_R2>.
	Found 2-bit shift register for signal <PLL_LOCK_R2>.
Unit <mcb_soft_calibration_inst> processed.

=========================================================================
Final Register Report

Macro Statistics
# Registers                                            : 3412
 Flip-Flops                                            : 3412
# Shift Registers                                      : 63
 2-bit shift register                                  : 57
 3-bit shift register                                  : 4
 4-bit shift register                                  : 2

=========================================================================

=========================================================================
*                           Partition Report                            *
=========================================================================

Partition Implementation Status
-------------------------------

  No Partitions were found in this design.

-------------------------------

=========================================================================
*                            Design Summary                             *
=========================================================================

Top Level Output File Name         : exp6t_disp.ngc

Primitive and Black Box Usage:
------------------------------
# BELS                             : 5034
#      GND                         : 30
#      INV                         : 68
#      LUT1                        : 172
#      LUT2                        : 746
#      LUT3                        : 717
#      LUT4                        : 452
#      LUT5                        : 869
#      LUT6                        : 1086
#      MULT_AND                    : 7
#      MUXCY                       : 367
#      MUXF7                       : 100
#      VCC                         : 22
#      XORCY                       : 398
# FlipFlops/Latches                : 3488
#      FD                          : 90
#      FDC                         : 1736
#      FDCE                        : 1009
#      FDDRRSE                     : 5
#      FDE                         : 122
#      FDP                         : 100
#      FDPE                        : 7
#      FDR                         : 171
#      FDRE                        : 236
#      FDS                         : 7
#      FDSE                        : 5
# RAMS                             : 11
#      RAMB16BWER                  : 11
# Shift Registers                  : 63
#      SRLC16E                     : 63
# Clock Buffers                    : 15
#      BUFG                        : 15
# IO Buffers                       : 101
#      BUFIO2                      : 2
#      IBUF                        : 10
#      IBUFDS                      : 3
#      IBUFG                       : 3
#      IOBUF                       : 18
#      IOBUFDS                     : 2
#      OBUF                        : 35
#      OBUFDS                      : 4
#      OBUFT                       : 22
#      OBUFTDS                     : 2
# DCMs                             : 2
#      DCM_SP                      : 2
# GigabitIOs                       : 2
#      GTPA1_DUAL                  : 2
# Others                           : 77
#      BUFPLL_MCB                  : 1
#      IODRP2                      : 2
#      IODRP2_MCB                  : 22
#      MCB                         : 1
#      OSERDES2                    : 43
#      PCIE_A1                     : 1
#      PLL_ADV                     : 3
#      PULLDOWN                    : 2
#      PULLUP                      : 2

Device utilization summary:
---------------------------

Selected Device : 6slx45tfgg484-3 


Slice Logic Utilization: 
 Number of Slice Registers:            3488  out of  54576     6%  
 Number of Slice LUTs:                 4173  out of  27288    15%  
    Number used as Logic:              4110  out of  27288    15%  
    Number used as Memory:               63  out of   6408     0%  
       Number used as SRL:               63

Slice Logic Distribution: 
 Number of LUT Flip Flop pairs used:   4915
   Number with an unused Flip Flop:    1427  out of   4915    29%  
   Number with an unused LUT:           742  out of   4915    15%  
   Number of fully used LUT-FF pairs:  2746  out of   4915    55%  
   Number of unique control sets:       168

IO Utilization: 
 Number of IOs:                         184
 Number of bonded IOBs:                 107  out of    296    36%  

Specific Feature Utilization:
 Number of Block RAM/FIFO:               11  out of    116     9%  
    Number using Block RAM only:         11
 Number of BUFG/BUFGCTRLs:               15  out of     16    93%  
 Number of PLL_ADVs:                      3  out of      4    75%  

---------------------------
Partition Resource Summary:
---------------------------

  No Partitions were found in this design.

---------------------------


=========================================================================
Timing Report

NOTE: THESE TIMING NUMBERS ARE ONLY A SYNTHESIS ESTIMATE.
      FOR ACCURATE TIMING INFORMATION PLEASE REFER TO THE TRACE REPORT
      GENERATED AFTER PLACE-and-ROUTE.

Clock Information:
------------------
--------------------------------------------+------------------------------------+-------+
Clock Signal                                | Clock buffer(FF name)              | Load  |
--------------------------------------------+------------------------------------+-------+
DP_CLK0                                     | IBUFG                              | 226   |
inst_sp6wrap/eptest_i/pll_base_i/CLKOUT2    | BUFG                               | 726   |
xtalclk                                     | dcm_sp_inst:CLKFX+u_pll_adv:CLKOUT3| 239   |
GTPCLKOUT1_DCM                              | BUFG                               | 1803  |
xtalclk                                     | dcm_sp_inst:CLKFX+u_pll_adv:CLKOUT2| 152   |
clk_wiz_v1_6_50x62x312/pll_base_inst/CLKOUT0| BUFG                               | 348   |
clk_wiz_v1_6_50x62x312/pll_base_inst/CLKOUT1| BUFG                               | 77    |
--------------------------------------------+------------------------------------+-------+

Asynchronous Control Signals Information:
----------------------------------------
No asynchronous control signals found in this design

Timing Summary:
---------------
Speed Grade: -3

   Minimum period: 23.986ns (Maximum Frequency: 41.692MHz)
   Minimum input arrival time before clock: 6.913ns
   Maximum output required time after clock: 5.789ns
   Maximum combinational path delay: 5.853ns

Timing Details:
---------------
All values displayed in nanoseconds (ns)

=========================================================================
Timing constraint: Default period analysis for Clock 'DP_CLK0'
  Clock period: 8.327ns (frequency: 120.087MHz)
  Total number of paths / destination ports: 4231 / 314
-------------------------------------------------------------------------
Delay:               8.327ns (Levels of Logic = 6)
  Source:            dp_main/aux_tx/aux_state_r_FSM_FFd3 (FF)
  Destination:       dp_main/aux_tx/aux_count_r_0 (FF)
  Source Clock:      DP_CLK0 rising
  Destination Clock: DP_CLK0 rising

  Data Path: dp_main/aux_tx/aux_state_r_FSM_FFd3 to dp_main/aux_tx/aux_count_r_0
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDC:C->Q             76   0.525   1.947  aux_state_r_FSM_FFd3 (aux_state_r_FSM_FFd3)
     LUT3:I0->O            3   0.235   1.081  Mmux_n07923151 (N283)
     LUT6:I1->O            1   0.254   0.688  Mmux_aux_count_w1513 (Mmux_aux_count_w1512)
     LUT6:I4->O            1   0.250   1.010  Mmux_aux_count_w1516 (Mmux_aux_count_w1515)
     LUT6:I1->O            1   0.254   0.579  Mmux_aux_count_w1517 (Mmux_aux_count_w1516)
     MUXF7:S->O            5   0.185   0.991  Mmux_aux_count_w1518 (N119)
     LUT5:I1->O            1   0.254   0.000  Mmux_aux_count_w201 (aux_count_w<4>)
     FDCE:D                    0.074          aux_count_r_4
    ----------------------------------------
    Total                      8.327ns (2.031ns logic, 6.296ns route)
                                       (24.4% logic, 75.6% route)

=========================================================================
Timing constraint: Default period analysis for Clock 'inst_sp6wrap/eptest_i/pll_base_i/CLKOUT2'
  Clock period: 8.185ns (frequency: 122.181MHz)
  Total number of paths / destination ports: 8291 / 902
-------------------------------------------------------------------------
Delay:               8.185ns (Levels of Logic = 5)
  Source:            inst_sp6wrap/app/PIO/PIO_EP/EP_RX/state_3 (FF)
  Destination:       inst_sp6wrap/app/PIO/PIO_EP/EP_RX/state_3 (FF)
  Source Clock:      inst_sp6wrap/eptest_i/pll_base_i/CLKOUT2 rising
  Destination Clock: inst_sp6wrap/eptest_i/pll_base_i/CLKOUT2 rising

  Data Path: inst_sp6wrap/app/PIO/PIO_EP/EP_RX/state_3 to inst_sp6wrap/app/PIO/PIO_EP/EP_RX/state_3
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDR:C->Q             56   0.525   1.816  state_3 (state_3)
     LUT3:I0->O            6   0.235   1.175  state[3]_tlp_type[6]_AND_43_o111 (N99)
     LUT5:I0->O            2   0.254   1.072  state[3]_trn_rsof_n_AND_38_o1 (state[3]_trn_rsof_n_AND_38_o)
     LUT6:I0->O            2   0.254   1.072  Mmux_n03569213 (N58)
     LUT6:I0->O            6   0.254   1.200  Mmux_n035692 (N45)
     LUT6:I0->O            1   0.254   0.000  Mmux_n03568 (state_next<3>)
     FDR:D                     0.074          state_3
    ----------------------------------------
    Total                      8.185ns (1.850ns logic, 6.335ns route)
                                       (22.6% logic, 77.4% route)

=========================================================================
Timing constraint: Default period analysis for Clock 'xtalclk'
  Clock period: 23.986ns (frequency: 41.692MHz)
  Total number of paths / destination ports: 33062 / 863
-------------------------------------------------------------------------
Delay:               5.996ns (Levels of Logic = 6)
  Source:            memc3_infrastructure_inst/powerup_pll_locked (FF)
  Destination:       memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/gen_term_calib.mcb_soft_calibration_top_inst/mcb_soft_calibration_inst/RST_reg (FF)
  Source Clock:      xtalclk rising 4.0X
  Destination Clock: xtalclk rising

  Data Path: memc3_infrastructure_inst/powerup_pll_locked to memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/gen_term_calib.mcb_soft_calibration_top_inst/mcb_soft_calibration_inst/RST_reg
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDCE:C->Q             2   0.525   0.617  powerup_pll_locked (powerup_pll_locked)
     LUT2:I1->O           76   0.254   1.719  rst_tmp1_1 (async_rst)
     end scope: 'memc3_infrastructure_inst'
     begin scope: 'memc3_wrapper_inst'
     begin scope: 'memc3_mcb_raw_wrapper_inst'
     LUT2:I1->O           35   0.254   1.335  int_sys_rst1_1 (int_sys_rst_0)
     begin scope: 'gen_term_calib.mcb_soft_calibration_top_inst'
     begin scope: 'mcb_soft_calibration_inst'
     LUT2:I1->O            1   0.254   0.579  non_violating_rst1 (non_violating_rst)
     FDP:PRE                   0.459          RST_reg
    ----------------------------------------
    Total                      5.996ns (1.746ns logic, 4.250ns route)
                                       (29.1% logic, 70.9% route)

=========================================================================
Timing constraint: Default period analysis for Clock 'GTPCLKOUT1_DCM'
  Clock period: 6.311ns (frequency: 158.445MHz)
  Total number of paths / destination ports: 12442 / 2708
-------------------------------------------------------------------------
Delay:               6.311ns (Levels of Logic = 3)
  Source:            dp_main/dp_main_tbc/tbc_state_r_FSM_FFd3 (FF)
  Destination:       dp_main/dp_main_tbc/tbc_rd_data03_r_0 (FF)
  Source Clock:      GTPCLKOUT1_DCM rising
  Destination Clock: GTPCLKOUT1_DCM rising

  Data Path: dp_main/dp_main_tbc/tbc_state_r_FSM_FFd3 to dp_main/dp_main_tbc/tbc_rd_data03_r_0
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDC:C->Q            217   0.525   2.166  tbc_state_r_FSM_FFd3 (tbc_state_r_FSM_FFd3)
     LUT3:I1->O            1   0.250   0.808  _n1225_inv1 (_n1225_inv1)
     LUT6:I3->O            1   0.235   0.000  _n1225_inv3_G (N41)
     MUXF7:I1->O          96   0.175   1.850  _n1225_inv3 (_n1225_inv)
     FDCE:CE                   0.302          tbc_rd_data03_r_0
    ----------------------------------------
    Total                      6.311ns (1.487ns logic, 4.824ns route)
                                       (23.6% logic, 76.4% route)

=========================================================================
Timing constraint: Default period analysis for Clock 'clk_wiz_v1_6_50x62x312/pll_base_inst/CLKOUT0'
  Clock period: 11.090ns (frequency: 90.169MHz)
  Total number of paths / destination ports: 35143 / 490
-------------------------------------------------------------------------
Delay:               11.090ns (Levels of Logic = 8)
  Source:            tx_dvi/enc2/st0_qm_r_4 (FF)
  Destination:       tx_dvi/enc2/st1_cnt_r_6 (FF)
  Source Clock:      clk_wiz_v1_6_50x62x312/pll_base_inst/CLKOUT0 rising
  Destination Clock: clk_wiz_v1_6_50x62x312/pll_base_inst/CLKOUT0 rising

  Data Path: tx_dvi/enc2/st0_qm_r_4 to tx_dvi/enc2/st1_cnt_r_6
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDC:C->Q             11   0.525   1.159  st0_qm_r_4 (st0_qm_r_4)
     LUT4:I0->O           10   0.254   1.287  Mram_st1_cnt1_hi111 (Mram_st1_cnt1_hi1)
     LUT5:I0->O           23   0.254   1.430  Madd_st1_cnt1_lut<1>1 (Madd_st1_cnt1_lut<1>)
     LUT5:I1->O           10   0.254   1.287  Madd_st1_cnt1_xor<2>11 (Msub__n0421_lut<3>)
     LUT6:I1->O           29   0.254   1.478  st1_case_cnt_eq (st1_case_cnt_eq)
     LUT3:I0->O            2   0.235   1.072  Mmux_st1_cnt_w1611 (N62)
     LUT6:I0->O            1   0.254   0.856  Mmux_st1_cnt_w141 (Mmux_st1_cnt_w14)
     LUT5:I1->O            1   0.254   0.000  Mmux_st1_cnt_w145_F (N12)
     MUXF7:I0->O           1   0.163   0.000  Mmux_st1_cnt_w145 (st1_cnt_w<6>)
     FDC:D                     0.074          st1_cnt_r_6
    ----------------------------------------
    Total                     11.090ns (2.521ns logic, 8.569ns route)
                                       (22.7% logic, 77.3% route)

=========================================================================
Timing constraint: Default period analysis for Clock 'clk_wiz_v1_6_50x62x312/pll_base_inst/CLKOUT1'
  Clock period: 2.368ns (frequency: 422.227MHz)
  Total number of paths / destination ports: 103 / 46
-------------------------------------------------------------------------
Delay:               2.368ns (Levels of Logic = 1)
  Source:            tx_dvi/tx3_r_3 (FF)
  Destination:       tx_dvi/tx0_out_r_0 (FF)
  Source Clock:      clk_wiz_v1_6_50x62x312/pll_base_inst/CLKOUT1 rising
  Destination Clock: clk_wiz_v1_6_50x62x312/pll_base_inst/CLKOUT1 rising

  Data Path: tx_dvi/tx3_r_3 to tx_dvi/tx0_out_r_0
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDC:C->Q             33   0.525   1.534  tx3_r_3 (tx3_r_3)
     LUT3:I0->O            1   0.235   0.000  Mmux_tx0_w11 (tx0_r_0)
     FDC:D                     0.074          tx0_out_r_0
    ----------------------------------------
    Total                      2.368ns (0.834ns logic, 1.534ns route)
                                       (35.2% logic, 64.8% route)

=========================================================================
Timing constraint: Default OFFSET IN BEFORE for Clock 'DP_CLK0'
  Total number of paths / destination ports: 3 / 2
-------------------------------------------------------------------------
Offset:              1.881ns (Levels of Logic = 1)
  Source:            DP_HPD (PAD)
  Destination:       aux_hpd_in_r_0 (FF)
  Destination Clock: DP_CLK0 rising

  Data Path: DP_HPD to aux_hpd_in_r_0
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     IBUF:I->O             1   1.228   0.579  DP_HPD_IBUF (DP_HPD_IBUF)
     FDC:D                     0.074          aux_hpd_in_r_0
    ----------------------------------------
    Total                      1.881ns (1.302ns logic, 0.579ns route)
                                       (69.2% logic, 30.8% route)

=========================================================================
Timing constraint: Default OFFSET IN BEFORE for Clock 'inst_sp6wrap/eptest_i/pll_base_i/CLKOUT2'
  Total number of paths / destination ports: 1644 / 1184
-------------------------------------------------------------------------
Offset:              6.913ns (Levels of Logic = 8)
  Source:            inst_sp6wrap/eptest_i/PCIE_A1:TRNRSRCRDYN (PAD)
  Destination:       inst_sp6wrap/app/PIO/PIO_EP/EP_RX/state_3 (FF)
  Destination Clock: inst_sp6wrap/eptest_i/pll_base_i/CLKOUT2 rising

  Data Path: inst_sp6wrap/eptest_i/PCIE_A1:TRNRSRCRDYN to inst_sp6wrap/app/PIO/PIO_EP/EP_RX/state_3
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
    PCIE_A1:TRNRSRCRDYN   18   0.000   0.000  PCIE_A1 (trn_rsrc_rdy_n)
     end scope: 'eptest_i'
     begin scope: 'app'
     begin scope: 'PIO'
     begin scope: 'PIO_EP'
     begin scope: 'EP_RX'
     LUT3:I2->O            6   0.254   1.175  state[3]_tlp_type[6]_AND_43_o111 (N99)
     LUT5:I0->O            2   0.254   1.072  state[3]_trn_rsof_n_AND_38_o1 (state[3]_trn_rsof_n_AND_38_o)
     LUT6:I0->O            2   0.254   1.072  Mmux_n03569213 (N58)
     LUT6:I0->O            6   0.254   1.200  Mmux_n035692 (N45)
     LUT6:I0->O            1   0.254   0.000  Mmux_n03568 (state_next<3>)
     FDR:D                     0.074          state_3
    ----------------------------------------
    Total                      6.913ns (2.394ns logic, 4.519ns route)
                                       (34.6% logic, 65.4% route)

=========================================================================
Timing constraint: Default OFFSET IN BEFORE for Clock 'xtalclk'
  Total number of paths / destination ports: 161 / 136
-------------------------------------------------------------------------
Offset:              5.144ns (Levels of Logic = 4)
  Source:            memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/samc_0:UOREFRSHFLAG (PAD)
  Destination:       memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/gen_term_calib.mcb_soft_calibration_top_inst/mcb_soft_calibration_inst/DQS_DELAY_0 (FF)
  Destination Clock: xtalclk rising

  Data Path: memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/samc_0:UOREFRSHFLAG to memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/gen_term_calib.mcb_soft_calibration_top_inst/mcb_soft_calibration_inst/DQS_DELAY_0
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
    MCB:UOREFRSHFLAG      11   0.000   0.000  samc_0 (uo_refrsh_flag)
     begin scope: 'gen_term_calib.mcb_soft_calibration_top_inst'
     begin scope: 'mcb_soft_calibration_inst'
     LUT6:I1->O            2   0.254   1.072  Inc_Dec_REFRSH_Flag[2]_GND_116_o_equal_177_o<2>1 (Inc_Dec_REFRSH_Flag[2]_GND_116_o_equal_177_o)
     LUT6:I0->O            2   0.254   0.893  _n1389_inv111 (N512)
     LUT6:I2->O            8   0.254   0.802  _n1389_inv (_n1389_inv)
     FDRE:CE                   0.302          DQS_DELAY_0
    ----------------------------------------
    Total                      5.144ns (2.377ns logic, 2.767ns route)
                                       (46.2% logic, 53.8% route)

=========================================================================
Timing constraint: Default OFFSET OUT AFTER for Clock 'DP_CLK0'
  Total number of paths / destination ports: 6 / 6
-------------------------------------------------------------------------
Offset:              4.311ns (Levels of Logic = 1)
  Source:            aux_hpd_r (FF)
  Destination:       led<4> (PAD)
  Source Clock:      DP_CLK0 rising

  Data Path: aux_hpd_r to led<4>
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDC:C->Q             19   0.525   1.071  aux_hpd_r (aux_hpd_r)
     OBUF:I->O                 2.715          led_4_OBUF (led<4>)
    ----------------------------------------
    Total                      4.311ns (3.240ns logic, 1.071ns route)
                                       (75.2% logic, 24.8% route)

=========================================================================
Timing constraint: Default OFFSET OUT AFTER for Clock 'xtalclk'
  Total number of paths / destination ports: 162 / 109
-------------------------------------------------------------------------
Offset:              4.959ns (Levels of Logic = 5)
  Source:            memc3_infrastructure_inst/powerup_pll_locked (FF)
  Destination:       memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/gen_term_calib.mcb_soft_calibration_top_inst/IODRP2_RZQ:T (PAD)
  Source Clock:      xtalclk rising 4.0X

  Data Path: memc3_infrastructure_inst/powerup_pll_locked to memc3_wrapper_inst/memc3_mcb_raw_wrapper_inst/gen_term_calib.mcb_soft_calibration_top_inst/IODRP2_RZQ:T
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDCE:C->Q             2   0.525   0.617  powerup_pll_locked (powerup_pll_locked)
     LUT2:I1->O           76   0.254   1.719  rst_tmp1_1 (async_rst)
     end scope: 'memc3_infrastructure_inst'
     begin scope: 'memc3_wrapper_inst'
     begin scope: 'memc3_mcb_raw_wrapper_inst'
     LUT2:I1->O           35   0.254   1.334  int_sys_rst1_1 (int_sys_rst_0)
     begin scope: 'gen_term_calib.mcb_soft_calibration_top_inst'
     INV:I->O              0   0.255   0.000  RZQ_ZIO_ODATAIN1_INV_0 (RZQ_ZIO_ODATAIN)
    IODRP2:ODATAIN             0.000          IODRP2_RZQ
    ----------------------------------------
    Total                      4.959ns (1.288ns logic, 3.671ns route)
                                       (26.0% logic, 74.0% route)

=========================================================================
Timing constraint: Default OFFSET OUT AFTER for Clock 'inst_sp6wrap/eptest_i/pll_base_i/CLKOUT2'
  Total number of paths / destination ports: 181 / 179
-------------------------------------------------------------------------
Offset:              5.789ns (Levels of Logic = 5)
  Source:            inst_sp6wrap/app/PIO/PIO_EP/EP_RX/bar_r_0 (FF)
  Destination:       GPIO1C<27> (PAD)
  Source Clock:      inst_sp6wrap/eptest_i/pll_base_i/CLKOUT2 rising

  Data Path: inst_sp6wrap/app/PIO/PIO_EP/EP_RX/bar_r_0 to GPIO1C<27>
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDRE:C->Q            45   0.525   1.585  bar_r_0 (bar_r_0)
     end scope: 'EP_RX'
     LUT2:I0->O            5   0.250   0.714  bar0_wr1 (bar0_wr)
     end scope: 'PIO_EP'
     end scope: 'PIO'
     end scope: 'app'
     end scope: 'inst_sp6wrap'
     OBUF:I->O                 2.715          GPIO1C_27_OBUF (GPIO1C<27>)
    ----------------------------------------
    Total                      5.789ns (3.490ns logic, 2.299ns route)
                                       (60.3% logic, 39.7% route)

=========================================================================
Timing constraint: Default OFFSET OUT AFTER for Clock 'clk_wiz_v1_6_50x62x312/pll_base_inst/CLKOUT1'
  Total number of paths / destination ports: 8 / 8
-------------------------------------------------------------------------
Offset:              3.819ns (Levels of Logic = 2)
  Source:            tx_dvi/DDR_tx0_p (FF)
  Destination:       TMDS_CH0_P (PAD)
  Source Clock:      clk_wiz_v1_6_50x62x312/pll_base_inst/CLKOUT1 rising

  Data Path: tx_dvi/DDR_tx0_p to TMDS_CH0_P
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDDRRSE:C0->Q         1   0.525   0.579  DDR_tx0_p (tx_ch0_ddr)
     OBUFDS:I->O               2.715          LVDS_tx0 (DVI_TX0_P)
     end scope: 'tx_dvi'
    ----------------------------------------
    Total                      3.819ns (3.240ns logic, 0.579ns route)
                                       (84.8% logic, 15.2% route)

=========================================================================
Timing constraint: Default path analysis
  Total number of paths / destination ports: 686 / 638
-------------------------------------------------------------------------
Delay:               5.853ns (Levels of Logic = 4)
  Source:            inst_sp6wrap/eptest_i/PCIE_A1:USERRSTN (PAD)
  Destination:       led<0> (PAD)

  Data Path: inst_sp6wrap/eptest_i/PCIE_A1:USERRSTN to led<0>
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
    PCIE_A1:USERRSTN       6   0.000   0.000  PCIE_A1 (trn_reset_n)
     end scope: 'eptest_i'
     INV:I->O             33   0.255   1.305  reset_o1_INV_0 (reset_o)
     end scope: 'inst_sp6wrap'
     INV:I->O              1   0.255   0.579  PCIRST_N1_INV_0 (led_0_OBUF)
     OBUF:I->O                 2.715          led_0_OBUF (led<0>)
    ----------------------------------------
    Total                      5.853ns (3.969ns logic, 1.884ns route)
                                       (67.8% logic, 32.2% route)

=========================================================================


Total REAL time to Xst completion: 137.00 secs
Total CPU time to Xst completion: 137.16 secs
 
--> 

Total memory usage is 243500 kilobytes

Number of errors   :    0 (   0 filtered)
Number of warnings : 3385 (   0 filtered)
Number of infos    :  259 (   0 filtered)

