Par Statistics
Total Non-vccgnd Signals=5482
Total Non-vccgnd Design Pins=19901
Total Non-vccgnd Conns=19901
Total Non-vccgnd Timing Constrained Conns=18250
Phase 1 CPU=14.9 sec
Phase 2 CPU=20.9 sec
Phase 3 CPU=36.9 sec
Phase 4 CPU=40.0 sec
Phase 5 CPU=61.8 sec
Phase 6 CPU=61.8 sec
Phase 7 CPU=61.8 sec
Phase 8 CPU=61.8 sec
Phase 9 CPU=64.9 sec
Phase 10 CPU=66.9 sec
AvgWirelenPerPin Fanout 1=6.0
AvgWirelenPerPin Fanout 2=4.0
AvgWirelenPerPin Fanout 3=5.3
AvgWirelenPerPin Fanout 4=7.3
AvgWirelenPerPin Fanout 10=3.2
AvgWirelenPerPin Fanout 50=3.8
AvgWirelenPerPin Fanout 100=11.5
AvgWirelenPerPin Fanout 500=8.6
AvgWirelenPerPin Fanout 5000=4.7
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
IRR Gamma=1.8430