

 ** \brief Calculate PLL output frequency from settings
#define __PLLCLK       ((__CLKMO  * __PLLN) / __PLLK)
						 4MHz      x 36     / 1 = 144MHz


/* Determine core clock frequency according to settings                       */
#define __MASTERCLK     (__PLLCLK)			144MHz



 ** \brief Define System Clock Frequency (Core Clock) from settings

#if   ((BSC_PSR_Val & 0x07) == 0)
  #define __HCLK         (__MASTERCLK / 1)	144MHz


 ** \brief APB0 Prescaler Register value definition
#define APBC0_PSR_Val         0x00000002     // <<< Define APBC0_PSR here
 ** - 2 = PCLK0 = HCLK / 4				36MHz



 ** \brief APB1 Prescaler Register value definition
 ** Bit#7 : APBC1EN
 ** - 0 = Disable PCLK1 output
 ** - 1 = Enables PCLK1 (default)
#define APBC1_PSR_Val         0x00000082    // <<< Define APBC1_PSR here



 ** \brief APB2 Prescaler Register value definition
 ** - 2 = PCLK2 = HCLK / 4
#define APBC2_PSR_Val         0x00000082    // <<< Define APBC2_PSR here

--------------------------------------------------------------
[　] ・A/Dを初期化する.

[　] ・A/Dをprintで動かす.

[　] ・

[　] ・
--------------------------------------------------------------

monitor/usercmd.c
monitor/smpl_adc12.c
monitor/Adc12Dev_FM3.c

callback.c
crt0.c
debug.c
main.c
usbfunc_demoapp.c
vector.c
monitor/board.c
monitor/fifo.c
monitor/flash.c
monitor/fm3_flash.c
monitor/gpio.c
monitor/monit.c
monitor/picwrt.c
monitor/picwrt2.c
monitor/usbio.c
monitor/usercmd.c
