------------------------------------------------------
Making executable binary:

cmake CMakeLists.txt
make
sudo cp libinput_raspicam_opencv.so /var/opt/mjpg-streamer/input_raspicam_opencv.so
sudo cp www/* /var/opt/mjpg-streamer/www/

------------------------------------------------------
Executing program:

On RPI
sudo /var/opt/mjpg-streamer/mjpg_streamer -i "/var/opt/mjpg-streamer/input_raspicam_opencv.so -fps 2 -x 640 -y 480 -websocket_port 9001" -o "/var/opt/mjpg-streamer/output_http.so -w /var/opt/mjpg-streamer/www -p 8080"

On PC (Google Crome)
http://IP_ADDR:8080/stream_websockets_button.html?9001
------------------------------------------------------
