### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.
To see the actual file transmitted to Xilinx, please click here.

software_version_and_target_device
beta | FALSE | build_version | 1756540
date_generated | Sat Apr 29 17:43:06 2017 | os_platform | WIN64
product_version | Vivado v2016.4 (64-bit) | project_id | da3947ffc8824b9fa5eaeab9f83961ef
project_iteration | 33 | random_id | 670d691206785d3d81b20868dd8a457f
registration_id | 670d691206785d3d81b20868dd8a457f | route_design | TRUE
target_device | xc7a35ti | target_family | artix7
target_package | csg324 | target_speed | -1L
tool_flow | Vivado

user_environment
cpu_name | Intel(R) Core(TM) i7-6950X CPU @ 3.00GHz | cpu_speed | 3000 MHz
os_name | Microsoft Windows 8 or later , 64-bit | os_release | major release (build 9200)
system_ram | 137.000 GB | total_processors | 1

vivado_usage

java_command_handlers
addsources=14 | autoconnecttarget=1 | editdelete=4 | launchprogramfpga=30
newproject=2 | openhardwaremanager=30 | openrecenttarget=3 | programdevice=31
projectsettingscmdhandler=3 | runbitgen=45 | runimplementation=1 | showview=13
viewtaskprojectmanager=18

other_data
guimode=1

project_data
constraintsetcount=1 | core_container=false | currentimplrun=impl_1 | currentsynthesisrun=synth_1
default_library=xil_defaultlib | designmode=RTL | export_simulation_activehdl=0 | export_simulation_ies=0
export_simulation_modelsim=0 | export_simulation_questa=0 | export_simulation_riviera=0 | export_simulation_vcs=0
export_simulation_xsim=0 | implstrategy=Vivado Implementation Defaults | launch_simulation_activehdl=0 | launch_simulation_ies=0
launch_simulation_modelsim=0 | launch_simulation_questa=0 | launch_simulation_riviera=0 | launch_simulation_vcs=0
launch_simulation_xsim=0 | simulator_language=Mixed | srcsetcount=70 | synthesisstrategy=Vivado Synthesis Defaults
target_language=Verilog | target_simulator=XSim | totalimplruns=1 | totalsynthesisruns=1

unisim_transformation
post_unisim_transformation
bufg=1 | carry4=836 | dsp48e1=53 | fdre=8002
fdse=26 | gnd=135 | ibuf=12 | lut1=1118
lut2=1939 | lut3=1901 | lut4=891 | lut5=1422
lut6=2401 | muxf7=101 | muxf8=36 | obuf=25
obuft=2 | ramb18e1=1 | rams32=1 | srlc32e=6
vcc=137
pre_unisim_transformation
bufg=1 | carry4=836 | dsp48e1=53 | fdre=8002
fdse=26 | gnd=135 | ibuf=10 | iobuf=2
lut1=1118 | lut2=1939 | lut3=1901 | lut4=891
lut5=1422 | lut6=2401 | muxf7=101 | muxf8=36
obuf=25 | ram32x1s=1 | ramb18e1=1 | srlc32e=6
vcc=137

power_opt_design
command_line_options_spo
-cell_types=default::all | -clocks=default::[not_specified] | -exclude_cells=default::[not_specified] | -include_cells=default::[not_specified]
usage
bram_ports_augmented=0 | bram_ports_newly_gated=0 | bram_ports_total=2 | flow_state=default
slice_registers_augmented=0 | slice_registers_newly_gated=0 | slice_registers_total=7960 | srls_augmented=0
srls_newly_gated=0 | srls_total=6

ip_statistics
hls_ip_2016_4/10
core_container=NA | hls_input_arch=others | hls_input_clock=8.000000 | hls_input_fixed=0
hls_input_float=0 | hls_input_part=xc7a35ticsg324-1l | hls_input_type=c | hls_syn_clock=6.411000
hls_syn_dsp=0 | hls_syn_ff=3505 | hls_syn_lat=-1 | hls_syn_lut=6284
hls_syn_mem=1 | hls_syn_tpt=none | iptotal=1
hls_ip_2016_4/1
core_container=NA | hls_input_arch=others | hls_input_clock=8.000000 | hls_input_fixed=0
hls_input_float=0 | hls_input_part=xc7a35ticsg324-1l | hls_input_type=c | hls_syn_clock=7.180000
hls_syn_dsp=4 | hls_syn_ff=533 | hls_syn_lat=-1 | hls_syn_lut=899
hls_syn_mem=0 | hls_syn_tpt=none | iptotal=1
hls_ip_2016_4/2
core_container=NA | hls_input_arch=others | hls_input_clock=8.000000 | hls_input_fixed=0
hls_input_float=0 | hls_input_part=xc7a35ticsg324-1l | hls_input_type=c | hls_syn_clock=9.570000
hls_syn_dsp=19 | hls_syn_ff=2749 | hls_syn_lat=-1 | hls_syn_lut=3382
hls_syn_mem=0 | hls_syn_tpt=none | iptotal=1
hls_ip_2016_4/3
core_container=NA | hls_input_arch=others | hls_input_clock=8.000000 | hls_input_fixed=0
hls_input_float=0 | hls_input_part=xc7a35ticsg324-1l | hls_input_type=c | hls_syn_clock=6.680000
hls_syn_dsp=8 | hls_syn_ff=207 | hls_syn_lat=-1 | hls_syn_lut=320
hls_syn_mem=0 | hls_syn_tpt=none | iptotal=1
hls_ip_2016_4/4
core_container=NA | hls_input_arch=others | hls_input_clock=8.000000 | hls_input_fixed=0
hls_input_float=0 | hls_input_part=xc7a35ticsg324-1l | hls_input_type=c | hls_syn_clock=7.180000
hls_syn_dsp=23 | hls_syn_ff=2163 | hls_syn_lat=-1 | hls_syn_lut=2798
hls_syn_mem=0 | hls_syn_tpt=none | iptotal=1
hls_ip_2016_4/5
core_container=NA | hls_input_arch=others | hls_input_clock=8.000000 | hls_input_fixed=0
hls_input_float=0 | hls_input_part=xc7a35ticsg324-1l | hls_input_type=c | hls_syn_clock=6.687880
hls_syn_dsp=4 | hls_syn_ff=336 | hls_syn_lat=-1 | hls_syn_lut=446
hls_syn_mem=0 | hls_syn_tpt=none | iptotal=1
hls_ip_2016_4/6
core_container=NA | hls_input_arch=others | hls_input_clock=8.000000 | hls_input_fixed=0
hls_input_float=0 | hls_input_part=xc7a35ticsg324-1l | hls_input_type=c | hls_syn_clock=7.491200
hls_syn_dsp=0 | hls_syn_ff=243 | hls_syn_lat=-1 | hls_syn_lut=645
hls_syn_mem=0 | hls_syn_tpt=none | iptotal=1
hls_ip_2016_4/7
core_container=NA | hls_input_arch=others | hls_input_clock=8.000000 | hls_input_fixed=0
hls_input_float=0 | hls_input_part=xc7a35ticsg324-1l | hls_input_type=c | hls_syn_clock=4.472400
hls_syn_dsp=0 | hls_syn_ff=374 | hls_syn_lat=-1 | hls_syn_lut=402
hls_syn_mem=0 | hls_syn_tpt=none | iptotal=1
hls_ip_2016_4/8
core_container=NA | hls_input_arch=others | hls_input_clock=8.000000 | hls_input_fixed=0
hls_input_float=0 | hls_input_part=xc7a35ticsg324-1l | hls_input_type=c | hls_syn_clock=5.377000
hls_syn_dsp=0 | hls_syn_ff=164 | hls_syn_lat=-1 | hls_syn_lut=263
hls_syn_mem=0 | hls_syn_tpt=none | iptotal=1
hls_ip_2016_4/9
core_container=NA | hls_input_arch=others | hls_input_clock=8.000000 | hls_input_fixed=0
hls_input_float=0 | hls_input_part=xc7a35ticsg324-1l | hls_input_type=c | hls_syn_clock=4.847600
hls_syn_dsp=0 | hls_syn_ff=1314 | hls_syn_lat=-1 | hls_syn_lut=690
hls_syn_mem=0 | hls_syn_tpt=none | iptotal=1

report_drc
command_line_options
-append=default::[not_specified] | -checks=default::[not_specified] | -fail_on=default::[not_specified] | -force=default::[not_specified]
-format=default::[not_specified] | -messages=default::[not_specified] | -name=default::[not_specified] | -return_string=default::[not_specified]
-ruledecks=default::[not_specified] | -upgrade_cw=default::[not_specified]
results
cfgbvs-1=1 | dpip-1=2 | dpop-1=14 | dpop-2=3

report_methodology
command_line_options
-append=default::[not_specified] | -checks=default::[not_specified] | -fail_on=default::[not_specified] | -force=default::[not_specified]
-format=default::[not_specified] | -messages=default::[not_specified] | -name=default::[not_specified] | -return_string=default::[not_specified]
results
synth-11=3 | synth-6=1 | synth-9=4 | timing-18=24

report_power
command_line_options
-advisory=default::[not_specified] | -append=default::[not_specified] | -file=[specified] | -format=default::text
-hier=default::power | -l=default::[not_specified] | -name=default::[not_specified] | -no_propagation=default::[not_specified]
-return_string=default::[not_specified] | -rpx=[specified] | -verbose=default::[not_specified] | -vid=default::[not_specified]
-xpe=default::[not_specified]
usage
airflow=250 (LFM) | ambient_temp=25.0 (C) | bi-dir_toggle=12.500000 | bidir_output_enable=1.000000
board_layers=12to15 (12 to 15 Layers) | board_selection=medium (10"x10") | bram=0.000028 | clocks=0.023657
confidence_level_clock_activity=High | confidence_level_design_state=High | confidence_level_device_models=Medium | confidence_level_internal_activity=Medium
confidence_level_io_activity=Low | confidence_level_overall=Low | customer=TBD | customer_class=TBD
devstatic=0.061962 | die=xc7a35ticsg324-1L | dsp=0.025164 | dsp_output_toggle=12.500000
dynamic=0.087031 | effective_thetaja=4.8 | enable_probability=0.990000 | family=artix7
ff_toggle=12.500000 | flow_state=routed | heatsink=medium (Medium Profile) | i/o=0.002528
input_toggle=12.500000 | junction_temp=25.7 (C) | logic=0.017334 | mgtavcc_dynamic_current=0.000000
mgtavcc_static_current=0.000000 | mgtavcc_total_current=0.000000 | mgtavcc_voltage=1.000000 | mgtavtt_dynamic_current=0.000000
mgtavtt_static_current=0.000000 | mgtavtt_total_current=0.000000 | mgtavtt_voltage=1.200000 | netlist_net_matched=NA
off-chip_power=0.000000 | on-chip_power=0.148993 | output_enable=1.000000 | output_load=5.000000
output_toggle=12.500000 | package=csg324 | pct_clock_constrained=7.000000 | pct_inputs_defined=8
platform=nt64 | process=typical | ram_enable=50.000000 | ram_write=50.000000
read_saif=False | set/reset_probability=0.000000 | signal_rate=False | signals=0.018320
simulation_file=None | speedgrade=-1L | static_prob=False | temp_grade=industrial
thetajb=6.8 (C/W) | thetasa=4.6 (C/W) | toggle_rate=False | user_board_temp=25.0 (C)
user_effective_thetaja=4.8 | user_junc_temp=25.7 (C) | user_thetajb=6.8 (C/W) | user_thetasa=4.6 (C/W)
vccadc_dynamic_current=0.000000 | vccadc_static_current=0.018000 | vccadc_total_current=0.018000 | vccadc_voltage=1.800000
vccaux_dynamic_current=0.000088 | vccaux_io_dynamic_current=0.000000 | vccaux_io_static_current=0.000000 | vccaux_io_total_current=0.000000
vccaux_io_voltage=1.800000 | vccaux_static_current=0.011362 | vccaux_total_current=0.011451 | vccaux_voltage=1.800000
vccbram_dynamic_current=0.000003 | vccbram_static_current=0.000107 | vccbram_total_current=0.000110 | vccbram_voltage=0.950000
vccint_dynamic_current=0.089072 | vccint_static_current=0.006009 | vccint_total_current=0.095080 | vccint_voltage=0.950000
vcco12_dynamic_current=0.000000 | vcco12_static_current=0.000000 | vcco12_total_current=0.000000 | vcco12_voltage=1.200000
vcco135_dynamic_current=0.000000 | vcco135_static_current=0.000000 | vcco135_total_current=0.000000 | vcco135_voltage=1.350000
vcco15_dynamic_current=0.000000 | vcco15_static_current=0.000000 | vcco15_total_current=0.000000 | vcco15_voltage=1.500000
vcco18_dynamic_current=0.000000 | vcco18_static_current=0.000000 | vcco18_total_current=0.000000 | vcco18_voltage=1.800000
vcco25_dynamic_current=0.000000 | vcco25_static_current=0.000000 | vcco25_total_current=0.000000 | vcco25_voltage=2.500000
vcco33_dynamic_current=0.000682 | vcco33_static_current=0.001000 | vcco33_total_current=0.001682 | vcco33_voltage=3.300000
version=2016.4

report_utilization
clocking
bufgctrl_available=32 | bufgctrl_fixed=0 | bufgctrl_used=1 | bufgctrl_util_percentage=3.13
bufhce_available=72 | bufhce_fixed=0 | bufhce_used=0 | bufhce_util_percentage=0.00
bufio_available=20 | bufio_fixed=0 | bufio_used=0 | bufio_util_percentage=0.00
bufmrce_available=10 | bufmrce_fixed=0 | bufmrce_used=0 | bufmrce_util_percentage=0.00
bufr_available=20 | bufr_fixed=0 | bufr_used=0 | bufr_util_percentage=0.00
mmcme2_adv_available=5 | mmcme2_adv_fixed=0 | mmcme2_adv_used=0 | mmcme2_adv_util_percentage=0.00
plle2_adv_available=5 | plle2_adv_fixed=0 | plle2_adv_used=0 | plle2_adv_util_percentage=0.00
dsp
dsp48e1_only_used=53 | dsps_available=90 | dsps_fixed=0 | dsps_used=53
dsps_util_percentage=58.89
io_standard
blvds_25=0 | diff_hstl_i=0 | diff_hstl_i_18=0 | diff_hstl_ii=0
diff_hstl_ii_18=0 | diff_hsul_12=0 | diff_mobile_ddr=0 | diff_sstl135=0
diff_sstl135_r=0 | diff_sstl15=0 | diff_sstl15_r=0 | diff_sstl18_i=0
diff_sstl18_ii=0 | hstl_i=0 | hstl_i_18=0 | hstl_ii=0
hstl_ii_18=0 | hsul_12=0 | lvcmos12=0 | lvcmos15=0
lvcmos18=0 | lvcmos25=0 | lvcmos33=1 | lvds_25=0
lvttl=0 | mini_lvds_25=0 | mobile_ddr=0 | pci33_3=0
ppds_25=0 | rsds_25=0 | sstl135=0 | sstl135_r=0
sstl15=0 | sstl15_r=0 | sstl18_i=0 | sstl18_ii=0
tmds_33=0
memory
block_ram_tile_available=50 | block_ram_tile_fixed=0 | block_ram_tile_used=0.5 | block_ram_tile_util_percentage=1.00
ramb18_available=100 | ramb18_fixed=0 | ramb18_used=1 | ramb18_util_percentage=1.00
ramb18e1_only_used=1 | ramb36_fifo_available=50 | ramb36_fifo_fixed=0 | ramb36_fifo_used=0
ramb36_fifo_util_percentage=0.00
primitives
bufg_functional_category=Clock | bufg_used=1 | carry4_functional_category=CarryLogic | carry4_used=836
dsp48e1_functional_category=Block Arithmetic | dsp48e1_used=53 | fdre_functional_category=Flop & Latch | fdre_used=7934
fdse_functional_category=Flop & Latch | fdse_used=26 | ibuf_functional_category=IO | ibuf_used=12
lut1_functional_category=LUT | lut1_used=98 | lut2_functional_category=LUT | lut2_used=1939
lut3_functional_category=LUT | lut3_used=1901 | lut4_functional_category=LUT | lut4_used=891
lut5_functional_category=LUT | lut5_used=1422 | lut6_functional_category=LUT | lut6_used=2401
muxf7_functional_category=MuxFx | muxf7_used=101 | muxf8_functional_category=MuxFx | muxf8_used=36
obuf_functional_category=IO | obuf_used=25 | obuft_functional_category=IO | obuft_used=2
ramb18e1_functional_category=Block Memory | ramb18e1_used=1 | rams32_functional_category=Distributed Memory | rams32_used=1
srlc32e_functional_category=Distributed Memory | srlc32e_used=6
slice_logic
f7_muxes_available=16300 | f7_muxes_fixed=0 | f7_muxes_used=101 | f7_muxes_util_percentage=0.62
f8_muxes_available=8150 | f8_muxes_fixed=0 | f8_muxes_used=36 | f8_muxes_util_percentage=0.44
lut_as_distributed_ram_fixed=0 | lut_as_distributed_ram_used=1 | lut_as_logic_available=20800 | lut_as_logic_fixed=0
lut_as_logic_used=7380 | lut_as_logic_util_percentage=35.48 | lut_as_memory_available=9600 | lut_as_memory_fixed=0
lut_as_memory_used=7 | lut_as_memory_util_percentage=0.07 | lut_as_shift_register_fixed=0 | lut_as_shift_register_used=6
register_as_flip_flop_available=41600 | register_as_flip_flop_fixed=0 | register_as_flip_flop_used=7960 | register_as_flip_flop_util_percentage=19.13
register_as_latch_available=41600 | register_as_latch_fixed=0 | register_as_latch_used=0 | register_as_latch_util_percentage=0.00
slice_luts_available=20800 | slice_luts_fixed=0 | slice_luts_used=7387 | slice_luts_util_percentage=35.51
slice_registers_available=41600 | slice_registers_fixed=0 | slice_registers_used=7960 | slice_registers_util_percentage=19.13
fully_used_lut_ff_pairs_fixed=19.13 | fully_used_lut_ff_pairs_used=280 | lut_as_distributed_ram_fixed=0 | lut_as_distributed_ram_used=1
lut_as_logic_available=20800 | lut_as_logic_fixed=0 | lut_as_logic_used=7380 | lut_as_logic_util_percentage=35.48
lut_as_memory_available=9600 | lut_as_memory_fixed=0 | lut_as_memory_used=7 | lut_as_memory_util_percentage=0.07
lut_as_shift_register_fixed=0 | lut_as_shift_register_used=6 | lut_ff_pairs_with_one_unused_flip_flop_fixed=6 | lut_ff_pairs_with_one_unused_flip_flop_used=3163
lut_ff_pairs_with_one_unused_lut_output_fixed=3163 | lut_ff_pairs_with_one_unused_lut_output_used=2956 | lut_flip_flop_pairs_available=20800 | lut_flip_flop_pairs_fixed=0
lut_flip_flop_pairs_used=3515 | lut_flip_flop_pairs_util_percentage=16.90 | slice_available=8150 | slice_fixed=0
slice_used=2809 | slice_util_percentage=34.47 | slicel_fixed=0 | slicel_used=1912
slicem_fixed=0 | slicem_used=897 | unique_control_sets_used=341 | using_o5_and_o6_fixed=341
using_o5_and_o6_used=0 | using_o5_output_only_fixed=0 | using_o5_output_only_used=0 | using_o6_output_only_fixed=0
using_o6_output_only_used=6
specific_feature
bscane2_available=4 | bscane2_fixed=0 | bscane2_used=0 | bscane2_util_percentage=0.00
capturee2_available=1 | capturee2_fixed=0 | capturee2_used=0 | capturee2_util_percentage=0.00
dna_port_available=1 | dna_port_fixed=0 | dna_port_used=0 | dna_port_util_percentage=0.00
efuse_usr_available=1 | efuse_usr_fixed=0 | efuse_usr_used=0 | efuse_usr_util_percentage=0.00
frame_ecce2_available=1 | frame_ecce2_fixed=0 | frame_ecce2_used=0 | frame_ecce2_util_percentage=0.00
icape2_available=2 | icape2_fixed=0 | icape2_used=0 | icape2_util_percentage=0.00
pcie_2_1_available=1 | pcie_2_1_fixed=0 | pcie_2_1_used=0 | pcie_2_1_util_percentage=0.00
startupe2_available=1 | startupe2_fixed=0 | startupe2_used=0 | startupe2_util_percentage=0.00
xadc_available=1 | xadc_fixed=0 | xadc_used=0 | xadc_util_percentage=0.00

router
usage
actual_expansions=7426951 | bogomips=0 | bram18=1 | bram36=0
bufg=0 | bufr=0 | congestion_level=0 | ctrls=341
dsp=53 | effort=2 | estimated_expansions=11695830 | ff=7960
global_clocks=1 | high_fanout_nets=9 | iob=37 | lut=7660
movable_instances=18026 | nets=22483 | pins=121515 | pll=0
router_runtime=0.000000 | router_timing_driven=1 | threads=2 | timing_constraints_exist=1

synthesis
command_line_options
-assert=default::[not_specified] | -bufg=default::12 | -cascade_dsp=default::auto | -constrset=default::[not_specified]
-control_set_opt_threshold=default::auto | -directive=default::default | -fanout_limit=default::10000 | -flatten_hierarchy=default::rebuilt
-fsm_extraction=default::auto | -gated_clock_conversion=default::off | -generic=default::[not_specified] | -include_dirs=default::[not_specified]
-keep_equivalent_registers=default::[not_specified] | -max_bram=default::-1 | -max_bram_cascade_height=default::-1 | -max_dsp=default::-1
-max_uram=default::-1 | -max_uram_cascade_height=default::-1 | -mode=default::default | -name=default::[not_specified]
-no_lc=default::[not_specified] | -no_srlextract=default::[not_specified] | -no_timing_driven=default::[not_specified] | -part=xc7a35ticsg324-1L
-resource_sharing=default::auto | -retiming=default::[not_specified] | -rtl=default::[not_specified] | -rtl_skip_constraints=default::[not_specified]
-rtl_skip_ip=default::[not_specified] | -seu_protect=default::none | -shreg_min_size=default::3 | -top=sns_top
-verilog_define=default::[not_specified]
usage
elapsed=00:02:37s | hls_ip=10 | memory_gain=836.309MB | memory_peak=1046.641MB