
    =========================== USB Port11 ===========================

Connection Status        : 0x01 (Device is connected)
Port Chain               : 2-11

      ========================== Summary =========================
Vendor ID                : 0xCAFE (Unknown Vendor)
Product ID               : 0x4020
USB Version              : 2.00 -> wrong, Device is Full-Speed only
Port maximum Speed       : High-Speed
Device maximum Speed     : Full-Speed
Device Connection Speed  : Full-Speed
Self powered             : no
Demanded Current         : 500 mA
Used Endpoints           : 1

      ======================== USB Device ========================

        +++++++++++++++++ Device Information ++++++++++++++++++
Device Description       : USB Composite Device
Device Path              : \\?\USB#VID_CAFE&PID_4020#123456#{a5dcbf10-6530-11d2-901f-00c04fb951ed} (GUID_DEVINTERFACE_USB_DEVICE)
Kernel Name              : \Device\USBPDO-17
Device ID                : USB\VID_CAFE&PID_4020\123456
Hardware IDs             : USB\VID_CAFE&PID_4020&REV_0100 USB\VID_CAFE&PID_4020
Driver KeyName           : {36fc9e60-c465-11cf-8056-444553540000}\0115 (GUID_DEVCLASS_USB)
Driver                   : \SystemRoot\System32\drivers\usbccgp.sys (Version: 10.0.19041.488  Date: 2020-09-09)
Driver Inf               : C:\WINDOWS\inf\usb.inf
Legacy BusType           : PNPBus
Class                    : USB
Class GUID               : {36fc9e60-c465-11cf-8056-444553540000} (GUID_DEVCLASS_USB)
Service                  : usbccgp
Enumerator               : USB
Location Info            : Port_#0011.Hub_#0003
Location IDs             : PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(11), ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS11)
Container ID             : {5be38ab7-bd9d-56f8-a92b-5e0595cd0ca4}
Manufacturer Info        : (標準 USB ホスト コントローラー)
Capabilities             : 0x94 (Removable, UniqueID, SurpriseRemovalOK)
Status                   : 0x0180600A (DN_DRIVER_LOADED, DN_STARTED, DN_DISABLEABLE, DN_REMOVABLE, DN_NT_ENUMERATOR, DN_NT_DRIVER)
Problem Code             : 0
Address                  : 11
HcDisableSelectiveSuspend: 0
EnableSelectiveSuspend   : 0
SelectiveSuspendEnabled  : 0
EnhancedPowerMgmtEnabled : 0
IdleInWorkingState       : 0
WakeFromSleepState       : 0
Power State              : D0 (supported: D0, D3, wake from D0)
 Child Device 1          : TinyUSB UVC (USB ビデオ デバイス)
  Device Path 1          : \\?\USB#VID_CAFE&PID_4020&MI_00#6&2333ca34&0&0000#{6994ad05-93ef-11d0-a3cc-00a0c9223196}\global (AM_KSCATEGORY_VIDEO)
  Device Path 2          : \\?\USB#VID_CAFE&PID_4020&MI_00#6&2333ca34&0&0000#{e5323777-f976-4f5b-9b55-b94699c46e44}\global (STATIC_KSCATEGORY_VIDEO_CAMERA)
  Device Path 3          : \\?\USB#VID_CAFE&PID_4020&MI_00#6&2333ca34&0&0000#{65e8773d-8f56-11d0-a3b9-00a0c9223196}\global (AM_KSCATEGORY_CAPTURE)
  Kernel Name            : \Device\000005fe
  Device ID              : USB\VID_CAFE&PID_4020&MI_00\6&2333CA34&0&0000
  Class                  : Camera
  Driver KeyName         : {ca3e7ab9-b4c3-4ae6-8251-579ef933890f}\0000 (GUID_DEVCLASS_CAMERA)
  Service                : usbvideo
  Location               : 0000.0014.0000.011.000.000.000.000.000
  LocationPaths          : PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(11)#USBMI(0)  PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(11)#USB(11)  ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS11)#USBMI(0)  ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS11)#USB(11)

        +++++++++++++++++ Registry USB Flags +++++++++++++++++
HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Control\usbflags\CAFE40200100
 osvc                    : REG_BINARY 00 00

        ---------------- Connection Information ---------------
Connection Index         : 0x0B (Port 11)
Connection Status        : 0x01 (DeviceConnected)
Current Config Value     : 0x01 (Configuration 1)
Device Address           : 0x14 (20)
Is Hub                   : 0x00 (no)
Device Bus Speed         : 0x01 (Full-Speed)
Number Of Open Pipes     : 0x00 (0 pipes to data endpoints)
Data (HexDump)           : 0B 00 00 00 12 01 00 02 EF 02 01 40 FE CA 20 40   ...........@.. @
                           00 01 01 02 03 01 01 01 00 14 00 00 00 00 00 01   ................
                           00 00 00                                          ...

        --------------- Connection Information V2 -------------
Connection Index         : 0x0B (11)
Length                   : 0x10 (16 bytes)
SupportedUsbProtocols    : 0x03
 Usb110                  : 1 (yes, port supports USB 1.1)
 Usb200                  : 1 (yes, port supports USB 2.0)
 Usb300                  : 0 (no, port not supports USB 3.0)
 ReservedMBZ             : 0x00
Flags                    : 0x00
 DevIsOpAtSsOrHigher     : 0 (Device is not operating at SuperSpeed or higher)
 DevIsSsCapOrHigher      : 0 (Device is not SuperSpeed capable or higher)
 DevIsOpAtSsPlusOrHigher : 0 (Device is not operating at SuperSpeedPlus or higher)
 DevIsSsPlusCapOrHigher  : 0 (Device is not SuperSpeedPlus capable or higher)
 ReservedMBZ             : 0x00
Data (HexDump)           : 0B 00 00 00 10 00 00 00 03 00 00 00 00 00 00 00   ................

    ---------------------- Device Descriptor ----------------------
bLength                  : 0x12 (18 bytes)
bDescriptorType          : 0x01 (Device Descriptor)
bcdUSB                   : 0x200 (USB Version 2.00) -> wrong, device is Full-Speed only
bDeviceClass             : 0xEF (Miscellaneous)
bDeviceSubClass          : 0x02
bDeviceProtocol          : 0x01 (IAD - Interface Association Descriptor)
bMaxPacketSize0          : 0x40 (64 bytes)
idVendor                 : 0xCAFE (Unknown Vendor)
idProduct                : 0x4020
bcdDevice                : 0x0100
iManufacturer            : 0x01 (String Descriptor 1)
 Language 0x0409         : "TinyUSB"
iProduct                 : 0x02 (String Descriptor 2)
 Language 0x0409         : "TinyUSB Device"
iSerialNumber            : 0x03 (String Descriptor 3)
 Language 0x0409         : "123456"
bNumConfigurations       : 0x01 (1 Configuration)
Data (HexDump)           : 12 01 00 02 EF 02 01 40 FE CA 20 40 00 01 01 02   .......@.. @....
                           03 01                                             ..

    ------------------ Configuration Descriptor -------------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x02 (Configuration Descriptor)
wTotalLength             : 0x00B0 (176 bytes)
bNumInterfaces           : 0x02 (2 Interfaces)
bConfigurationValue      : 0x01 (Configuration 1)
iConfiguration           : 0x00 (No String Descriptor)
bmAttributes             : 0x80
 D7: Reserved, set 1     : 0x01
 D6: Self Powered        : 0x00 (no)
 D5: Remote Wakeup       : 0x00 (no)
 D4..0: Reserved, set 0  : 0x00
MaxPower                 : 0xFA (500 mA)
Data (HexDump)           : 09 02 B0 00 02 01 00 80 FA 08 0B 00 02 0E 03 00   ................
                           04 09 04 00 00 00 0E 01 01 04 0D 24 01 50 01 28   ...........$.P.(
                           00 C0 FC 9B 01 01 01 12 24 02 01 01 02 00 00 00   ........$.......
                           00 00 00 00 00 03 00 00 00 09 24 03 02 01 01 00   ..........$.....
                           01 00 09 04 01 00 00 0E 02 01 00 0E 24 01 01 55   ............$..U
                           00 81 00 02 00 00 00 01 00 1B 24 04 01 01 59 55   ..........$...YU
                           59 32 00 00 10 00 80 00 00 AA 00 38 9B 71 10 01   Y2.........8.q..
                           00 00 00 00 26 24 05 01 00 80 00 60 00 00 00 03   ....&$.....`....
                           00 00 00 1E 00 00 00 03 00 40 42 0F 00 00 40 42   .........@B...@B
                           0F 00 80 96 98 00 40 42 0F 00 06 24 0D 01 01 04   ......@B...$....
                           09 04 01 01 01 0E 02 01 00 07 05 81 05 00 01 01   ................

        ------------------- IAD Descriptor --------------------
bLength                  : 0x08 (8 bytes)
bDescriptorType          : 0x0B (Interface Association Descriptor)
bFirstInterface          : 0x00 (Interface 0)
bInterfaceCount          : 0x02 (2 Interfaces)
bFunctionClass           : 0x0E (Video)
bFunctionSubClass        : 0x03 (Video Interface Collection)
bFunctionProtocol        : 0x00 (PC_PROTOCOL_UNDEFINED)
iFunction                : 0x04 (String Descriptor 4)
 Language 0x0409         : "TinyUSB UVC"
Data (HexDump)           : 08 0B 00 02 0E 03 00 04                           ........

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x00 (Interface 0)
bAlternateSetting        : 0x00
bNumEndpoints            : 0x00 (Default Control Pipe only)
bInterfaceClass          : 0x0E (Video)
bInterfaceSubClass       : 0x01 (Video Control)
bInterfaceProtocol       : 0x01  *!*ERROR  must be 0 for this class
iInterface               : 0x04 (String Descriptor 4)
 Language 0x0409         : "TinyUSB UVC"
Data (HexDump)           : 09 04 00 00 00 0E 01 01 04                        .........

        ------- Video Control Interface Header Descriptor -----
bLength                  : 0x0D (13 bytes)
bDescriptorType          : 0x24 (Video Control Interface)
bDescriptorSubtype       : 0x01 (Video Control Header)
bcdUVC                   : 0x0150 (UVC Version 1.50)
wTotalLength             : 0x0028 (40 bytes)
dwClockFreq              : 0x019BFCC0 (27 MHz)
bInCollection            : 0x01 (1 VideoStreaming interface)
baInterfaceNr[1]         : 0x01 (Interface 1)
Data (HexDump)           : 0D 24 01 50 01 28 00 C0 FC 9B 01 01 01            .$.P.(.......

        -------- Video Control Input Terminal Descriptor ------
bLength                  : 0x12 (18 bytes)
bDescriptorType          : 0x24 (Video Control Interface)
bDescriptorSubtype       : 0x02 (Input Terminal)
bTerminalID              : 0x01 (1)
wTerminalType            : 0x0201 (ITT_CAMERA)
bAssocTerminal           : 0x00 (Not associated with an Output Terminal)
iTerminal                : 0x00 (No String Descriptor)
Camera Input Terminal Data:
wObjectiveFocalLengthMin : 0x0000
wObjectiveFocalLengthMax : 0x0000
wOcularFocalLength       : 0x0000
bControlSize             : 0x03 (3 bytes)
bmControls               : 0x00, 0x00, 0x00
 D0                      : 0   no -  Scanning Mode
 D1                      : 0   no -  Auto-Exposure Mode
 D2                      : 0   no -  Auto-Exposure Priority
 D3                      : 0   no -  Exposure Time (Absolute)
 D4                      : 0   no -  Exposure Time (Relative)
 D5                      : 0   no -  Focus (Absolute)
 D6                      : 0   no -  Focus (Relative)
 D7                      : 0   no -  Iris (Absolute)
 D8                      : 0   no -  Iris (Relative)
 D9                      : 0   no -  Zoom (Absolute)
 D10                     : 0   no -  Zoom (Relative)
 D11                     : 0   no -  Pan (Absolute)
 D12                     : 0   no -  Pan (Relative)
 D13                     : 0   no -  Roll (Absolute)
 D14                     : 0   no -  Roll (Relative)
 D15                     : 0   no -  Tilt (Absolute)
 D16                     : 0   no -  Tilt (Relative)
 D17                     : 0   no -  Focus Auto
 D18                     : 0   no -  Reserved
 D19                     : 0   no -  Reserved
 D20                     : 0   no -  Reserved
 D21                     : 0   no -  Reserved
 D22                     : 0   no -  Reserved
 D23                     : 0   no -  Reserved
Data (HexDump)           : 12 24 02 01 01 02 00 00 00 00 00 00 00 00 03 00   .$..............
                           00 00                                             ..

        ------- Video Control Output Terminal Descriptor ------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x24 (Video Control Interface)
bDescriptorSubtype       : 0x03 (Output Terminal)
bTerminalID              : 0x02 (2)
wTerminalType            : 0x0101 (TT_STREAMING)
bAssocTerminal           : 0x00 (Not associated with an Input Terminal)
bSourceID                : 0x01 (1)
iTerminal                : 0x00 (No String Descriptor)
Data (HexDump)           : 09 24 03 02 01 01 00 01 00                        .$.......

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x01 (Interface 1)
bAlternateSetting        : 0x00
bNumEndpoints            : 0x00 (Default Control Pipe only)
bInterfaceClass          : 0x0E (Video)
bInterfaceSubClass       : 0x02 (Video Streaming)
bInterfaceProtocol       : 0x01  *!*ERROR  must be 0 for this class
iInterface               : 0x00 (No String Descriptor)
Data (HexDump)           : 09 04 01 00 00 0E 02 01 00                        .........

        ---- VC-Specific VS Video Input Header Descriptor -----
bLength                  : 0x0E (14 bytes)
bDescriptorType          : 0x24 (Video Streaming Interface)
bDescriptorSubtype       : 0x01 (Input Header)
bNumFormats              : 0x01
wTotalLength             : 0x0055 (85 bytes)
bEndpointAddress         : 0x81 (Direction=IN  EndpointID=1)
bmInfo                   : 0x00 (Dynamic Format Change not supported)
bTerminalLink            : 0x02 (Output Terminal ID 2)
bStillCaptureMethod      : 0x00 (No Still Capture)
nbTriggerSupport         : 0x00 (Hardware Triggering not supported)
bTriggerUsage            : 0x00 (Host will initiate still image capture)
bControlSize             : 0x01 (1 bytes each)
Video Payload Format 1   : 0x00
 D0                      : 0   no -  Key Frame Rate
 D1                      : 0   no -  P Frame Rate
 D2                      : 0   no -  Compression Quality
 D3                      : 0   no -  Compression Window Size
 D4                      : 0   no -  Generate Key Frame
 D5                      : 0   no -  Update Frame Segment
 D6                      : 0   no -  Reserved
 D7                      : 0   no -  Reserved
Data (HexDump)           : 0E 24 01 01 55 00 81 00 02 00 00 00 01 00         .$..U.........

        ------- VS Uncompressed Format Type Descriptor --------
bLength                  : 0x1B (27 bytes)
bDescriptorType          : 0x24 (Video Streaming Interface)
bDescriptorSubtype       : 0x04 (Uncompressed Format Type)
bFormatIndex             : 0x01 (1)
bNumFrameDescriptors     : 0x01 (1 Frame Descriptor)
guidFormat               : {32595559-0000-0010-8000-00AA00389B71} (YUY2)
bBitsPerPixel            : 0x10 (16 bits per pixel)
bDefaultFrameIndex       : 0x01 (Index 1)
bAspectRatioX            : 0x00
bAspectRatioY            : 0x00
bmInterlaceFlags         : 0x00
 D0 IL stream or variable: 0 (no)
 D1 Fields per frame     : 0 (2 fields)
 D2 Field 1 first        : 0 (no)
 D3 Reserved             : 0
 D4..5 Field pattern     : 0 (Field 1 only)
 D6..7 Display Mode      : 0 (Bob only)
bCopyProtect             : 0x00 (No restrictions)
Data (HexDump)           : 1B 24 04 01 01 59 55 59 32 00 00 10 00 80 00 00   .$...YUY2.......
                           AA 00 38 9B 71 10 01 00 00 00 00                  ..8.q......

        -------- VS Uncompressed Frame Type Descriptor --------
---> This is the Default (optimum) Frame index
bLength                  : 0x26 (38 bytes)
bDescriptorType          : 0x24 (Video Streaming Interface)
bDescriptorSubtype       : 0x05 (Uncompressed Frame Type)
bFrameIndex              : 0x01
bmCapabilities           : 0x00
wWidth                   : 0x0080 (128)
wHeight                  : 0x0060 (96)
dwMinBitRate             : 0x00030000 (196608 bps -> 24.500 KB/s)
dwMaxBitRate             : 0x001E0000 (1966080 bps -> 245.750 KB/s)
dwMaxVideoFrameBufferSize: 0x00030000 (196608 bytes)
dwDefaultFrameInterval   : 0x000F4240 (100.0000 ms -> 10.000 fps)
bFrameIntervalType       : 0x00 (0 discrete frame intervals supported)
dwMinFrameInterval       : 0x000F4240 (100.0000 ms -> 10.000 fps)
dwMaxFrameInterval       : 0x00989680 (1000.0000 ms -> 1.000 fps)
dwFrameIntervalStep      : 0x000F4240
Data (HexDump)           : 26 24 05 01 00 80 00 60 00 00 00 03 00 00 00 1E   &$.....`........
                           00 00 00 03 00 40 42 0F 00 00 40 42 0F 00 80 96   .....@B...@B....
                           98 00 40 42 0F 00                                 ..@B..

        ------- VS Color Matching Descriptor Descriptor -------
bLength                  : 0x06 (6 bytes)
bDescriptorType          : 0x24 (Video Streaming Interface)
bDescriptorSubtype       : 0x0D (Color Matching)
bColorPrimaries          : 0x01 (BT.709, sRGB)
bTransferCharacteristics : 0x01 (BT.709)
bMatrixCoefficients      : 0x04 (SMPTE 170M)
Data (HexDump)           : 06 24 0D 01 01 04                                 .$....

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x01 (Interface 1)
bAlternateSetting        : 0x01
bNumEndpoints            : 0x01 (1 Endpoint)
bInterfaceClass          : 0x0E (Video)
bInterfaceSubClass       : 0x02 (Video Streaming)
bInterfaceProtocol       : 0x01  *!*ERROR  must be 0 for this class
iInterface               : 0x00 (No String Descriptor)
Data (HexDump)           : 09 04 01 01 01 0E 02 01 00                        .........

        ----------------- Endpoint Descriptor -----------------
bLength                  : 0x07 (7 bytes)
bDescriptorType          : 0x05 (Endpoint Descriptor)
bEndpointAddress         : 0x81 (Direction=IN EndpointID=1)
bmAttributes             : 0x05 (TransferType=Isochronous  SyncType=Asynchronous  EndpointType=Data)
wMaxPacketSize           : 0x0100 (256 bytes)
bInterval                : 0x01 (1 ms)
Data (HexDump)           : 07 05 81 05 00 01 01                              .......

    ----------------- Device Qualifier Descriptor -----------------
Error                    : ERROR_GEN_FAILURE  (*!*ERROR   USB 2.0 devices must provide a Device Qualifier Descriptor)

      -------------------- String Descriptors -------------------
             ------ String Descriptor 0 ------
bLength                  : 0x04 (4 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language ID[0]           : 0x0409 (English - United States)
Data (HexDump)           : 04 03 09 04                                       ....
             ------ String Descriptor 1 ------
bLength                  : 0x10 (16 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "TinyUSB"
Data (HexDump)           : 10 03 54 00 69 00 6E 00 79 00 55 00 53 00 42 00   ..T.i.n.y.U.S.B.
             ------ String Descriptor 2 ------
bLength                  : 0x1E (30 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "TinyUSB Device"
Data (HexDump)           : 1E 03 54 00 69 00 6E 00 79 00 55 00 53 00 42 00   ..T.i.n.y.U.S.B.
                           20 00 44 00 65 00 76 00 69 00 63 00 65 00          .D.e.v.i.c.e.
             ------ String Descriptor 3 ------
bLength                  : 0x0E (14 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "123456"
Data (HexDump)           : 0E 03 31 00 32 00 33 00 34 00 35 00 36 00         ..1.2.3.4.5.6.
             ------ String Descriptor 4 ------
bLength                  : 0x18 (24 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "TinyUSB UVC"
Data (HexDump)           : 18 03 54 00 69 00 6E 00 79 00 55 00 53 00 42 00   ..T.i.n.y.U.S.B.
                           20 00 55 00 56 00 43 00                            .U.V.C.
