
    =========================== USB Port11 ===========================

Connection Status        : 0x01 (Device is connected)
Port Chain               : 2-11

      ========================== Summary =========================
Vendor ID                : 0x2E8A (Raspberry Pi (Trading) Limited)
Product ID               : 0x0003
USB Version              : 1.10
Port maximum Speed       : High-Speed
Device maximum Speed     : Full-Speed
Device Connection Speed  : Full-Speed
Self powered             : no
Demanded Current         : 500 mA
Used Endpoints           : 5

      ======================== USB Device ========================

        +++++++++++++++++ Device Information ++++++++++++++++++
Device Description       : USB Composite Device
Device Path              : \\?\USB#VID_2E8A&PID_0003#E0C912952D54#{a5dcbf10-6530-11d2-901f-00c04fb951ed} (GUID_DEVINTERFACE_USB_DEVICE)
Kernel Name              : \Device\USBPDO-7
Device ID                : USB\VID_2E8A&PID_0003\E0C912952D54
Hardware IDs             : USB\VID_2E8A&PID_0003&REV_0100 USB\VID_2E8A&PID_0003
Driver KeyName           : {36fc9e60-c465-11cf-8056-444553540000}\0030 (GUID_DEVCLASS_USB)
Driver                   : \SystemRoot\System32\drivers\usbccgp.sys (Version: 10.0.19041.488  Date: 2020-09-09)
Driver Inf               : C:\WINDOWS\inf\usb.inf
Legacy BusType           : PNPBus
Class                    : USB
Class GUID               : {36fc9e60-c465-11cf-8056-444553540000} (GUID_DEVCLASS_USB)
Service                  : usbccgp
Enumerator               : USB
Location Info            : Port_#0011.Hub_#0003
Location IDs             : PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(11), ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS11)
Container ID             : {4ba12f58-c1a4-57fe-bf4f-c2ba1105700e}
Manufacturer Info        : (標準 USB ホスト コントローラー)
Capabilities             : 0x94 (Removable, UniqueID, SurpriseRemovalOK)
Status                   : 0x0180600A (DN_DRIVER_LOADED, DN_STARTED, DN_DISABLEABLE, DN_REMOVABLE, DN_NT_ENUMERATOR, DN_NT_DRIVER)
Problem Code             : 0
Address                  : 11
HcDisableSelectiveSuspend: 0
EnableSelectiveSuspend   : 0
SelectiveSuspendEnabled  : 0
EnhancedPowerMgmtEnabled : 0
IdleInWorkingState       : 0
WakeFromSleepState       : 0
Power State              : D0 (supported: D0, D3, wake from D0)
 Child Device 1          : USB 大容量記憶装置
  Device ID              : USB\VID_2E8A&PID_0003&MI_00\6&2F5B6A17&1&0000
  Class                  : USB
  Driver KeyName         : {36fc9e60-c465-11cf-8056-444553540000}\0033 (GUID_DEVCLASS_USB)
  Service                : USBSTOR
  Location               : 0000.0014.0000.011.000.000.000.000.000
  LocationPaths          : PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(11)#USBMI(0)  PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(11)#USB(11)  ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS11)#USBMI(0)  ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS11)#USB(11)
   Child Device 1        : RPI RP2 USB Device (ディスク ドライブ) (Disk2)
    Device Path          : \\?\USBSTOR#Disk&Ven_RPI&Prod_RP2&Rev_2#7&3adfbf33&0&E0C912952D54&0#{53f56307-b6bf-11d0-94f2-00a0c91efb8b} (GUID_DEVINTERFACE_DISK)
    Kernel Name          : \Device\00000109
    Device ID            : USBSTOR\DISK&VEN_RPI&PROD_RP2&REV_2\7&3ADFBF33&0&E0C912952D54&0
    Class                : DiskDrive
    Driver KeyName       : {4d36e967-e325-11ce-bfc1-08002be10318}\0007 (GUID_DEVCLASS_DISKDRIVE)
    Service              : disk
     Volume              : \\?\Volume{a751a706-9783-11ec-b4f2-0009dd429377}\
     Kernel Name         : \Device\HarddiskVolume9
     Mountpoint          : H:\
 Child Device 2          : RP2 Boot (Nano RP2040 Connect Picoboot IF)
  Device Path 1          : \\?\USB#VID_2E8A&PID_0003&MI_01#6&2f5b6a17&1&0001#{51de5bfa-d59d-4f3e-9b36-0b4b210dd53f}
  Device Path 2          : \\?\USB#VID_2E8A&PID_0003&MI_01#6&2f5b6a17&1&0001#{dee824ef-729b-4a0e-9c14-b7117d33a817} (GUID_DEVINTERFACE_WINUSB)
  Kernel Name            : \Device\00000107
  Device ID              : USB\VID_2E8A&PID_0003&MI_01\6&2F5B6A17&1&0001
  Class                  : USBDevice
  Driver KeyName         : {88bae032-5a81-49f0-bc3d-a4ff138216d6}\0003 (GUID_DEVCLASS_USBDEVICE)
  Service                : WINUSB
  Location               : 0000.0014.0000.011.000.000.000.000.000
  LocationPaths          : PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(11)#USBMI(1)  ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS11)#USBMI(1)

        ---------------- Connection Information ---------------
Connection Index         : 0x0B (Port 11)
Connection Status        : 0x01 (DeviceConnected)
Current Config Value     : 0x01 (Configuration 1)
Device Address           : 0x17 (23)
Is Hub                   : 0x00 (no)
Device Bus Speed         : 0x01 (Full-Speed)
Number Of Open Pipes     : 0x04 (4 pipes to data endpoints)
Pipe[0]                  : EndpointID=3  Direction=OUT  ScheduleOffset=0  Type=Bulk  wMaxPacketSize=64   bInterval=0
Pipe[1]                  : EndpointID=4  Direction=IN   ScheduleOffset=0  Type=Bulk  wMaxPacketSize=64   bInterval=0
Pipe[2]                  : EndpointID=1  Direction=IN   ScheduleOffset=0  Type=Bulk  wMaxPacketSize=64   bInterval=0
Pipe[3]                  : EndpointID=2  Direction=OUT  ScheduleOffset=0  Type=Bulk  wMaxPacketSize=64   bInterval=0
Data (HexDump)           : 0B 00 00 00 12 01 10 01 00 00 00 40 8A 2E 03 00   ...........@....
                           00 01 01 02 03 01 01 01 00 17 00 04 00 00 00 01   ................
                           00 00 00 07 05 03 02 40 00 00 00 00 00 00 07 05   .......@........
                           84 02 40 00 00 00 00 00 00 07 05 81 02 40 00 00   ..@..........@..
                           00 00 00 00 07 05 02 02 40 00 00 00 00 00 00      ........@......

        --------------- Connection Information V2 -------------
Connection Index         : 0x0B (11)
Length                   : 0x10 (16 bytes)
SupportedUsbProtocols    : 0x03
 Usb110                  : 1 (yes, port supports USB 1.1)
 Usb200                  : 1 (yes, port supports USB 2.0)
 Usb300                  : 0 (no, port not supports USB 3.0)
 ReservedMBZ             : 0x00
Flags                    : 0x00
 DevIsOpAtSsOrHigher     : 0 (Device is not operating at SuperSpeed or higher)
 DevIsSsCapOrHigher      : 0 (Device is not SuperSpeed capable or higher)
 DevIsOpAtSsPlusOrHigher : 0 (Device is not operating at SuperSpeedPlus or higher)
 DevIsSsPlusCapOrHigher  : 0 (Device is not SuperSpeedPlus capable or higher)
 ReservedMBZ             : 0x00
Data (HexDump)           : 0B 00 00 00 10 00 00 00 03 00 00 00 00 00 00 00   ................

    ---------------------- Device Descriptor ----------------------
bLength                  : 0x12 (18 bytes)
bDescriptorType          : 0x01 (Device Descriptor)
bcdUSB                   : 0x110 (USB Version 1.10)
bDeviceClass             : 0x00 (defined by the interface descriptors)
bDeviceSubClass          : 0x00
bDeviceProtocol          : 0x00
bMaxPacketSize0          : 0x40 (64 bytes)
idVendor                 : 0x2E8A (Raspberry Pi (Trading) Limited)
idProduct                : 0x0003
bcdDevice                : 0x0100
iManufacturer            : 0x01 (String Descriptor 1)
 Language 0x0409         : "Raspberry Pi"
iProduct                 : 0x02 (String Descriptor 2)
 Language 0x0409         : "RP2 Boot"
iSerialNumber            : 0x03 (String Descriptor 3)
 Language 0x0409         : "E0C912952D54"
bNumConfigurations       : 0x01 (1 Configuration)
Data (HexDump)           : 12 01 10 01 00 00 00 40 8A 2E 03 00 00 01 01 02   .......@........
                           03 01                                             ..

    ------------------ Configuration Descriptor -------------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x02 (Configuration Descriptor)
wTotalLength             : 0x0037 (55 bytes)
bNumInterfaces           : 0x02 (2 Interfaces)
bConfigurationValue      : 0x01 (Configuration 1)
iConfiguration           : 0x00 (No String Descriptor)
bmAttributes             : 0x80
 D7: Reserved, set 1     : 0x01
 D6: Self Powered        : 0x00 (no)
 D5: Remote Wakeup       : 0x00 (no)
 D4..0: Reserved, set 0  : 0x00
MaxPower                 : 0xFA (500 mA)
Data (HexDump)           : 09 02 37 00 02 01 00 80 FA 09 04 00 00 02 08 06   ..7.............
                           50 00 07 05 81 02 40 00 00 07 05 02 02 40 00 00   P.....@......@..
                           09 04 01 00 02 FF 00 00 00 07 05 03 02 40 00 00   .............@..
                           07 05 84 02 40 00 00                              ....@..

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x00 (Interface 0)
bAlternateSetting        : 0x00
bNumEndpoints            : 0x02 (2 Endpoints)
bInterfaceClass          : 0x08 (Mass Storage)
bInterfaceSubClass       : 0x06 (SCSI transparent command set)
bInterfaceProtocol       : 0x50 (Bulk-Only Transport)
iInterface               : 0x00 (No String Descriptor)
Data (HexDump)           : 09 04 00 00 02 08 06 50 00                        .......P.

        ----------------- Endpoint Descriptor -----------------
bLength                  : 0x07 (7 bytes)
bDescriptorType          : 0x05 (Endpoint Descriptor)
bEndpointAddress         : 0x81 (Direction=IN EndpointID=1)
bmAttributes             : 0x02 (TransferType=Bulk)
wMaxPacketSize           : 0x0040 (64 bytes)
bInterval                : 0x00 (ignored)
Data (HexDump)           : 07 05 81 02 40 00 00                              ....@..

        ----------------- Endpoint Descriptor -----------------
bLength                  : 0x07 (7 bytes)
bDescriptorType          : 0x05 (Endpoint Descriptor)
bEndpointAddress         : 0x02 (Direction=OUT EndpointID=2)
bmAttributes             : 0x02 (TransferType=Bulk)
wMaxPacketSize           : 0x0040 (64 bytes)
bInterval                : 0x00 (ignored)
Data (HexDump)           : 07 05 02 02 40 00 00                              ....@..

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x01 (Interface 1)
bAlternateSetting        : 0x00
bNumEndpoints            : 0x02 (2 Endpoints)
bInterfaceClass          : 0xFF (Vendor Specific)
bInterfaceSubClass       : 0x00
bInterfaceProtocol       : 0x00
iInterface               : 0x00 (No String Descriptor)
Data (HexDump)           : 09 04 01 00 02 FF 00 00 00                        .........

        ----------------- Endpoint Descriptor -----------------
bLength                  : 0x07 (7 bytes)
bDescriptorType          : 0x05 (Endpoint Descriptor)
bEndpointAddress         : 0x03 (Direction=OUT EndpointID=3)
bmAttributes             : 0x02 (TransferType=Bulk)
wMaxPacketSize           : 0x0040 (64 bytes)
bInterval                : 0x00 (ignored)
Data (HexDump)           : 07 05 03 02 40 00 00                              ....@..

        ----------------- Endpoint Descriptor -----------------
bLength                  : 0x07 (7 bytes)
bDescriptorType          : 0x05 (Endpoint Descriptor)
bEndpointAddress         : 0x84 (Direction=IN EndpointID=4)
bmAttributes             : 0x02 (TransferType=Bulk)
wMaxPacketSize           : 0x0040 (64 bytes)
bInterval                : 0x00 (ignored)
Data (HexDump)           : 07 05 84 02 40 00 00                              ....@..

      -------------------- String Descriptors -------------------
             ------ String Descriptor 0 ------
bLength                  : 0x04 (4 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language ID[0]           : 0x0409 (English - United States)
Data (HexDump)           : 04 03 09 04                                       ....
             ------ String Descriptor 1 ------
bLength                  : 0x1A (26 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "Raspberry Pi"
Data (HexDump)           : 1A 03 52 00 61 00 73 00 70 00 62 00 65 00 72 00   ..R.a.s.p.b.e.r.
                           72 00 79 00 20 00 50 00 69 00                     r.y. .P.i.
             ------ String Descriptor 2 ------
bLength                  : 0x12 (18 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "RP2 Boot"
Data (HexDump)           : 12 03 52 00 50 00 32 00 20 00 42 00 6F 00 6F 00   ..R.P.2. .B.o.o.
                           74 00                                             t.
             ------ String Descriptor 3 ------
bLength                  : 0x1A (26 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "E0C912952D54"
Data (HexDump)           : 1A 03 45 00 30 00 43 00 39 00 31 00 32 00 39 00   ..E.0.C.9.1.2.9.
                           35 00 32 00 44 00 35 00 34 00                     5.2.D.5.4.
