/*
 * The MIT License (MIT)
 *
 * Copyright (c) 2019 Ha Thach (tinyusb.org)
 *
 * Permission is hereby granted, free of charge, to any person obtaining a copy
 * of this software and associated documentation files (the "Software"), to deal
 * in the Software without restriction, including without limitation the rights
 * to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
 * copies of the Software, and to permit persons to whom the Software is
 * furnished to do so, subject to the following conditions:
 *
 * The above copyright notice and this permission notice shall be included in
 * all copies or substantial portions of the Software.
 *
 * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
 * IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
 * FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
 * AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
 * LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
 * OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN
 * THE SOFTWARE.
 *
 */

#ifndef _TUSB_CONFIG_H_
#define _TUSB_CONFIG_H_

#ifdef __cplusplus
extern "C" {
#endif

//--------------------------------------------------------------------+
// Board Specific Configuration
//--------------------------------------------------------------------+

// RHPort number used for device can be defined by board.mk, default to port 0
#ifndef BOARD_TUD_RHPORT
#define BOARD_TUD_RHPORT      0
#endif

// RHPort max operational speed can defined by board.mk
#ifndef BOARD_TUD_MAX_SPEED
#define BOARD_TUD_MAX_SPEED   OPT_MODE_DEFAULT_SPEED
#endif

//--------------------------------------------------------------------
// COMMON CONFIGURATION
//--------------------------------------------------------------------

// defined by compiler flags for flexibility
#ifndef CFG_TUSB_MCU
#error CFG_TUSB_MCU must be defined
#endif

#ifndef CFG_TUSB_OS
#define CFG_TUSB_OS               OPT_OS_NONE
#endif

#ifndef CFG_TUSB_DEBUG
#define CFG_TUSB_DEBUG            0
#endif

// Enable Device stack
#define CFG_TUD_ENABLED           1

// Default is max speed that hardware controller could support with on-chip PHY
#define CFG_TUD_MAX_SPEED         BOARD_TUD_MAX_SPEED

/* USB DMA on some MCUs can only access a specific SRAM region with restriction on alignment.
 * Tinyusb use follows macros to declare transferring memory so that they can be put
 * into those specific section.
 * e.g
 * - CFG_TUSB_MEM SECTION : __attribute__ (( section(".usb_ram") ))
 * - CFG_TUSB_MEM_ALIGN   : __attribute__ ((aligned(4)))
 */
#ifndef CFG_TUSB_MEM_SECTION
#define CFG_TUSB_MEM_SECTION
#endif

#ifndef CFG_TUSB_MEM_ALIGN
#define CFG_TUSB_MEM_ALIGN        __attribute__ ((aligned(4)))
#endif

//--------------------------------------------------------------------
// DEVICE CONFIGURATION
//--------------------------------------------------------------------

#ifndef CFG_TUD_ENDPOINT0_SIZE
#define CFG_TUD_ENDPOINT0_SIZE    64
#endif

//------------- CLASS -------------//
#define CFG_TUD_AUDIO             1
#define CFG_TUD_CDC               0
#define CFG_TUD_MSC               0
#define CFG_TUD_HID               0
#define CFG_TUD_MIDI              0
#define CFG_TUD_VENDOR            0

//--------------------------------------------------------------------
// AUDIO CLASS DRIVER CONFIGURATION
//--------------------------------------------------------------------

// Have a look into audio_device.h for all configurations

#define CFG_TUD_AUDIO_FUNC_1_DESC_LEN                 TUD_AUDIO_MIC_FOUR_CH_DESC_LEN

#define CFG_TUD_AUDIO_FUNC_1_N_AS_INT                 1
#define CFG_TUD_AUDIO_FUNC_1_CTRL_BUF_SZ              64

#define CFG_TUD_AUDIO_ENABLE_EP_IN                    1
#define CFG_TUD_AUDIO_FUNC_1_N_BYTES_PER_SAMPLE_TX    2         // This value is not required by the driver, it parses this information from the descriptor once the alternate interface is set by the host - we use it for the setup
#define CFG_TUD_AUDIO_FUNC_1_N_CHANNELS_TX            4         // This value is not required by the driver, it parses this information from the descriptor once the alternate interface is set by the host - we use it for the setup
#define CFG_TUD_AUDIO_EP_SZ_IN                        (48 + 1) * CFG_TUD_AUDIO_FUNC_1_N_BYTES_PER_SAMPLE_TX * CFG_TUD_AUDIO_FUNC_1_N_CHANNELS_TX      // 48 Samples (48 kHz) x 2 Bytes/Sample x CFG_TUD_AUDIO_N_CHANNELS_TX Channels - the Windows driver always needs an extra sample per channel of space more, otherwise it complains... found by trial and error
#define CFG_TUD_AUDIO_FUNC_1_EP_IN_SZ_MAX             CFG_TUD_AUDIO_EP_SZ_IN
#define CFG_TUD_AUDIO_FUNC_1_EP_IN_SW_BUF_SZ          CFG_TUD_AUDIO_EP_SZ_IN

#define CFG_TUD_AUDIO_ENABLE_ENCODING                 1
#define CFG_TUD_AUDIO_ENABLE_TYPE_I_ENCODING          1
#define CFG_TUD_AUDIO_FUNC_1_CHANNEL_PER_FIFO_TX      2         // One I2S stream contains two channels, each stream is saved within one support FIFO - this value is currently fixed, the driver does not support a changing value
#define CFG_TUD_AUDIO_FUNC_1_N_TX_SUPP_SW_FIFO        (CFG_TUD_AUDIO_FUNC_1_N_CHANNELS_TX / CFG_TUD_AUDIO_FUNC_1_CHANNEL_PER_FIFO_TX)
#define CFG_TUD_AUDIO_FUNC_1_TX_SUPP_SW_FIFO_SZ       (CFG_TUD_AUDIO_EP_SZ_IN / CFG_TUD_AUDIO_FUNC_1_N_TX_SUPP_SW_FIFO)

#ifdef __cplusplus
}
#endif

#endif /* _TUSB_CONFIG_H_ */
