
    =========================== USB Port11 ===========================

Connection Status        : 0x01 (Device is connected)
Port Chain               : 2-11

      ========================== Summary =========================
Vendor ID                : 0xCAFE (Unknown Vendor)
Product ID               : 0x4000
USB Version              : 2.00 -> wrong, Device is Full-Speed only
Port maximum Speed       : High-Speed
Device maximum Speed     : Full-Speed
Device Connection Speed  : Full-Speed
Self powered             : no
Demanded Current         : 100 mA
Used Endpoints           : 1

      ======================== USB Device ========================

        +++++++++++++++++ Device Information ++++++++++++++++++
Device Description       : TinyUSB Device
Device Path 1            : \\?\USB#VID_CAFE&PID_4000#123456#{e21d6d45-3277-4cc4-8193-5b5ada9535df}
Device Path 2            : \\?\USB#VID_CAFE&PID_4000#123456#{a5dcbf10-6530-11d2-901f-00c04fb951ed} (GUID_DEVINTERFACE_USB_DEVICE)
Kernel Name              : \Device\USBPDO-16
Device ID                : USB\VID_CAFE&PID_4000\123456
Hardware IDs             : USB\VID_CAFE&PID_4000&REV_0100 USB\VID_CAFE&PID_4000
Driver KeyName           : {eb781aaf-9c70-4523-a5df-642a87eca567}\0000
Driver                   : \SystemRoot\system32\DRIVERS\libusb0.sys (Version: 1.2.6.0  Date: 2018-10-29)
Driver Inf               : C:\WINDOWS\inf\oem148.inf
Legacy BusType           : PNPBus
Class                    : LibUsbDevices
Class GUID               : {eb781aaf-9c70-4523-a5df-642a87eca567}
Service                  : libusb0
Enumerator               : USB
Location Info            : Port_#0011.Hub_#0003
Location IDs             : PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(11), ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS11)
Container ID             : {c732b6b5-43c1-524a-bfae-562572d08e5d}
Manufacturer Info        : (Undefined Vendor)
Capabilities             : 0x94 (Removable, UniqueID, SurpriseRemovalOK)
Status                   : 0x0180600A (DN_DRIVER_LOADED, DN_STARTED, DN_DISABLEABLE, DN_REMOVABLE, DN_NT_ENUMERATOR, DN_NT_DRIVER)
Problem Code             : 0
HcDisableSelectiveSuspend: 0
EnableSelectiveSuspend   : 0
SelectiveSuspendEnabled  : 0
EnhancedPowerMgmtEnabled : 0
IdleInWorkingState       : 0
WakeFromSleepState       : 0
Power State              : D0 (supported: D0, D3, wake from D0)

        +++++++++++++++++ Registry USB Flags +++++++++++++++++
HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Control\usbflags\CAFE40000100
 osvc                    : REG_BINARY 00 00

        ---------------- Connection Information ---------------
Connection Index         : 0x0B (Port 11)
Connection Status        : 0x01 (DeviceConnected)
Current Config Value     : 0x01 (Configuration 1)
Device Address           : 0x03 (3)
Is Hub                   : 0x00 (no)
Device Bus Speed         : 0x01 (Full-Speed)
Number Of Open Pipes     : 0x00 (0 pipes to data endpoints)
Data (HexDump)           : 0B 00 00 00 12 01 00 02 00 00 00 40 FE CA 00 40   ...........@...@
                           00 01 01 02 03 01 01 01 00 03 00 00 00 00 00 01   ................
                           00 00 00                                          ...

        --------------- Connection Information V2 -------------
Connection Index         : 0x0B (11)
Length                   : 0x10 (16 bytes)
SupportedUsbProtocols    : 0x03
 Usb110                  : 1 (yes, port supports USB 1.1)
 Usb200                  : 1 (yes, port supports USB 2.0)
 Usb300                  : 0 (no, port not supports USB 3.0)
 ReservedMBZ             : 0x00
Flags                    : 0x00
 DevIsOpAtSsOrHigher     : 0 (Device is not operating at SuperSpeed or higher)
 DevIsSsCapOrHigher      : 0 (Device is not SuperSpeed capable or higher)
 DevIsOpAtSsPlusOrHigher : 0 (Device is not operating at SuperSpeedPlus or higher)
 DevIsSsPlusCapOrHigher  : 0 (Device is not SuperSpeedPlus capable or higher)
 ReservedMBZ             : 0x00
Data (HexDump)           : 0B 00 00 00 10 00 00 00 03 00 00 00 00 00 00 00   ................

    ---------------------- Device Descriptor ----------------------
bLength                  : 0x12 (18 bytes)
bDescriptorType          : 0x01 (Device Descriptor)
bcdUSB                   : 0x200 (USB Version 2.00) -> wrong, device is Full-Speed only
bDeviceClass             : 0x00 (defined by the interface descriptors)
bDeviceSubClass          : 0x00
bDeviceProtocol          : 0x00
bMaxPacketSize0          : 0x40 (64 bytes)
idVendor                 : 0xCAFE (Unknown Vendor)
idProduct                : 0x4000
bcdDevice                : 0x0100
iManufacturer            : 0x01 (String Descriptor 1)
 Language 0x0409         : "TinyUSB"
iProduct                 : 0x02 (String Descriptor 2)
 Language 0x0409         : "TinyUSB Device"
iSerialNumber            : 0x03 (String Descriptor 3)
 Language 0x0409         : "123456"
bNumConfigurations       : 0x01 (1 Configuration)
Data (HexDump)           : 12 01 00 02 00 00 00 40 FE CA 00 40 00 01 01 02   .......@...@....
                           03 01                                             ..

    ------------------ Configuration Descriptor -------------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x02 (Configuration Descriptor)
wTotalLength             : 0x001B (27 bytes)
bNumInterfaces           : 0x01 (1 Interface)
bConfigurationValue      : 0x01 (Configuration 1)
iConfiguration           : 0x00 (No String Descriptor)
bmAttributes             : 0x80
 D7: Reserved, set 1     : 0x01
 D6: Self Powered        : 0x00 (no)
 D5: Remote Wakeup       : 0x00 (no)
 D4..0: Reserved, set 0  : 0x00
MaxPower                 : 0x32 (100 mA)
Data (HexDump)           : 09 02 1B 00 01 01 00 80 32 09 04 00 00 00 FE 01   ........2.......
                           01 04 09 21 0D E8 03 00 10 01 01                  ...!.......

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x00 (Interface 0)
bAlternateSetting        : 0x00
bNumEndpoints            : 0x00 (Default Control Pipe only)
bInterfaceClass          : 0xFE (Application Specific)
bInterfaceSubClass       : 0x01 (Device Firmware Upgrade)
bInterfaceProtocol       : 0x01 (Runtime)
iInterface               : 0x04 (String Descriptor 4)
 Language 0x0409         : "TinyUSB DFU runtime"
Data (HexDump)           : 09 04 00 00 00 FE 01 01 04                        .........

        ----- Device Firmware Update Functional Descriptor ----
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x21 (DFU Functional Descriptor)
bmAttributes             : 0x0D
 Bit 7..4: reserved      : 0x00
 Bit 3: WillDetach       : 0x01
 Bit 2: ManifestTolerant : 0x01
 Bit 1: CanUpload        : 0x00
 Bit 0: CanDownload      : 0x01
wDetachTimeOut           : 0x03E8 (1000 ms)
wTransferSize            : 0x1000 (max 4096 bytes)
bcdDFUVersion            : 0x0101 (Version 1.1)
Data (HexDump)           : 09 21 0D E8 03 00 10 01 01                        .!.......

    ----------------- Device Qualifier Descriptor -----------------
Error                    : ERROR_GEN_FAILURE  (*!*ERROR   USB 2.0 devices must provide a Device Qualifier Descriptor)

      -------------------- String Descriptors -------------------
             ------ String Descriptor 0 ------
bLength                  : 0x04 (4 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language ID[0]           : 0x0409 (English - United States)
Data (HexDump)           : 04 03 09 04                                       ....
             ------ String Descriptor 1 ------
bLength                  : 0x10 (16 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "TinyUSB"
Data (HexDump)           : 10 03 54 00 69 00 6E 00 79 00 55 00 53 00 42 00   ..T.i.n.y.U.S.B.
             ------ String Descriptor 2 ------
bLength                  : 0x1E (30 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "TinyUSB Device"
Data (HexDump)           : 1E 03 54 00 69 00 6E 00 79 00 55 00 53 00 42 00   ..T.i.n.y.U.S.B.
                           20 00 44 00 65 00 76 00 69 00 63 00 65 00          .D.e.v.i.c.e.
             ------ String Descriptor 3 ------
bLength                  : 0x0E (14 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "123456"
Data (HexDump)           : 0E 03 31 00 32 00 33 00 34 00 35 00 36 00         ..1.2.3.4.5.6.
             ------ String Descriptor 4 ------
bLength                  : 0x28 (40 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "TinyUSB DFU runtime"
Data (HexDump)           : 28 03 54 00 69 00 6E 00 79 00 55 00 53 00 42 00   (.T.i.n.y.U.S.B.
                           20 00 44 00 46 00 55 00 20 00 72 00 75 00 6E 00    .D.F.U. .r.u.n.
                           74 00 69 00 6D 00 65 00                           t.i.m.e.
