
    =========================== USB Port11 ===========================

Connection Status        : 0x01 (Device is connected)
Port Chain               : 2-11

      ========================== Summary =========================
Vendor ID                : 0xCAFE (Unknown Vendor)
Product ID               : 0x4010
USB Version              : 2.00 -> wrong, Device is Full-Speed only
Port maximum Speed       : High-Speed
Device maximum Speed     : Full-Speed
Device Connection Speed  : Full-Speed
Self powered             : no
Demanded Current         : 100 mA
Used Endpoints           : 1

      ======================== USB Device ========================

        +++++++++++++++++ Device Information ++++++++++++++++++
Device Description       : USB Composite Device
Device Path              : \\?\USB#VID_CAFE&PID_4010#000001#{a5dcbf10-6530-11d2-901f-00c04fb951ed} (GUID_DEVINTERFACE_USB_DEVICE)
Kernel Name              : \Device\USBPDO-17
Device ID                : USB\VID_CAFE&PID_4010\000001
Hardware IDs             : USB\VID_CAFE&PID_4010&REV_0100 USB\VID_CAFE&PID_4010
Driver KeyName           : {36fc9e60-c465-11cf-8056-444553540000}\0034 (GUID_DEVCLASS_USB)
Driver                   : \SystemRoot\System32\drivers\usbccgp.sys (Version: 10.0.19041.488  Date: 2020-09-09)
Driver Inf               : C:\WINDOWS\inf\usb.inf
Legacy BusType           : PNPBus
Class                    : USB
Class GUID               : {36fc9e60-c465-11cf-8056-444553540000} (GUID_DEVCLASS_USB)
Service                  : usbccgp
Enumerator               : USB
Location Info            : Port_#0011.Hub_#0003
Location IDs             : PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(11), ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS11)
Container ID             : {65f74f5e-981c-5fc2-8faf-4eddf6127035}
Manufacturer Info        : (標準 USB ホスト コントローラー)
Capabilities             : 0x94 (Removable, UniqueID, SurpriseRemovalOK)
Status                   : 0x0180600A (DN_DRIVER_LOADED, DN_STARTED, DN_DISABLEABLE, DN_REMOVABLE, DN_NT_ENUMERATOR, DN_NT_DRIVER)
Problem Code             : 0
Address                  : 11
HcDisableSelectiveSuspend: 0
EnableSelectiveSuspend   : 0
SelectiveSuspendEnabled  : 0
EnhancedPowerMgmtEnabled : 0
IdleInWorkingState       : 0
WakeFromSleepState       : 0
Power State              : D0 (supported: D0, D3, wake from D0)
 Child Device 1          : TinyUSB headset (USB オーディオ 2.0)
  Device Path 1          : \\?\USB#VID_CAFE&PID_4010&MI_00#6&1708f169&0&0000#{eb115ffc-10c8-4964-831d-6dcb02e6f23f}\msft_wave (STATIC_KSCATEGORY_REALTIME)
  Device Path 2          : \\?\USB#VID_CAFE&PID_4010&MI_00#6&1708f169&0&0000#{6994ad04-93ef-11d0-a3cc-00a0c9223196}\msft_wave (AM_KSCATEGORY_AUDIO)
  Device Path 3          : \\?\USB#VID_CAFE&PID_4010&MI_00#6&1708f169&0&0000#{dda54a40-1e4c-11d1-a050-405705c10000}\msft_topo (STATIC_KSCATEGORY_TOPOLOGY)
  Device Path 4          : \\?\USB#VID_CAFE&PID_4010&MI_00#6&1708f169&0&0000#{65e8773d-8f56-11d0-a3b9-00a0c9223196}\msft_wave (AM_KSCATEGORY_CAPTURE)
  Device Path 5          : \\?\USB#VID_CAFE&PID_4010&MI_00#6&1708f169&0&0000#{65e8773e-8f56-11d0-a3b9-00a0c9223196}\msft_wave (AM_KSCATEGORY_RENDER)
  Kernel Name            : -
  Device ID              : USB\VID_CAFE&PID_4010&MI_00\6&1708F169&0&0000
  Class                  : MEDIA
  Driver KeyName         : {4d36e96c-e325-11ce-bfc1-08002be10318}\0008 (GUID_DEVCLASS_MEDIA)
  Service                : usbaudio2
  Location               : 0000.0014.0000.011.000.000.000.000.000
  LocationPaths          : PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(11)#USBMI(0)  PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(11)#USB(11)  ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS11)#USBMI(0)  ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS11)#USB(11)
   Child Device 1        : ヘッドホン (TinyUSB headset) (オーディオ エンドポイント)
    Device ID            : SWD\MMDEVAPI\{0.0.0.00000000}.{F68EE7BF-0C55-45C4-8CF8-A34F0CCF8AD7}
    Class                : AudioEndpoint
    Driver KeyName       : {c166523c-fe0c-4a94-a586-f1a80cfbbf3e}\0008 (AUDIOENDPOINT_CLASS_UUID)
   Child Device 2        : マイク (TinyUSB headset) (オーディオ エンドポイント)
    Device ID            : SWD\MMDEVAPI\{0.0.1.00000000}.{27EA259C-3D56-42C1-9D8D-1E0698BBB5C1}
    Class                : AudioEndpoint
    Driver KeyName       : {c166523c-fe0c-4a94-a586-f1a80cfbbf3e}\0007 (AUDIOENDPOINT_CLASS_UUID)

        +++++++++++++++++ Registry USB Flags +++++++++++++++++
HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Control\usbflags\CAFE40100100
 osvc                    : REG_BINARY 00 00

        ---------------- Connection Information ---------------
Connection Index         : 0x0B (Port 11)
Connection Status        : 0x01 (DeviceConnected)
Current Config Value     : 0x01 (Configuration 1)
Device Address           : 0x13 (19)
Is Hub                   : 0x00 (no)
Device Bus Speed         : 0x01 (Full-Speed)
Number Of Open Pipes     : 0x00 (0 pipes to data endpoints)
Data (HexDump)           : 0B 00 00 00 12 01 00 02 EF 02 01 40 FE CA 10 40   ...........@...@
                           00 01 01 02 03 01 01 01 00 13 00 00 00 00 00 01   ................
                           00 00 00                                          ...

        --------------- Connection Information V2 -------------
Connection Index         : 0x0B (11)
Length                   : 0x10 (16 bytes)
SupportedUsbProtocols    : 0x03
 Usb110                  : 1 (yes, port supports USB 1.1)
 Usb200                  : 1 (yes, port supports USB 2.0)
 Usb300                  : 0 (no, port not supports USB 3.0)
 ReservedMBZ             : 0x00
Flags                    : 0x00
 DevIsOpAtSsOrHigher     : 0 (Device is not operating at SuperSpeed or higher)
 DevIsSsCapOrHigher      : 0 (Device is not SuperSpeed capable or higher)
 DevIsOpAtSsPlusOrHigher : 0 (Device is not operating at SuperSpeedPlus or higher)
 DevIsSsPlusCapOrHigher  : 0 (Device is not SuperSpeedPlus capable or higher)
 ReservedMBZ             : 0x00
Data (HexDump)           : 0B 00 00 00 10 00 00 00 03 00 00 00 00 00 00 00   ................

    ---------------------- Device Descriptor ----------------------
bLength                  : 0x12 (18 bytes)
bDescriptorType          : 0x01 (Device Descriptor)
bcdUSB                   : 0x200 (USB Version 2.00) -> wrong, device is Full-Speed only
bDeviceClass             : 0xEF (Miscellaneous)
bDeviceSubClass          : 0x02
bDeviceProtocol          : 0x01 (IAD - Interface Association Descriptor)
bMaxPacketSize0          : 0x40 (64 bytes)
idVendor                 : 0xCAFE (Unknown Vendor)
idProduct                : 0x4010
bcdDevice                : 0x0100
iManufacturer            : 0x01 (String Descriptor 1)
 Language 0x0409         : "TinyUSB"
iProduct                 : 0x02 (String Descriptor 2)
 Language 0x0409         : "TinyUSB headset"
iSerialNumber            : 0x03 (String Descriptor 3)
 Language 0x0409         : "000001"
bNumConfigurations       : 0x01 (1 Configuration)
Data (HexDump)           : 12 01 00 02 EF 02 01 40 FE CA 10 40 00 01 01 02   .......@...@....
                           03 01                                             ..

    ------------------ Configuration Descriptor -------------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x02 (Configuration Descriptor)
wTotalLength             : 0x0141 (321 bytes)
bNumInterfaces           : 0x03 (3 Interfaces)
bConfigurationValue      : 0x01 (Configuration 1)
iConfiguration           : 0x00 (No String Descriptor)
bmAttributes             : 0x80
 D7: Reserved, set 1     : 0x01
 D6: Self Powered        : 0x00 (no)
 D5: Remote Wakeup       : 0x00 (no)
 D4..0: Reserved, set 0  : 0x00
MaxPower                 : 0x32 (100 mA)
Data (HexDump)           : 09 02 41 01 03 01 00 80 32 08 0B 00 03 01 00 20   ..A.....2...... 
                           00 09 04 00 00 00 01 01 20 02 09 24 01 00 02 04   ........ ..$....
                           5D 00 00 08 24 0A 04 03 07 00 00 11 24 02 01 01   ]...$.......$...
                           01 00 04 02 00 00 00 00 00 00 00 00 12 24 06 02   .............$..
                           01 0F 00 00 00 0F 00 00 00 0F 00 00 00 00 0C 24   ...............$
                           03 03 02 03 00 02 04 00 00 00 11 24 02 11 01 02   ...........$....
                           00 04 01 00 00 00 00 00 00 00 00 0C 24 03 13 01   ............$...
                           01 00 11 04 00 00 00 09 04 01 00 00 01 02 20 05   .............. .
                           09 04 01 01 01 01 02 20 05 10 24 01 01 00 01 01   ....... ..$.....
                           00 00 00 02 00 00 00 00 00 06 24 02 01 02 10 07   ..........$.....
                           05 01 09 84 01 01 08 25 01 00 00 01 01 00 09 04   .......%........
                           01 02 01 01 02 20 05 10 24 01 01 00 01 01 00 00   ..... ..$.......
                           00 02 00 00 00 00 00 06 24 02 01 04 18 07 05 01   ........$.......
                           09 08 03 01 08 25 01 00 00 01 01 00 09 04 02 00   .....%..........
                           00 01 02 20 04 09 04 02 01 01 01 02 20 04 10 24   ... ........ ..$
                           01 13 00 01 01 00 00 00 01 00 00 00 00 00 06 24   ...............$
                           02 01 02 10 07 05 81 05 C2 00 01 08 25 01 00 00   ............%...
                           00 00 00 09 04 02 02 01 01 02 20 04 10 24 01 13   .......... ..$..
                           00 01 01 00 00 00 01 00 00 00 00 00 06 24 02 01   .............$..
                           04 18 07 05 81 05 84 01 01 08 25 01 00 00 00 00   ..........%.....
                           00                                                .

        ------------------- IAD Descriptor --------------------
bLength                  : 0x08 (8 bytes)
bDescriptorType          : 0x0B (Interface Association Descriptor)
bFirstInterface          : 0x00 (Interface 0)
bInterfaceCount          : 0x03 (3 Interfaces)
bFunctionClass           : 0x01 (Audio)
bFunctionSubClass        : 0x00 (undefined)
bFunctionProtocol        : 0x20 (AF 2.0)
iFunction                : 0x00 (No String Descriptor)
Data (HexDump)           : 08 0B 00 03 01 00 20 00                           ...... .

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x00 (Interface 0)
bAlternateSetting        : 0x00
bNumEndpoints            : 0x00 (Default Control Pipe only)
bInterfaceClass          : 0x01 (Audio)
bInterfaceSubClass       : 0x01 (Audio Control)
bInterfaceProtocol       : 0x20 (Device Protocol Version 2.0)
iInterface               : 0x02 (String Descriptor 2)
 Language 0x0409         : "TinyUSB headset"
Data (HexDump)           : 09 04 00 00 00 01 01 20 02                        ....... .

        ---- Audio Control Interface Header Descriptor 2.0 ----
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x01 (Header 2.0)
bcdADC                   : 0x0200 (2.0)
bCategory                : 0x04 (headset)
wTotalLength             : 0x005D (93 bytes)
bmControls               : 0x00
 D1..0: Latency          : 0x00 (not present)
 D7..2: Reserved         : 0x00
Data (HexDump)           : 09 24 01 00 02 04 5D 00 00                        .$....]..

        --- Audio Control Clock Source Unit Descriptor 2.0 ----
bLength                  : 0x08 (8 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x0A (Clock Source 2.0)
bClockID                 : 0x04
bmAttributes             : 0x03
 D1..0: Clock Type       : 0x03
 D2   : Sync to SOF      : 0x00
 D7..3: Reserved         : 0x00
bmControls               : 0x07
 D1..0: Clock Frequency  : 0x03 (host programmable)
 D3..2: Clock Validity   : 0x01 (read only)
 D7..4: Reserved         : 0x00
bAssocTerminal           : 0x00
iClockSource             : 0x00 (No String Descriptor)
Data (HexDump)           : 08 24 0A 04 03 07 00 00                           .$......

        ----- Audio Control Input Terminal Descriptor 2.0 -----
bLength                  : 0x11 (17 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x02 (Input Terminal 2.0)
bTerminalID              : 0x01 (1)
wTerminalType            : 0x0101 (USB Streaming)
bAssocTerminal           : 0x00
bCSourceID               : 0x04 (4)
bNrChannels              : 0x02 (2 Channels)
bmChannelConfig          : 0x00000000 (-)
iChannelNames            : 0x00 (No String Descriptor)
bmControls               : 0x0000
 D1..0  : Copy Protect   : 0x00 (not present)
 D3..2  : Connector      : 0x00 (not present)
 D5..4  : Overload       : 0x00 (not present)
 D7..6  : Cluster        : 0x00 (not present)
 D9..8  : Underflow      : 0x00 (not present)
 D11..10: Overflow       : 0x00 (not present)
 D15..12: Reserved       : 0x00
iTerminal                : 0x00 (No String Descriptor)
Data (HexDump)           : 11 24 02 01 01 01 00 04 02 00 00 00 00 00 00 00   .$..............
                           00                                                .

        ------ Audio Control Feature Unit Descriptor 2.0 ------
bLength                  : 0x12 (18 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x06 (Feature Unit 2.0)
bUnitID                  : 0x02 (2)
bSourceID                : 0x01 (1)
bmaControls[0]           : 0x0F, 0x00, 0x00, 0x00
 D1..0  : Mute            : 0x03 (host programmable)
 D3..2  : Volume          : 0x03 (host programmable)
 D5..4  : Bass            : 0x00 (not present)
 D7..6  : Mid             : 0x00 (not present)
 D9..8  : Treble          : 0x00 (not present)
 D11..10: Graph Equalizer : 0x00 (not present)
 D13..12: Automatic Gain  : 0x00 (not present)
 D15..14: Delay           : 0x00 (not present)
 D17..16: Bass Boost      : 0x00 (not present)
 D19..18: Loudness        : 0x00 (not present)
 D21..20: Input Gain      : 0x00 (not present)
 D23..22: Input Gain Pad  : 0x00 (not present)
 D25..24: Phase Inverter  : 0x00 (not present)
 D27..26: Underflow       : 0x00 (not present)
 D29..28: Overflow        : 0x00 (not present)
 D31..30: reserved        : 0x00 (not present)
bmaControls[1]           : 0x0F, 0x00, 0x00, 0x00
 D1..0  : Mute            : 0x03 (host programmable)
 D3..2  : Volume          : 0x03 (host programmable)
 D5..4  : Bass            : 0x00 (not present)
 D7..6  : Mid             : 0x00 (not present)
 D9..8  : Treble          : 0x00 (not present)
 D11..10: Graph Equalizer : 0x00 (not present)
 D13..12: Automatic Gain  : 0x00 (not present)
 D15..14: Delay           : 0x00 (not present)
 D17..16: Bass Boost      : 0x00 (not present)
 D19..18: Loudness        : 0x00 (not present)
 D21..20: Input Gain      : 0x00 (not present)
 D23..22: Input Gain Pad  : 0x00 (not present)
 D25..24: Phase Inverter  : 0x00 (not present)
 D27..26: Underflow       : 0x00 (not present)
 D29..28: Overflow        : 0x00 (not present)
 D31..30: reserved        : 0x00 (not present)
bmaControls[2]           : 0x0F, 0x00, 0x00, 0x00
 D1..0  : Mute            : 0x03 (host programmable)
 D3..2  : Volume          : 0x03 (host programmable)
 D5..4  : Bass            : 0x00 (not present)
 D7..6  : Mid             : 0x00 (not present)
 D9..8  : Treble          : 0x00 (not present)
 D11..10: Graph Equalizer : 0x00 (not present)
 D13..12: Automatic Gain  : 0x00 (not present)
 D15..14: Delay           : 0x00 (not present)
 D17..16: Bass Boost      : 0x00 (not present)
 D19..18: Loudness        : 0x00 (not present)
 D21..20: Input Gain      : 0x00 (not present)
 D23..22: Input Gain Pad  : 0x00 (not present)
 D25..24: Phase Inverter  : 0x00 (not present)
 D27..26: Underflow       : 0x00 (not present)
 D29..28: Overflow        : 0x00 (not present)
 D31..30: reserved        : 0x00 (not present)
iFeature                 : 0x00 (No String Descriptor)
Data (HexDump)           : 12 24 06 02 01 0F 00 00 00 0F 00 00 00 0F 00 00   .$..............
                           00 00                                             ..

        ----- Audio Control Output Terminal Descriptor 2.0 ----
bLength                  : 0x0C (12 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x03 (Output Terminal 2.0)
bTerminalID              : 0x03 (3)
wTerminalType            : 0x0302 (Headphones)
bAssocTerminal           : 0x00 (0)
bSourceID                : 0x02 (2)
bCSourceID               : 0x04 (4)
iTerminal                : 0x00 (No String Descriptor)
Data (HexDump)           : 0C 24 03 03 02 03 00 02 04 00 00 00               .$..........

        ----- Audio Control Input Terminal Descriptor 2.0 -----
bLength                  : 0x11 (17 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x02 (Input Terminal 2.0)
bTerminalID              : 0x11 (17)
wTerminalType            : 0x0201 (Microphone)
bAssocTerminal           : 0x00
bCSourceID               : 0x04 (4)
bNrChannels              : 0x01 (1 Channel)
bmChannelConfig          : 0x00000000 (-)
iChannelNames            : 0x00 (No String Descriptor)
bmControls               : 0x0000
 D1..0  : Copy Protect   : 0x00 (not present)
 D3..2  : Connector      : 0x00 (not present)
 D5..4  : Overload       : 0x00 (not present)
 D7..6  : Cluster        : 0x00 (not present)
 D9..8  : Underflow      : 0x00 (not present)
 D11..10: Overflow       : 0x00 (not present)
 D15..12: Reserved       : 0x00
iTerminal                : 0x00 (No String Descriptor)
Data (HexDump)           : 11 24 02 11 01 02 00 04 01 00 00 00 00 00 00 00   .$..............
                           00                                                .

        ----- Audio Control Output Terminal Descriptor 2.0 ----
bLength                  : 0x0C (12 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x03 (Output Terminal 2.0)
bTerminalID              : 0x13 (19)
wTerminalType            : 0x0101 (USB Streaming)
bAssocTerminal           : 0x00 (0)
bSourceID                : 0x11 (17)
bCSourceID               : 0x04 (4)
iTerminal                : 0x00 (No String Descriptor)
Data (HexDump)           : 0C 24 03 13 01 01 00 11 04 00 00 00               .$..........

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x01 (Interface 1)
bAlternateSetting        : 0x00
bNumEndpoints            : 0x00 (Default Control Pipe only)
bInterfaceClass          : 0x01 (Audio)
bInterfaceSubClass       : 0x02 (Audio Streaming)
bInterfaceProtocol       : 0x20 (Device Protocol Version 2.0)
iInterface               : 0x05 (String Descriptor 5)
 Language 0x0409         : "TinyUSB Microphone"
Data (HexDump)           : 09 04 01 00 00 01 02 20 05                        ....... .

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x01 (Interface 1)
bAlternateSetting        : 0x01
bNumEndpoints            : 0x01 (1 Endpoint)
bInterfaceClass          : 0x01 (Audio)
bInterfaceSubClass       : 0x02 (Audio Streaming)
bInterfaceProtocol       : 0x20 (Device Protocol Version 2.0)
iInterface               : 0x05 (String Descriptor 5)
 Language 0x0409         : "TinyUSB Microphone"
Data (HexDump)           : 09 04 01 01 01 01 02 20 05                        ....... .

        ------ Audio Streaming Interface Descriptor 2.0 -------
bLength                  : 0x10 (16 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x01 (AS General)
bTerminalLink            : 0x01 (1)
bmControls               : 0x00
 D1..0: Active Alt Settng: 0x00 (not present)
 D3..2: Valid Alt Settng : 0x00 (not present)
 D7..4: Reserved         : 0x00
bFormatType              : 0x01 (FORMAT_TYPE_I)
bmFormats                : 0x00000001 (PCM)
bNrChannels              : 0x02 (2 channels)
bmChannelConfig          : 0x00000000 (-)
iChannelNames            : 0x00 (No String Descriptor)
Data (HexDump)           : 10 24 01 01 00 01 01 00 00 00 02 00 00 00 00 00   .$..............

        ----- Audio Streaming Format Type Descriptor 2.0 ------
bLength                  : 0x06 (6 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x02 (Format Type)
bFormatType              : 0x01 (FORMAT_TYPE_I)
bSubslotSize             : 0x02 (2 bytes)
bBitResolution           : 0x10 (16 bits)
Data (HexDump)           : 06 24 02 01 02 10                                 .$....

        ----------------- Endpoint Descriptor -----------------
bLength                  : 0x07 (7 bytes)
bDescriptorType          : 0x05 (Endpoint Descriptor)
bEndpointAddress         : 0x01 (Direction=OUT EndpointID=1)
bmAttributes             : 0x09 (TransferType=Isochronous  SyncType=Adaptive  EndpointType=Data)
wMaxPacketSize           : 0x0184 (388 bytes)
bInterval                : 0x01 (1 ms)
Data (HexDump)           : 07 05 01 09 84 01 01                              .......

        ----------- Audio Data Endpoint Descriptor ------------
bLength                  : 0x08 (8 bytes)
bDescriptorType          : 0x25 (Audio Endpoint Descriptor)
bDescriptorSubtype       : 0x01 (General)
bmAttributes             : 0x00
 D0   : Sampling Freq    : 0x00 (not supported)
 D1   : Pitch            : 0x00 (not supported)
 D6..2: Reserved         : 0x00
 D7   : MaxPacketsOnly   : 0x00 (no)
bLockDelayUnits          : 0x00 (Undefined)
wLockDelay               : 0x0101
Data (HexDump)           : 08 25 01 00 00 01 01 00                           .%......

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x01 (Interface 1)
bAlternateSetting        : 0x02
bNumEndpoints            : 0x01 (1 Endpoint)
bInterfaceClass          : 0x01 (Audio)
bInterfaceSubClass       : 0x02 (Audio Streaming)
bInterfaceProtocol       : 0x20 (Device Protocol Version 2.0)
iInterface               : 0x05 (String Descriptor 5)
 Language 0x0409         : "TinyUSB Microphone"
Data (HexDump)           : 09 04 01 02 01 01 02 20 05                        ....... .

        ------ Audio Streaming Interface Descriptor 2.0 -------
bLength                  : 0x10 (16 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x01 (AS General)
bTerminalLink            : 0x01 (1)
bmControls               : 0x00
 D1..0: Active Alt Settng: 0x00 (not present)
 D3..2: Valid Alt Settng : 0x00 (not present)
 D7..4: Reserved         : 0x00
bFormatType              : 0x01 (FORMAT_TYPE_I)
bmFormats                : 0x00000001 (PCM)
bNrChannels              : 0x02 (2 channels)
bmChannelConfig          : 0x00000000 (-)
iChannelNames            : 0x00 (No String Descriptor)
Data (HexDump)           : 10 24 01 01 00 01 01 00 00 00 02 00 00 00 00 00   .$..............

        ----- Audio Streaming Format Type Descriptor 2.0 ------
bLength                  : 0x06 (6 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x02 (Format Type)
bFormatType              : 0x01 (FORMAT_TYPE_I)
bSubslotSize             : 0x04 (4 bytes)
bBitResolution           : 0x18 (24 bits)
Data (HexDump)           : 06 24 02 01 04 18                                 .$....

        ----------------- Endpoint Descriptor -----------------
bLength                  : 0x07 (7 bytes)
bDescriptorType          : 0x05 (Endpoint Descriptor)
bEndpointAddress         : 0x01 (Direction=OUT EndpointID=1)
bmAttributes             : 0x09 (TransferType=Isochronous  SyncType=Adaptive  EndpointType=Data)
wMaxPacketSize           : 0x0308 (776 bytes)
bInterval                : 0x01 (1 ms)
Data (HexDump)           : 07 05 01 09 08 03 01                              .......

        ----------- Audio Data Endpoint Descriptor ------------
bLength                  : 0x08 (8 bytes)
bDescriptorType          : 0x25 (Audio Endpoint Descriptor)
bDescriptorSubtype       : 0x01 (General)
bmAttributes             : 0x00
 D0   : Sampling Freq    : 0x00 (not supported)
 D1   : Pitch            : 0x00 (not supported)
 D6..2: Reserved         : 0x00
 D7   : MaxPacketsOnly   : 0x00 (no)
bLockDelayUnits          : 0x00 (Undefined)
wLockDelay               : 0x0101
Data (HexDump)           : 08 25 01 00 00 01 01 00                           .%......

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x02 (Interface 2)
bAlternateSetting        : 0x00
bNumEndpoints            : 0x00 (Default Control Pipe only)
bInterfaceClass          : 0x01 (Audio)
bInterfaceSubClass       : 0x02 (Audio Streaming)
bInterfaceProtocol       : 0x20 (Device Protocol Version 2.0)
iInterface               : 0x04 (String Descriptor 4)
 Language 0x0409         : "TinyUSB Speakers"
Data (HexDump)           : 09 04 02 00 00 01 02 20 04                        ....... .

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x02 (Interface 2)
bAlternateSetting        : 0x01
bNumEndpoints            : 0x01 (1 Endpoint)
bInterfaceClass          : 0x01 (Audio)
bInterfaceSubClass       : 0x02 (Audio Streaming)
bInterfaceProtocol       : 0x20 (Device Protocol Version 2.0)
iInterface               : 0x04 (String Descriptor 4)
 Language 0x0409         : "TinyUSB Speakers"
Data (HexDump)           : 09 04 02 01 01 01 02 20 04                        ....... .

        ------ Audio Streaming Interface Descriptor 2.0 -------
bLength                  : 0x10 (16 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x01 (AS General)
bTerminalLink            : 0x13 (19)
bmControls               : 0x00
 D1..0: Active Alt Settng: 0x00 (not present)
 D3..2: Valid Alt Settng : 0x00 (not present)
 D7..4: Reserved         : 0x00
bFormatType              : 0x01 (FORMAT_TYPE_I)
bmFormats                : 0x00000001 (PCM)
bNrChannels              : 0x01 (1 channel)
bmChannelConfig          : 0x00000000 (-)
iChannelNames            : 0x00 (No String Descriptor)
Data (HexDump)           : 10 24 01 13 00 01 01 00 00 00 01 00 00 00 00 00   .$..............

        ----- Audio Streaming Format Type Descriptor 2.0 ------
bLength                  : 0x06 (6 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x02 (Format Type)
bFormatType              : 0x01 (FORMAT_TYPE_I)
bSubslotSize             : 0x02 (2 bytes)
bBitResolution           : 0x10 (16 bits)
Data (HexDump)           : 06 24 02 01 02 10                                 .$....

        ----------------- Endpoint Descriptor -----------------
bLength                  : 0x07 (7 bytes)
bDescriptorType          : 0x05 (Endpoint Descriptor)
bEndpointAddress         : 0x81 (Direction=IN EndpointID=1)
bmAttributes             : 0x05 (TransferType=Isochronous  SyncType=Asynchronous  EndpointType=Data)
wMaxPacketSize           : 0x00C2 (194 bytes)
bInterval                : 0x01 (1 ms)
Data (HexDump)           : 07 05 81 05 C2 00 01                              .......

        ----------- Audio Data Endpoint Descriptor ------------
bLength                  : 0x08 (8 bytes)
bDescriptorType          : 0x25 (Audio Endpoint Descriptor)
bDescriptorSubtype       : 0x01 (General)
bmAttributes             : 0x00
 D0   : Sampling Freq    : 0x00 (not supported)
 D1   : Pitch            : 0x00 (not supported)
 D6..2: Reserved         : 0x00
 D7   : MaxPacketsOnly   : 0x00 (no)
bLockDelayUnits          : 0x00 (Undefined)
wLockDelay               : 0x0000
Data (HexDump)           : 08 25 01 00 00 00 00 00                           .%......

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x02 (Interface 2)
bAlternateSetting        : 0x02
bNumEndpoints            : 0x01 (1 Endpoint)
bInterfaceClass          : 0x01 (Audio)
bInterfaceSubClass       : 0x02 (Audio Streaming)
bInterfaceProtocol       : 0x20 (Device Protocol Version 2.0)
iInterface               : 0x04 (String Descriptor 4)
 Language 0x0409         : "TinyUSB Speakers"
Data (HexDump)           : 09 04 02 02 01 01 02 20 04                        ....... .

        ------ Audio Streaming Interface Descriptor 2.0 -------
bLength                  : 0x10 (16 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x01 (AS General)
bTerminalLink            : 0x13 (19)
bmControls               : 0x00
 D1..0: Active Alt Settng: 0x00 (not present)
 D3..2: Valid Alt Settng : 0x00 (not present)
 D7..4: Reserved         : 0x00
bFormatType              : 0x01 (FORMAT_TYPE_I)
bmFormats                : 0x00000001 (PCM)
bNrChannels              : 0x01 (1 channel)
bmChannelConfig          : 0x00000000 (-)
iChannelNames            : 0x00 (No String Descriptor)
Data (HexDump)           : 10 24 01 13 00 01 01 00 00 00 01 00 00 00 00 00   .$..............

        ----- Audio Streaming Format Type Descriptor 2.0 ------
bLength                  : 0x06 (6 bytes)
bDescriptorType          : 0x24 (Audio Interface Descriptor)
bDescriptorSubtype       : 0x02 (Format Type)
bFormatType              : 0x01 (FORMAT_TYPE_I)
bSubslotSize             : 0x04 (4 bytes)
bBitResolution           : 0x18 (24 bits)
Data (HexDump)           : 06 24 02 01 04 18                                 .$....

        ----------------- Endpoint Descriptor -----------------
bLength                  : 0x07 (7 bytes)
bDescriptorType          : 0x05 (Endpoint Descriptor)
bEndpointAddress         : 0x81 (Direction=IN EndpointID=1)
bmAttributes             : 0x05 (TransferType=Isochronous  SyncType=Asynchronous  EndpointType=Data)
wMaxPacketSize           : 0x0184 (388 bytes)
bInterval                : 0x01 (1 ms)
Data (HexDump)           : 07 05 81 05 84 01 01                              .......

        ----------- Audio Data Endpoint Descriptor ------------
bLength                  : 0x08 (8 bytes)
bDescriptorType          : 0x25 (Audio Endpoint Descriptor)
bDescriptorSubtype       : 0x01 (General)
bmAttributes             : 0x00
 D0   : Sampling Freq    : 0x00 (not supported)
 D1   : Pitch            : 0x00 (not supported)
 D6..2: Reserved         : 0x00
 D7   : MaxPacketsOnly   : 0x00 (no)
bLockDelayUnits          : 0x00 (Undefined)
wLockDelay               : 0x0000
Data (HexDump)           : 08 25 01 00 00 00 00 00                           .%......

    ----------------- Device Qualifier Descriptor -----------------
Error                    : ERROR_GEN_FAILURE  (*!*ERROR   USB 2.0 devices must provide a Device Qualifier Descriptor)

      -------------------- String Descriptors -------------------
             ------ String Descriptor 0 ------
bLength                  : 0x04 (4 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language ID[0]           : 0x0409 (English - United States)
Data (HexDump)           : 04 03 09 04                                       ....
             ------ String Descriptor 1 ------
bLength                  : 0x10 (16 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "TinyUSB"
Data (HexDump)           : 10 03 54 00 69 00 6E 00 79 00 55 00 53 00 42 00   ..T.i.n.y.U.S.B.
             ------ String Descriptor 2 ------
bLength                  : 0x20 (32 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "TinyUSB headset"
Data (HexDump)           : 20 03 54 00 69 00 6E 00 79 00 55 00 53 00 42 00    .T.i.n.y.U.S.B.
                           20 00 68 00 65 00 61 00 64 00 73 00 65 00 74 00    .h.e.a.d.s.e.t.
             ------ String Descriptor 3 ------
bLength                  : 0x0E (14 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "000001"
Data (HexDump)           : 0E 03 30 00 30 00 30 00 30 00 30 00 31 00         ..0.0.0.0.0.1.
             ------ String Descriptor 4 ------
bLength                  : 0x22 (34 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "TinyUSB Speakers"
Data (HexDump)           : 22 03 54 00 69 00 6E 00 79 00 55 00 53 00 42 00   ".T.i.n.y.U.S.B.
                           20 00 53 00 70 00 65 00 61 00 6B 00 65 00 72 00    .S.p.e.a.k.e.r.
                           73 00                                             s.
             ------ String Descriptor 5 ------
bLength                  : 0x26 (38 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "TinyUSB Microphone"
Data (HexDump)           : 26 03 54 00 69 00 6E 00 79 00 55 00 53 00 42 00   &.T.i.n.y.U.S.B.
                           20 00 4D 00 69 00 63 00 72 00 6F 00 70 00 68 00    .M.i.c.r.o.p.h.
                           6F 00 6E 00 65 00                                 o.n.e.
