LYNX_RGB Project Status
Project File: | lynx_rgb.ise | Current State: | Programming File Generated
Module Name: | lynx_rgb | Errors: | No Errors
Target Device: | xc3s50an-4tqg144 | Warnings: | 174 Warnings
Product Version: | ISE 9.2.04i | Updated: | ? 2 20 12:23:03 2010

LYNX_RGB Partition Summary
No partition information was found.

Device Utilization Summary
Logic Utilization | Used | Available | Utilization | Note(s)
Number of Slice Flip Flops | 161 | 1,408 | 11% |
Number of 4 input LUTs | 136 | 1,408 | 9% |
Logic Distribution |  |  |  |
Number of occupied Slices | 113 | 704 | 16% |
Number of Slices containing only related logic | 113 | 113 | 100% |
Number of Slices containing unrelated logic | 0 | 113 | 0% |
Total Number of 4 input LUTs | 136 | 1,408 | 9% |
Number of bonded IOBs | 70 | 108 | 64% |
IOB Flip Flops | 4 |  |  |
IOB Master Pads | 4 |  |  |
IOB Slave Pads | 4 |  |  |
Number of ODDR2s used | 1 |  |  |
Number of GCLKs | 3 | 24 | 12% |
Number of DCMs | 1 | 2 | 50% |
Total equivalent gate count for design | 9,176 |  |  |
Additional JTAG gate count for IOBs | 3,360 |  |  |

Performance Summary
Final Timing Score: | 39 | Pinout Data: | Pinout Report
Routing Results: | All Signals Completely Routed | Clock Data: | Clock Report
Timing Constraints: | 1 Failing Constraint |  |

Detailed Reports
Report Name | Status | Generated | Errors | Warnings | Infos
Synthesis Report | Current | ? 2 19 18:28:06 2010 | 0 | 89 Warnings | 0
Translation Report | Current | ? 2 19 18:28:12 2010 | 0 | 11 Warnings | 1 Info
Map Report | Current | ? 2 19 18:28:22 2010 | 0 | 38 Warnings | 5 Infos
Place and Route Report | Current | ? 2 19 18:28:32 2010 | 0 | 36 Warnings | 2 Infos
Static Timing Report | Current | ? 2 19 18:28:36 2010 | 0 | 0 | 2 Infos
Bitgen Report | Current | ? 2 19 18:28:43 2010 | 0 | 0 | 0